| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- isf_SensorConfig_t : isf_dsa_adapter.h
- isf_SensorDataTypes_t : isf_sensor_types.h
- isf_SensorHandle_t : isf_dsa_adapter.h
- isf_SensorTypes_t : isf_sensor_types.h
- isf_sm_begin_sensor_data() : isf_sm_api.h
- isf_sm_end_sensor_data() : isf_sm_api.h
- isf_sm_find_sensor_by_type() : isf_sm_api.h
- isf_sm_get_sensor_data() : isf_sm_api.h
- isf_sm_subscribe_sensor_data() : isf_sm_api.h
- isf_sm_unsubscribe_sensor_data() : isf_sm_api.h
- isf_status_enum : isf.h
- isf_status_t : isf.h
- isf_system_sync() : isf_init.h , isf_init.c
- sema_bm_access : bus_management.c
- SENSOR_ACTIVE : isf_sensors.h
- SENSOR_BOOT : isf_sensors.h
- SENSOR_DATA_READY_EVENT : rli_project.c , fsl_fusion_virt_3D_orient.c
- SENSOR_ERROR_CHECKID : isf_sensors.h
- SENSOR_ERROR_GETDATA : isf_sensors.h
- SENSOR_ERROR_SETMODE : isf_sensors.h
- sensor_mode_t : isf_sensors.h
- SENSOR_READY : isf_sensors.h
- Sensor_sensors_en : isf_sensor_configuration.h
- SENSOR_STANDBY : isf_sensors.h
- SENSOR_STATE_CONFIGURED : isf_sensors.h
- SENSOR_STATE_INITIALIZED : isf_sensors.h
- SENSOR_STATE_STARTED : isf_sensors.h
- SENSOR_STATE_UNINITIALIZED : isf_sensors.h
- SENSORFS : fusion_config.h
- SensorId_t : isf_sensor_configuration.h
- Serial_ISF_UART1_Init() : Serial_ISF_UART1.c
- Serial_ISF_UART1_Init_METHOD_ENABLED : Serial_ISF_UART1.h
- Serial_ISF_UART1_Interrupt() : Serial_ISF_UART1.c
- Serial_ISF_UART1_OnBlockReceived() : UART_CH1.c
- Serial_ISF_UART1_OnBlockReceived_EVENT_ENABLED : Serial_ISF_UART1.h
- Serial_ISF_UART1_OnBlockSent() : UART_CH1.c
- Serial_ISF_UART1_OnBlockSent_EVENT_ENABLED : Serial_ISF_UART1.h
- Serial_ISF_UART1_PRPH_BASE_ADDRESS : Serial_ISF_UART1.h
- Serial_ISF_UART1_ReceiveBlock() : Serial_ISF_UART1.c
- Serial_ISF_UART1_ReceiveBlock_METHOD_ENABLED : Serial_ISF_UART1.h
- Serial_ISF_UART1_SendBlock() : Serial_ISF_UART1.c
- Serial_ISF_UART1_SendBlock_METHOD_ENABLED : Serial_ISF_UART1.h
- Serial_ISF_UART1_TDeviceDataPtr : Serial_ISF_UART1.h
- SET_FIELD : App1.c , rli_project.c
- SetPortE_Gpio() : bus_management.c
- shutdown_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- SINDELTAMAX : fusion.c
- SM_API_ALTERNATE_OFFERED : isf_sm_types.h
- SM_API_ERR_ALREADY_BEGUN : isf_sm_types.h
- SM_API_ERR_BUFFERLOCK_TIMEOUT : isf_sm_types.h
- SM_API_ERR_DATATYPE_NOT_SUPPORTED : isf_sm_types.h
- SM_API_ERR_FIFO_OVER_LIMIT : isf_sm_types.h
- SM_API_ERR_INVALID_HANDLE : isf_sm_types.h
- SM_API_ERR_INVALID_PTR : isf_sm_types.h
- SM_API_ERR_LOCK_CREATION_FAILED : isf_sm_types.h
- SM_API_ERR_MAX_TAPS_PER_SENSOR : isf_sm_types.h
- SM_API_ERR_NO_MEMORY : isf_sm_types.h
- SM_API_ERR_NOT_YET_BEGUN : isf_sm_types.h
- SM_API_ERR_SAMPLE_TAP_RATE : isf_sm_types.h
- SM_API_ERR_SENSOR_ALREADY_INITIALIZED : isf_sm_types.h
- SM_API_ERR_SENSOR_ID : isf_sm_types.h
- SM_API_ERR_SENSOR_INIT_FAILED : isf_sm_types.h
- SM_API_ERR_SENSOR_NOT_AVAIL : isf_sm_types.h
- SM_API_ERR_SETTINGS_TO_USE : isf_sm_types.h
- SM_API_ERR_SUBSCRIBER_COUNT : isf_sm_types.h
- SM_API_ERR_TOKEN_ID : isf_sm_types.h
- SM_BEST_POSSIBLE_SETTINGS : isf_sm_types.h
- SM_CURRENT_SETTINGS : isf_sm_types.h
- SM_GIVEN_SETTINGS : isf_sm_types.h
- SM_MAX_FIFO_DEPTH : isf_sm_types.h
- SM_MAX_SUBSCRIBERS_PER_SENSOR : isf_sm_types.h
- sm_result_t : isf_sm_types.h
- sm_token_t : isf_sm_types.h
- SMALLMODULUS : orientation.c
- SMALLQ0 : orientation.c
- SP_MB0 : ci_protocol_mbox.h
- SP_MB1 : ci_protocol_mbox.h
- SP_MB2 : ci_protocol_mbox.h
- SP_MB3 : ci_protocol_mbox.h
- SP_MB4 : ci_protocol_mbox.h
- SPI_ASYNC : isf_spi_master_adapter.h
- SPI_BUS_0 : isf_sysconf_comms.c
- spi_clock_phase_t : fsl_spi_hal.h
- spi_clock_polarity_t : fsl_spi_hal.h
- spi_comm_flag : isf_spi_master_adapter.h
- spi_config_t : fsl_spi_hal.h
- spi_hal_disable() : fsl_spi_hal.c
- spi_hal_enable() : fsl_spi_hal.c
- spi_handle_t : fsl_spi_master_driver.h
- SPI_LOCK_COMMON : isf_spi_master_adapter.h
- SPI_LOCK_READ : isf_spi_master_adapter.h
- spi_lock_type : isf_spi_master_adapter.h
- spi_master_adapter_acquire_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_configure() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_config() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_state() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_init() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_read() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_start() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_stop() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_write() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_busConfig_t : isf_spi_master_types.h
- spi_master_busHandle : isf_sysconf_comms.c , isf_spi_master_adapter.c
- spi_master_busHandle_t : isf_spi_master_types.h
- spi_master_configure_bus() : fsl_spi_master_driver.h , fsl_spi_master_driver.c
- spi_master_Endpoint_t : isf_spi_master_adapter.h
- spi_master_init() : fsl_spi_master_driver.h , fsl_spi_master_driver.c
- spi_master_instance_tbl : isf_fsl_spi_master_PEx.c , fsl_spi_master_driver.c
- spi_master_lock : isf_spi_master_adapter.c , isf_sysconf_comms.c
- spi_master_rdlock : isf_sysconf_comms.c , isf_spi_master_adapter.c
- spi_master_readFlags_t : isf_spi_master_adapter.h
- spi_master_slave_mode_t : fsl_spi_hal.h
- spi_master_slaveInfo_t : isf_spi_master_types.h
- spi_master_state : fsl_spi_master_driver.c
- spi_master_state_t : fsl_spi_master_driver.h
- spi_master_transfer() : fsl_spi_master_driver.c , fsl_spi_master_driver.h
- spi_master_transfer_async() : fsl_spi_master_driver.c , fsl_spi_master_driver.h
- spi_master_writeFlags_t : isf_spi_master_adapter.h
- spi_mater_slaveCmd_t : isf_spi_master_types.h
- SPI_NUM_BUS : isf_sysconf_comms.c
- SPI_PEX_READ_EVENT_ERROR : fsl_spi_master_driver.h
- SPI_PEX_READ_EVENT_SUCCESS : fsl_spi_master_driver.h
- SPI_PEX_WRITE_EVENT_ERROR : fsl_spi_master_driver.h
- SPI_PEX_WRITE_EVENT_SUCCESS : fsl_spi_master_driver.h
- spi_pin_mode_t : fsl_spi_hal.h
- spi_shift_direction_t : fsl_spi_hal.h
- spi_ss_output_mode_t : fsl_spi_hal.h
- spi_status_t : fsl_spi_hal.h
- SPI_SYNC : isf_spi_master_adapter.h
- spi_user_config_t : fsl_spi_master_driver.h
- SPIMasterBus1_OnBlockReceived() : SPI_CH1.c
- SPIMasterBus1_OnBlockSent() : SPI_CH1.c
- start_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- START_TIMER : fusion_exec.c
- startof : App1.c
- STATUS_00_REG : mpl3115.h
- stop_sensor() : isf_dsa_direct.c , isf_dsa_direct.h
- STOP_TIMER : fusion_exec.c
- STREAM_COCO_BIT : ci_protocol_stream.h
- STREAM_COCO_BIT_MASK : ci_protocol_stream.h
- STREAM_CRC_BYTESIZE : ci_protocol_stream.h
- STREAM_CRC_DISABLED : isf_ci_stream.h
- STREAM_CRC_ENABLED : isf_ci_stream.h
- STREAM_PROTOCOL_CMD_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_CMD_STATUS_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_DISABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_ENABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_STREAMID : ci_protocol_stream.h
- STREAM_PROTOCOL_RECV_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_DEFAULT_ARRAY_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_CMD_ECHO : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_DATASTART : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_RESPDATALENGTH_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_SUBCMD_BYTESIZE : ci_protocol_stream.h
- SubscriptionSettingChoices : isf_sm_types.h
- SubscriptionSettingsChoices_t : isf_sm_types.h
- swdelay() : bus_management.c
- synchCreate : isf_init.c
- sys_channelId_t : isf_sysconf_types.h
- SYS_NUM_CHANNEL_IDS : isf_sysconf_comms.h
- sys_protocolType_t : isf_sysconf_types.h
- system_timer_init() : MQX1.c
- system_timer_start() : MQX1.c
- SystemTimer1_GetTicsPerSecond() : MQX1.c
- SystemTimer1_OnCounterRestart() : MQX1.c

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.