| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
fxas21000_ODR_Table_tag Struct Reference
fsl_fxas21002_i2cspi_3D_gyro module documentation

the structure defines the ODR table between Hybrid and normal mode of FXAS21000 operation. More...

`#include <fsl_fxas21002_i2cspi_3D_gyro.h>`

Collaboration diagram for fxas21000_ODR_Table_tag:

## Data Fields
uint32 | periodNormalMode
uint8 | configVal

## Detailed Description

the structure defines the ODR table between Hybrid and normal mode of FXAS21000 operation.

Definition at line 90 of file fsl_fxas21002_i2cspi_3D_gyro.h.

## Field Documentation

uint8 configVal

configuration value correspond to given ODR in millisecond.

Definition at line 92 of file fsl_fxas21002_i2cspi_3D_gyro.h.

uint32 periodNormalMode

Normal Mode ODR value in millisecond.

Definition at line 91 of file fsl_fxas21002_i2cspi_3D_gyro.h.

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxas21002_i2cspi_3D_gyro.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.