| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
I2CDeviceInfo Struct Reference
I2c_master

Information necessary to communicate with an I2C slave device. More...

`#include <fsl_i2c_master_driver.h>`

Collaboration diagram for I2CDeviceInfo:

## Data Fields
uint16_t | address
uint32_t | baudRate_kbps
LDD_I2C_TAddrType | addrType

## Detailed Description

Information necessary to communicate with an I2C slave device.

Definition at line 30 of file fsl_i2c_master_driver.h.

## Field Documentation

uint16_t address

The slave's 7-bit or 10 bit address.

Definition at line 32 of file fsl_i2c_master_driver.h.

Referenced by device_connect(), and i2c_master_transfer().

LDD_I2C_TAddrType addrType

Address Types.

Definition at line 34 of file fsl_i2c_master_driver.h.

Referenced by i2c_master_transfer().

uint32_t baudRate_kbps

The baud rate in kbps to use with this slave device.

Definition at line 33 of file fsl_i2c_master_driver.h.

Referenced by i2c_master_adapter_configure().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/fsl_i2c_master_driver.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.