| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
device_cmd_packet_t Struct Reference
rli_project module documentation

rli overall application state buffer format. More...

Collaboration diagram for device_cmd_packet_t:

## Data Fields
uint8 | appId
uint8 | cmd
uint16 | nWrite
uint8 | nRead

## Detailed Description

rli overall application state buffer format.

Definition at line 88 of file rli_project.c.

## Field Documentation

uint8 appId

Application ID

Definition at line 91 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint8 cmd

Host command

Definition at line 94 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint8 nRead

Number of bytes to read/write

Definition at line 100 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint16 nWrite

Register Offset

Definition at line 97 of file rli_project.c.

Referenced by rli_ci_app_callback().

The documentation for this struct was generated from the following file:

- ISF/RLI/Source/rli_project.c

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.