| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
uart_BusConfig_struct Struct Reference

`#include <isf_uart_types.h>`

Collaboration diagram for uart_BusConfig_struct:

## Data Fields
isf_duration_t | timeout
uart_user_config_t | config

## Detailed Description

Definition at line 17 of file isf_uart_types.h.

## Field Documentation

uart_user_config_t config

Uart configuration information.

Definition at line 19 of file isf_uart_types.h.

Referenced by uart_adapter_configure(), and uart_adapter_init().

isf_duration_t timeout

The bus timeout value to use.

Definition at line 18 of file isf_uart_types.h.

Referenced by uart_adapter_acquire_lock(), uart_adapter_configure(), uart_adapter_get_endpoint(), uart_adapter_read(), uart_adapter_start(), uart_adapter_stop(), and uart_adapter_write().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_uart_types.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.