| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- i
- l
- m
- o
- p
- q
- r
- s
- t
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages

### - s -

- isf_sm_begin_sensor_data() : isf_sm_api.h
- isf_sm_end_sensor_data() : isf_sm_api.h
- isf_sm_find_sensor_by_type() : isf_sm_api.h
- isf_sm_get_sensor_data() : isf_sm_api.h
- isf_sm_subscribe_sensor_data() : isf_sm_api.h
- isf_sm_unsubscribe_sensor_data() : isf_sm_api.h
- isf_system_sync() : isf_init.h , isf_init.c
- Serial_ISF_UART1_Init() : Serial_ISF_UART1.c
- Serial_ISF_UART1_Interrupt() : Serial_ISF_UART1.c
- Serial_ISF_UART1_OnBlockReceived() : UART_CH1.c
- Serial_ISF_UART1_OnBlockSent() : UART_CH1.c
- Serial_ISF_UART1_ReceiveBlock() : Serial_ISF_UART1.c
- Serial_ISF_UART1_SendBlock() : Serial_ISF_UART1.c
- SetPortE_Gpio() : bus_management.c
- shutdown_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- spi_hal_disable() : fsl_spi_hal.c
- spi_hal_enable() : fsl_spi_hal.c
- spi_master_adapter_acquire_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_configure() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_config() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_state() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_init() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_read() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_start() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_stop() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_write() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_configure_bus() : fsl_spi_master_driver.h , fsl_spi_master_driver.c
- spi_master_init() : fsl_spi_master_driver.h , fsl_spi_master_driver.c
- spi_master_transfer() : fsl_spi_master_driver.c , fsl_spi_master_driver.h
- spi_master_transfer_async() : fsl_spi_master_driver.h , fsl_spi_master_driver.c
- SPIMasterBus1_OnBlockReceived() : SPI_CH1.c
- SPIMasterBus1_OnBlockSent() : SPI_CH1.c
- start_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- stop_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- swdelay() : bus_management.c
- system_timer_init() : MQX1.c
- system_timer_start() : MQX1.c
- SystemTimer1_GetTicsPerSecond() : MQX1.c
- SystemTimer1_OnCounterRestart() : MQX1.c

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.