| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
fxos8700_ODR_Table_tag Struct Reference
fsl_fxos8700_i2cspi_6D_AccMag module documentation

the structure defines the ODR table between Hybrid and normal mode of device operation. More...

`#include <fsl_fxos8700_i2cspi_6D_AccMag.h>`

Collaboration diagram for fxos8700_ODR_Table_tag:

## Data Fields
uint32 | periodNormalMode
uint32 | periodHybridMode
uint8 | configVal

## Detailed Description

the structure defines the ODR table between Hybrid and normal mode of device operation.

Definition at line 93 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

## Field Documentation

uint8 configVal

configuration value correspond to given ODR in millisecond.

Definition at line 96 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

uint32 periodHybridMode

Hybrid mode ODR value in millisecond.

Definition at line 95 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

uint32 periodNormalMode

Normal Mode ODR value in millisecond.

Definition at line 94 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxos8700_i2cspi_6D_AccMag.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.