| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Structures | Functions | Variables
fsl_fusion_virt_3D_orient.h File Reference
`#include "PE_Types.h"`
`#include "PE_Error.h"`
`#include "PE_Const.h"`
`#include "IO_Map.h"`
`#include "Cpu.h"`
`#include "fusion_config.h"`
`#include "fusion_types.h"`
`#include "fusion_exec.h"`
`#include "isf_sm_types.h"`
`#include "isf_sensor_base_types.h"`
`#include "isf_dsa_adapter.h"`
`#include "magnetic.h"`
Include dependency graph for fsl_fusion_virt_3D_orient.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | fsl_orientation_DataBuffer_t
struct | fsl_fusion_Sensor_Specific_Settings_t
struct | fsl_fusion_DeviceDescriptor_t

## Functions
isf_dsa_status_t | fsl_fusion_virt_3D_orient_Initialize (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the orientation sensor adapter initialization. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_ValidateSettings (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSubSettings)
| This is the concrete implementation of the orientation sensor adapter for validating current settings. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_Configure (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
| This is the concrete implementation of the fusion sensor adapter configuration function. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_StartData (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the orientation sensor adapter for start Data. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_EndData (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the orientation sensor adapter for End Data. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_Calibrate (isf_SensorHandle_t *pSensorHandle, void *pCalData)
| This is the concrete implementation of the orientation sensor adapter for calibration . More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_Shutdown (isf_SensorHandle_t *pSensorHandle)
| This is the concrete implementation of the orientation sensor adapter for shutdown . More...
void | fsl_fusion_virt_3D_orient_PeriodicCallback (void *pSensorHandle)
| The orientation sensor adapter's periodic processing function. More...
isf_dsa_status_t | fsl_fusion_virt_3D_orient_Convert (volatile isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *pNativeSample, void *pConvertedSample, int32 *numBytes)
| This function coverts the raw sample data to the desired output type. More...
void | fsl_MagCal_task (uint32_t task_init_data)
void | fsl_fusion_task (uint32_t task_init_data)

## Variables
isf_SensorTypes_t | fsl_fusion_SupportedSensorTypes []
| Supported sensor and data types for MMA8652. More...
isf_SensorDataTypes_t | fsl_fusion_SupportedDataTypes []

## Detailed Description

Version
  01.00

Definition in file fsl_fusion_virt_3D_orient.h.

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.