| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages

### - b -

- bandwidth : fxas21002_Sensor_Specific_Settings_t
- baudRate : UartConfig , UartUserConfig
- baudRate_kbps : I2CDeviceInfo
- bitCountPerChar : UartConfig , UartUserConfig
- Bits : ci_ctrl_reg_t , ci_stream_ctrl_reg1_t
- blockTransferMode : ci_ctrl_reg_t
- bufferLock : isf_fifo_t
- build_code : device_info_t
- buildCode : isf_lib_info_t
- buildTime : isf_lib_info_t
- busConfig : i2c_Master_BusHandle_struct , spi_master_CommSpecificInfo_t , spi_mater_BusHandle_struct , uart_BusHandle_struct
- busFrequencyKHz : SPIUserConfig
- busHandle : dm_ChannelDescriptor_struct
- busState : i2c_Master_BusHandle_struct , spi_mater_BusHandle_struct , uart_BusHandle_struct
- byte_cnt : ci_host_cmd_packet_t
- byte_id : qr_config_t
- bytes_left : ci_app_resp_packet_t
- bytes_xfer : ci_app_resp_packet_t
- bytesLeft : ci_tx_packet_t

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.