| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Functions | Variables
fsl_pit_driver.c File Reference

fsl_pit_driver.c implements the PIT driver. More...

`#include "fsl_pit_driver.h"`
`#include "BM_pit_instance.h"`
`#include "isf_fsl_TU_PEx.h"`
Include dependency graph for fsl_pit_driver.c:

Go to the source code of this file.

## Functions
void | pit_init_module (bool isRunInDebug)
| Initialize PIT module. More...
void | pit_init_channel (uint32_t timer, const pit_user_config_t *config)
| Initialize PIT channel. More...
void | pit_shutdown (void)
| Disable PIT module and gate control. More...
void | pit_timer_start (uint32_t timer)
| Start timer counting. More...
void | pit_timer_stop (uint32_t timer)
| Stop timer counting. More...
void | pit_set_timer_period_us (uint32_t timer, uint32_t us)
| Set timer period in microsecond units. More...
uint32_t | pit_read_timer_us (uint32_t timer)
| Read current timer value in microsecond units. More...
void | pit_init (bool bEnableirq, uint32 usec)
| Complete initialization of the PIT timer. More...

## Variables
uint64_t | pitSourceClock

## Detailed Description

fsl_pit_driver.c implements the PIT driver.

File: fsl_pit_driver.c

Copyright (c) 2014, Freescale Semiconductor, Inc.

Definition in file fsl_pit_driver.c.

## Variable Documentation

uint64_t pitSourceClock

Definition at line 26 of file fsl_pit_driver.c.

Referenced by pit_init_module(), and pit_read_timer_us().

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.