| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Structures | Typedefs
isf_fsl_spi_master_PEx.h File Reference
`#include "PE_Types.h"`
Include dependency graph for isf_fsl_spi_master_PEx.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | spi_master_instance_PEx
| This structure contains i2c LLD function pointers. More...

## Typedefs
typedef LDD_TDeviceData *(* | fnSPIInit_t )(LDD_TUserData *apUserData)
| This is the function pointer signature for i2c initialization. More...
typedef LDD_TError(* | fnSPIRead_t )(LDD_TDeviceData *apDevice, LDD_TData *BufferPtr, uint16_t Size)
| This is the function pointer signature for reading the data from a specified device. More...
typedef LDD_TError(* | fnSPIWrite_t )(LDD_TDeviceData *apDevice, LDD_TData *BufferPtr, uint16_t Size)
| This is the the function pointer signature for writing the data to a specified device. More...

## Typedef Documentation

typedef LDD_TDeviceData*(* fnSPIInit_t)(LDD_TUserData *apUserData)

This is the function pointer signature for i2c initialization.

Definition at line 14 of file isf_fsl_spi_master_PEx.h.

typedef LDD_TError(* fnSPIRead_t)(LDD_TDeviceData *apDevice, LDD_TData *BufferPtr, uint16_t Size)

This is the function pointer signature for reading the data from a specified device.

Definition at line 18 of file isf_fsl_spi_master_PEx.h.

typedef LDD_TError(* fnSPIWrite_t)(LDD_TDeviceData *apDevice, LDD_TData *BufferPtr, uint16_t Size)

This is the the function pointer signature for writing the data to a specified device.

Definition at line 22 of file isf_fsl_spi_master_PEx.h.

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.