| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
spi_master_instance_PEx Struct Reference

This structure contains i2c LLD function pointers. More...

`#include <isf_fsl_spi_master_PEx.h>`

Collaboration diagram for spi_master_instance_PEx:

## Data Fields
fnSPIInit_t | fnSPILLDInit
fnSPIRead_t | fnSPICLLDRead
fnSPIWrite_t | fnSPILLDWrite

## Detailed Description

This structure contains i2c LLD function pointers.

Definition at line 26 of file isf_fsl_spi_master_PEx.h.

## Field Documentation

fnSPIRead_t fnSPICLLDRead

Read from a device.

Definition at line 28 of file isf_fsl_spi_master_PEx.h.

fnSPIInit_t fnSPILLDInit

Initialize a spi LDD component.

Definition at line 27 of file isf_fsl_spi_master_PEx.h.

Referenced by spi_master_init().

fnSPIWrite_t fnSPILLDWrite

Write to a device.

Definition at line 29 of file isf_fsl_spi_master_PEx.h.

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_fsl_spi_master_PEx.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.