| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
Analog_1_SensorData_Float_t Struct Reference
fsl_Sensor_Analog_1_Functions module documentation

Standard fixed type for three axis accelerometers. More...

`#include <fsl_Sensor_Analog_1_Functions.h>`

Collaboration diagram for Analog_1_SensorData_Float_t:

## Data Fields
isf_timestamp_t | timestamp
isf_Analog_1_float_data_t | sensorData [MAX_ADC_CHANNELS]

## Detailed Description

Standard fixed type for three axis accelerometers.

Definition at line 143 of file fsl_Sensor_Analog_1_Functions.h.

## Field Documentation

isf_Analog_1_float_data_t sensorData[MAX_ADC_CHANNELS]

Definition at line 145 of file fsl_Sensor_Analog_1_Functions.h.

Referenced by Analog_1_float_converter().

isf_timestamp_t timestamp

Definition at line 144 of file fsl_Sensor_Analog_1_Functions.h.

Referenced by Analog_1_float_converter().

The documentation for this struct was generated from the following file:

- fsl_Sensor_Analog_1_Functions.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.