| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- isf_SensorConfig_t : isf_dsa_adapter.h
- isf_SensorDataTypes_t : isf_sensor_types.h
- isf_SensorHandle_t : isf_dsa_adapter.h
- isf_SensorTypes_t : isf_sensor_types.h
- isf_sm_begin_sensor_data() : isf_sm_api.h
- isf_sm_end_sensor_data() : isf_sm_api.h
- isf_sm_find_sensor_by_type() : isf_sm_api.h
- isf_sm_get_sensor_data() : isf_sm_api.h
- isf_sm_subscribe_sensor_data() : isf_sm_api.h
- isf_sm_unsubscribe_sensor_data() : isf_sm_api.h
- isf_status_enum : isf.h
- isf_status_t : isf.h
- isf_swap2byte() : isf_util.h , isf_util.c
- isf_swap4byte() : isf_util.h , isf_util.c
- isf_system_sync() : bus_management.c , task_ci.c , isf_init.h , isf_init.c
- SampleRates : MMA955x_2.c , MMA955x_1.c
- SCS_BASE_ADDR : isf_systick_defs.h
- SelectedAFEPriority : MMA955x_1.c , MMA955x_2.c
- SelectedMBoxPriority : MMA955x_1.c , MMA955x_2.c
- SelectedSampleRate : MMA955x_1.c , MMA955x_2.c
- sema_bm_access : bus_management.c
- sema_ev_access : isf_eventhandler.c
- SENSOR_ACTIVE : isf_sensors.h
- SENSOR_BOOT : isf_sensors.h
- SENSOR_DATA_READY_EVENT : rli_project.c , fsl_fusion_virt_3D_orient.c
- SENSOR_ERROR_CHECKID : isf_sensors.h
- SENSOR_ERROR_GETDATA : isf_sensors.h
- SENSOR_ERROR_SETMODE : isf_sensors.h
- SENSOR_IDX_Accelerometer0 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer1 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer2 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer3 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer4 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer5 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer6 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer7 : BasicApp1_types.h
- SENSOR_IDX_Altitude15 : BasicApp1_types.h
- SENSOR_IDX_Analog19 : BasicApp1_types.h
- SENSOR_IDX_Custom18 : BasicApp1_types.h
- SENSOR_IDX_Gyrometer10 : BasicApp1_types.h
- SENSOR_IDX_Gyrometer11 : BasicApp1_types.h
- SENSOR_IDX_Magnetometer8 : BasicApp1_types.h
- SENSOR_IDX_Magnetometer9 : BasicApp1_types.h
- SENSOR_IDX_Orientation14 : BasicApp1_types.h
- SENSOR_IDX_Pedometer16 : BasicApp1_types.h
- SENSOR_IDX_Pedometer17 : BasicApp1_types.h
- SENSOR_IDX_Pressure12 : BasicApp1_types.h
- SENSOR_IDX_Temperature13 : BasicApp1_types.h
- sensor_mode_t : isf_sensors.h
- SENSOR_READY : isf_sensors.h
- Sensor_sensors_en : isf_sensor_configuration.h
- SENSOR_STANDBY : isf_sensors.h
- SENSOR_STATE_CONFIGURED : isf_sensors.h
- SENSOR_STATE_INITIALIZED : isf_sensors.h
- SENSOR_STATE_STARTED : isf_sensors.h
- SENSOR_STATE_UNINITIALIZED : isf_sensors.h
- sensordataHandler_t : BasicApp1_types.h
- SensorEnable_OutConfig0 : SensorEnable.c , SensorEnable.h
- SENSORFS : fusion_config.h
- SensorId_t : isf_sensor_configuration.h
- sensorType : fsl_Sensor_Analog_1_Functions.c
- SET_FIELD : App1.c , rli_project.c , mma8491q.h
- shutdown_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- ShutdownCmd : FXLC95000_1.c , FXLC95000_2.c
- ShutdownSequence : FXLC95000_1.c , FXLC95000_2.c
- SleepApplication : MMA955x_1.c , MMA955x_2.c
- SM_API_ALTERNATE_OFFERED : isf_sm_types.h
- SM_API_ERR_ALREADY_BEGUN : isf_sm_types.h
- SM_API_ERR_BUFFERLOCK_TIMEOUT : isf_sm_types.h
- SM_API_ERR_DATATYPE_NOT_SUPPORTED : isf_sm_types.h
- SM_API_ERR_FIFO_OVER_LIMIT : isf_sm_types.h
- SM_API_ERR_INVALID_HANDLE : isf_sm_types.h
- SM_API_ERR_INVALID_PTR : isf_sm_types.h
- SM_API_ERR_LOCK_CREATION_FAILED : isf_sm_types.h
- SM_API_ERR_MAX_TAPS_PER_SENSOR : isf_sm_types.h
- SM_API_ERR_NO_MEMORY : isf_sm_types.h
- SM_API_ERR_NOT_YET_BEGUN : isf_sm_types.h
- SM_API_ERR_SAMPLE_TAP_RATE : isf_sm_types.h
- SM_API_ERR_SENSOR_ALREADY_INITIALIZED : isf_sm_types.h
- SM_API_ERR_SENSOR_ID : isf_sm_types.h
- SM_API_ERR_SENSOR_INIT_FAILED : isf_sm_types.h
- SM_API_ERR_SENSOR_NOT_AVAIL : isf_sm_types.h
- SM_API_ERR_SETTINGS_TO_USE : isf_sm_types.h
- SM_API_ERR_SUBSCRIBER_COUNT : isf_sm_types.h
- SM_API_ERR_TOKEN_ID : isf_sm_types.h
- SM_BEST_POSSIBLE_SETTINGS : isf_sm_types.h
- SM_CURRENT_SETTINGS : isf_sm_types.h
- SM_GIVEN_SETTINGS : isf_sm_types.h
- SM_MAX_FIFO_DEPTH : isf_sm_types.h
- SM_MAX_SUBSCRIBERS_PER_SENSOR : isf_sm_types.h
- sm_result_t : isf_sm_types.h
- sm_token_t : isf_sm_types.h
- SMALLMODULUS : orientation.c
- SMALLQ0 : orientation.c
- SP_MB0 : ci_protocol_mbox.h
- SP_MB1 : ci_protocol_mbox.h
- SP_MB2 : ci_protocol_mbox.h
- SP_MB3 : ci_protocol_mbox.h
- SP_MB4 : ci_protocol_mbox.h
- SPI_ASYNC : isf_spi_master_adapter.h
- SPI_BUS_0 : isf_sysconf_comms.c
- spi_busHandle : isf_spi_master_adapter.c , isf_sysconf_comms.c
- spi_comm_flag : isf_spi_master_adapter.h
- spi_lock : isf_spi_master_adapter.c , isf_sysconf_comms.c
- SPI_LOCK_COMMON : isf_spi_master_adapter.h
- SPI_LOCK_READ : isf_spi_master_adapter.h
- spi_lock_type : isf_spi_master_adapter.h
- spi_master_adapter_acquire_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_configure() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_config() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_get_state() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_init() : isf_spi_master_adapter.c , isf_spi_master_adapter.h
- spi_master_adapter_read() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_endpoint() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_release_lock() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_start() : isf_spi_master_adapter.c , isf_spi_master_adapter.h
- spi_master_adapter_stop() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_adapter_write() : isf_spi_master_adapter.h , isf_spi_master_adapter.c
- spi_master_busConfig_t : isf_spi_master_types.h
- spi_master_busHandle_t : isf_spi_master_types.h
- spi_master_Endpoint_t : isf_spi_master_adapter.h
- spi_master_readFlags_t : isf_spi_master_adapter.h
- spi_master_slaveInfo_t : isf_spi_master_types.h
- spi_master_writeFlags_t : isf_spi_master_adapter.h
- spi_mater_slaveCmd_t : isf_spi_master_types.h
- SPI_NUM_BUS : isf_sysconf_comms.c
- spi_rdlock : isf_sysconf_comms.c , isf_spi_master_adapter.c
- SPI_SYNC : isf_spi_master_adapter.h
- SPISelect_OutConfig0 : SPISelect.c , SPISelect.h
- start_sensor() : isf_dsa_direct.h , isf_dsa_direct.c
- START_TIMER : fusion_exec.c
- StartDataCmd : FXLC95000_1.c , FXLC95000_2.c
- StartDataSequence : FXLC95000_2.c , FXLC95000_1.c
- startof : fxlc95000.h , App1.c
- STATUS_00_REG : mpl3115.h
- STOP_PERIODIC_READ : rli_project.c
- stop_sensor() : isf_dsa_direct.c , isf_dsa_direct.h
- STOP_TIMER : fusion_exec.c
- STREAM_COCO_BIT : ci_protocol_stream.h
- STREAM_COCO_BIT_MASK : ci_protocol_stream.h
- STREAM_CRC_BYTESIZE : ci_protocol_stream.h
- STREAM_CRC_DISABLED : isf_ci_stream.h
- STREAM_CRC_ENABLED : isf_ci_stream.h
- STREAM_PROTOCOL_CMD_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_CMD_STATUS_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_DISABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_ENABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_STREAMID : ci_protocol_stream.h
- STREAM_PROTOCOL_RECV_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_DEFAULT_ARRAY_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_CMD_ECHO : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_DATASTART : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_RESPDATALENGTH_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_SUBCMD_BYTESIZE : ci_protocol_stream.h
- SubscriptionSettingChoices : isf_sm_types.h
- SubscriptionSettingsChoices_t : isf_sm_types.h
- swdelay() : bus_management.c
- synchCreate : isf_init.c
- sys_channelId_t : isf_sysconf_types.h
- SYS_NUM_CHANNEL_IDS : isf_sysconf_comms.h
- sys_protocolType_t : isf_sysconf_types.h
- SYST_CALIB : isf_systick_defs.h
- SYST_CSR : isf_systick_defs.h
- SYST_CVR : isf_systick_defs.h
- SYST_RVR : isf_systick_defs.h
- SYSTEM_DEVICE_ID : version.h
- SysTick : isf_systick_defs.h
- SysTick_BASE_ADDR : isf_systick_defs.h
- SysTick_BASE_PTR : isf_systick_defs.h
- SysTick_CALIB_REG : isf_systick_defs.h
- SysTick_CSR_REG : isf_systick_defs.h
- SysTick_CVR_REG : isf_systick_defs.h
- SysTick_RVR_REG : isf_systick_defs.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.