| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
isf_AngularVelocity1D_RawCount_t Struct Reference

Standard raw type for single axis accelerometers. More...

`#include <isf_gyrometer_types.h>`

Collaboration diagram for isf_AngularVelocity1D_RawCount_t:

## Data Fields
isf_timestamp_t | timestamp
isf_gyrometer_dps_raw_16count_t | angularVelocity

## Detailed Description

Standard raw type for single axis accelerometers.

Definition at line 44 of file isf_gyrometer_types.h.

## Field Documentation

isf_gyrometer_dps_raw_16count_t angularVelocity

Definition at line 46 of file isf_gyrometer_types.h.

isf_timestamp_t timestamp

Definition at line 45 of file isf_gyrometer_types.h.

The documentation for this struct was generated from the following file:

- SensorGeneric/isf_gyrometer_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.