| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Macros | Variables
ADC1 module documentation

## Macros
#define | FSL_ADC1 0
| Device instance number. More...

## Variables
const adc16_converter_config_t | ADC1_InitConfig0
| ADC configuration declaration. More...
const adc16_hw_cmp_config_t | ADC1_HwConfig0
| HW compare configuration declaration. More...
const adc16_chn_config_t | ADC1_ChnConfig0
| Channel configuration declaration. More...
const adc16_converter_config_t | ADC1_InitConfig0
| ADC configuration declaration. More...
const adc16_hw_cmp_config_t | ADC1_HwConfig0
| HW compare configuration declaration. More...
const adc16_chn_config_t | ADC1_ChnConfig0
| Channel configuration declaration. More...

## Detailed Description

## Macro Definition Documentation

#define FSL_ADC1 0

Device instance number.

Definition at line 76 of file ADC1.h.

Referenced by Analog_1_fsl_Sensor_Generic_Analog_Initialize(), Analog_1_fsl_Sensor_Generic_Analog_Shutdown(), Analog_1_fsl_Sensor_Generic_Analog_StartData(), Analog_1_fsl_Sensor_Generic_AnalogCallback(), and Components_Init().

## Variable Documentation

const adc16_chn_config_t ADC1_ChnConfig0

Initial value:
= {
.chnIdx = kAdc16Chn4b,
.convCompletedIntEnable = false,
.diffConvEnable = false
}

Channel configuration declaration.

Definition at line 81 of file ADC1.c.

Referenced by Analog_1_fsl_Sensor_Generic_Analog_StartData(), and Components_Init().

const adc16_chn_config_t ADC1_ChnConfig0

Channel configuration declaration.

Definition at line 81 of file ADC1.c.

Referenced by Analog_1_fsl_Sensor_Generic_Analog_StartData(), and Components_Init().

const adc16_hw_cmp_config_t ADC1_HwConfig0

Initial value:
= {
.hwCmpEnable = false,
.hwCmpGreaterThanEnable = false,
.hwCmpRangeEnable = false,
.cmpValue1 = 0U,
.cmpValue2 = 0U,
}

HW compare configuration declaration.

Definition at line 72 of file ADC1.c.

const adc16_hw_cmp_config_t ADC1_HwConfig0

HW compare configuration declaration.

Definition at line 72 of file ADC1.c.

const adc16_converter_config_t ADC1_InitConfig0

Initial value:
= {
.lowPowerEnable = false,
.clkDividerMode = kAdc16ClkDividerOf1,
.longSampleTimeEnable = false,
.resolution = kAdc16ResolutionBitOfSingleEndAs8,
.clkSrc = kAdc16ClkSrcOfBusClk,
.asyncClkEnable = false,
.highSpeedEnable = false,
.longSampleCycleMode = kAdc16LongSampleCycleOf24,
.hwTriggerEnable = false,
.refVoltSrc = kAdc16RefVoltSrcOfVref,
.continuousConvEnable = false,
.dmaEnable = false,
}

ADC configuration declaration.

Definition at line 57 of file ADC1.c.

Referenced by Analog_1_fsl_Sensor_Generic_Analog_Initialize(), and Components_Init().

const adc16_converter_config_t ADC1_InitConfig0

ADC configuration declaration.

Definition at line 57 of file ADC1.c.

Referenced by Analog_1_fsl_Sensor_Generic_Analog_Initialize(), and Components_Init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.