| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxls8471_DataBuffer_t Struct Reference
fsl_fxls8471_i2cspi_3D_accel module documentation

This structure defines the dummy DSA data buffer format. More...

`#include <fsl_fxls8471_i2cspi_3D_accel.h>`

Collaboration diagram for fxls8471_DataBuffer_t:

## Data Fields
uint32 | timeStamp
int16 | accel [3]

## Detailed Description

This structure defines the dummy DSA data buffer format.

Definition at line 48 of file fsl_fxls8471_i2cspi_3D_accel.h.

## Field Documentation

int16 accel[3]

The accelerometer data

Definition at line 50 of file fsl_fxls8471_i2cspi_3D_accel.h.

Referenced by fsl_fxls8471_i2cspi_3D_accel_Initialize(), and fsl_fxls8471_i2cspi_3D_accel_PeriodicCallback().

uint32 timeStamp

The time stamp for the data packet.

Definition at line 49 of file fsl_fxls8471_i2cspi_3D_accel.h.

Referenced by fsl_fxls8471_i2cspi_3D_accel_Initialize(), and fsl_fxls8471_i2cspi_3D_accel_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxls8471_i2cspi_3D_accel.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.