| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- c
- d
- f
- i
- j
- l
- m
- n
- p
- q
- r
- s
- t
- u
- x
- y
- z

### - c -

- CHX : matrix.h
- CHY : matrix.h
- CHZ : matrix.h
- CI_CMD_DEVICE_READ : isf_ci.h
- CI_CMD_DEVICE_WRITE : isf_ci.h
- CI_CMD_GET_APP_SUBSCRIPTION : isf_ci.h
- CI_CMD_MAX : isf_ci.h
- CI_CMD_READ_APP_DATA : isf_ci.h
- CI_CMD_READ_APP_STATUS : isf_ci.h
- CI_CMD_READ_CONFIG : isf_ci.h
- CI_CMD_READ_VERSION : isf_ci.h
- CI_CMD_RESET_APP : isf_ci.h
- CI_CMD_STREAM_CREATE_STREAM : isf_ci_stream.h
- CI_CMD_STREAM_DELETE_STREAM : isf_ci_stream.h
- CI_CMD_STREAM_DISABLE_CRC : isf_ci_stream.h
- CI_CMD_STREAM_DISABLE_DATA_UPDATE : isf_ci_stream.h
- CI_CMD_STREAM_ENABLE_CRC : isf_ci_stream.h
- CI_CMD_STREAM_ENABLE_DATA_UPDATE : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_GET_FIRST_STREAMID : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_GET_NEXT_STREAMID : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_NUMBER_STREAMS : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_STREAM_CONFIG : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_TRIGGER_STATE : isf_ci_stream.h
- CI_CMD_STREAM_MAX : isf_ci_stream.h
- CI_CMD_STREAM_RESET : isf_ci_stream.h
- CI_CMD_STREAM_RESET_TRIGGER : isf_ci_stream.h
- CI_CMD_UPDATE_QUICKREAD : isf_ci.h
- CI_CMD_WRITE_CONFIG : isf_ci.h
- CI_CMD_WRITE_SREC_FLASH : isf_ci.h
- CI_ERROR_CB_NOT_REGISTERED : isf_ci.h
- CI_ERROR_COMMAND : isf_ci.h
- CI_ERROR_FIFO_ALLOCATED : isf_ci.h
- CI_ERROR_FIFO_BUSY : isf_ci.h
- CI_ERROR_FIFO_OVERSIZE : isf_ci.h
- CI_ERROR_INVALID_LENGTH : isf_ci.h
- CI_ERROR_MAX : isf_ci.h
- CI_ERROR_NONE : isf_ci.h
- CI_ERROR_PARAM : isf_ci.h
- CI_ESCAPE_STATE_WAIT_1ST_CHAR : task_ci.h
- CI_ESCAPE_STATE_WAIT_2ND_CHAR : task_ci.h
- CI_INVALID_COUNT : isf_ci.h
- CI_PACKET_RECV_STATUS_NO : task_ci.h
- CI_PACKET_RECV_STATUS_YES : task_ci.h
- CI_PROTOCOL_ID_MAX : isf_ci_protocol.h
- CI_PROTOCOL_ID_MBOX : isf_ci_protocol.h
- CI_PROTOCOL_ID_NULL : isf_ci_protocol.h
- CI_PROTOCOL_ID_Protocol1 : isf_ci_protocol.h
- CI_RESP_QUICKREAD : isf_ci.h
- CI_RW_NULL : isf_ci.h
- CI_RW_READ : isf_ci.h
- CI_RW_WRITE : isf_ci.h
- CI_RX_STATE_GETTINGPACKETDATA2 : task_ci.h
- CI_RX_STATE_NULL : task_ci.h
- CI_RX_STATE_WAITFORPACKETMARKER1 : task_ci.h
- CI_STATUS_STREAM_DATA_UPDATE : isf_ci_stream.h
- CI_STATUS_STREAM_DATASETID_NOTUSED : isf_ci_stream.h
- CI_STATUS_STREAM_ERR : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_CRC : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASET_LENGTH_INVALID : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASETID_EXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASETID_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_CMD : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_NUM_PARM : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_PARM : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_NULL_POINTER : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_NUMELEMENTS_INVALID : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_OUT_OF_MEMORY : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_SENDDATA_TO_HOST : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAM_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAMID_EXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAMID_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_MAX : isf_ci_stream.h
- CI_STATUS_STREAM_STREAM_END_OF_LIST : isf_ci_stream.h
- CI_STATUS_STREAM_SUCCESS : isf_ci_stream.h
- CI_TX_STATE_NULL : task_ci.h
- CI_TX_STATE_SEND_ENDMARKER4 : task_ci.h
- CI_TX_STATE_SEND_PACKETDATA2 : task_ci.h
- CI_TX_STATE_SEND_STARTMARKER1 : task_ci.h
- COMM_CHANNEL_I2C1 : isf_sysconf_comms.h
- COMM_CHANNEL_INTERNAL : isf_sysconf_comms.h
- COMM_CHANNEL_SPI1 : isf_sysconf_comms.h
- COMM_CHANNEL_UART2 : isf_sysconf_comms.h
- COMM_ERROR_BUF_SIZE : isf_comm.h
- COMM_ERROR_DEV_CLOSED : isf_comm.h
- COMM_ERROR_INIT : isf_comm.h
- COMM_ERROR_LOCK : isf_comm.h
- COMM_ERROR_NO_ACK : isf_comm.h
- COMM_ERROR_NOEXIST : isf_comm.h
- COMM_ERROR_NULL_PTR : isf_comm.h
- COMM_ERROR_OTHER : isf_comm.h
- COMM_ERROR_STOP : isf_comm.h
- COMM_ERROR_TIME_OUT : isf_comm.h
- COMM_STATE_ARB_LOST : isf_comm.h
- COMM_STATE_ERROR : isf_comm.h
- COMM_STATE_INIT : isf_comm.h
- COMM_STATE_NO_INIT : isf_comm.h
- COMM_STATE_OK : isf_comm.h
- COMM_STATE_STOPPED : isf_comm.h
- CONFIGURE_PERIODIC_READ : rli_project.c
- Custom_1_CTRL_REG1 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_CTRL_REG2 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_DATA_OVERWRITE : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ERROR : fsl_Sensor_Custom_1_Functions.h
- Custom_1_STATUS_00 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SUCCESS : fsl_Sensor_Custom_1_Functions.h
- Custom_1_WHO_AM_I : fsl_Sensor_Custom_1_Functions.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.