| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

OutY.h
Go to the documentation of this file.
1 /* ###################################################################
2 ** This component module is generated by Processor Expert. Do not modify it.
3 ** Filename : OutY.h
4 ** Project : ISF2P2_K64F_MQX_PROJ
5 ** Processor : MK64FN1M0VLL12
6 ** Component : fsl_gpio
7 ** Version : Component 1.2.0, Driver 01.00, CPU db: 3.00.000
8 ** Repository : KSDK 1.2.0
9 ** Compiler : GNU C Compiler
10 ** Date/Time : 2016-10-06, 13:38, # CodeGen: 0
11 ** Contents :
12 ** GPIO_DRV_Init - void GPIO_DRV_Init(const gpio_input_pin_user_config_t * inputPins,const...
13 ** GPIO_DRV_InputPinInit - void GPIO_DRV_InputPinInit(const gpio_input_pin_user_config_t * inputPin);
14 ** GPIO_DRV_OutputPinInit - void GPIO_DRV_OutputPinInit(const gpio_output_pin_user_config_t * outputPin);
15 ** GPIO_DRV_GetPinDir - gpio_pin_direction_t GPIO_DRV_GetPinDir(uint32_t pinName);
16 ** GPIO_DRV_SetPinDir - void GPIO_DRV_SetPinDir(uint32_t pinName,gpio_pin_direction_t direction);
17 ** GPIO_DRV_WritePinOutput - void GPIO_DRV_WritePinOutput(uint32_t pinName,uint32_t output);
18 ** GPIO_DRV_SetPinOutput - void GPIO_DRV_SetPinOutput(uint32_t pinName);
19 ** GPIO_DRV_ClearPinOutput - void GPIO_DRV_ClearPinOutput(uint32_t pinName);
20 ** GPIO_DRV_TogglePinOutput - void GPIO_DRV_TogglePinOutput(uint32_t pinName);
21 ** GPIO_DRV_ReadPinInput - uint32_t GPIO_DRV_ReadPinInput(uint32_t pinName);
22 ** GPIO_DRV_SetDigitalFilterCmd - void GPIO_DRV_SetDigitalFilterCmd(uint32_t pinName,bool isDigitalFilterEnabled);
23 ** GPIO_DRV_IsPinIntPending - bool GPIO_DRV_IsPinIntPending(uint32_t pinName);
24 ** GPIO_DRV_ClearPinIntFlag - void GPIO_DRV_ClearPinIntFlag(uint32_t pinName);
25 **
26 ** Copyright : 1997 - 2015 Freescale Semiconductor, Inc.
27 ** All Rights Reserved.
28 **
29 ** Redistribution and use in source and binary forms, with or without modification,
30 ** are permitted provided that the following conditions are met:
31 **
32 ** o Redistributions of source code must retain the above copyright notice, this list
33 ** of conditions and the following disclaimer.
34 **
35 ** o Redistributions in binary form must reproduce the above copyright notice, this
36 ** list of conditions and the following disclaimer in the documentation and/or
37 ** other materials provided with the distribution.
38 **
39 ** o Neither the name of Freescale Semiconductor, Inc. nor the names of its
40 ** contributors may be used to endorse or promote products derived from this
41 ** software without specific prior written permission.
42 **
43 ** THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
44 ** ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
45 ** WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
46 ** DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
47 ** ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
48 ** (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
49 ** LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
50 ** ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
51 ** (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
52 ** SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
53 **
54 ** http: www.freescale.com
55 ** mail: support@freescale.com
56 ** ###################################################################*/
57 /*!
58 ** @file OutY.h
59 ** @version 01.00
60 */
61 /*!
62 ** @addtogroup OutY_module OutY module documentation
63 ** @{
64 */
65
66 #ifndef __OutY_H
67 #define __OutY_H
68
69 /* MODULE OutY. */
70
71 /* Include inherited beans */
72 #include "clockMan1.h"
73 #include "fsl_gpio_driver.h"
74
75
76 /*! @brief Configuration structure 0 for input pins */
77 extern const gpio_input_pin_user_config_t OutY_OutConfig0[];
78
79
80 /*! @brief Pin names */
81 enum _OutY_pinNames{
82 J1_5 = GPIO_MAKE_PIN(GPIOC_IDX, 1U),
83 };
84
85
86 #endif
87
88 /*!
89 ** @}
90 */
91 /*
92 ** ###################################################################
93 **
94 ** This file was created by Processor Expert 10.5 [05.21]
95 ** for the Freescale Kinetis series of microcontrollers.
96 **
97 ** ###################################################################
98 */
clockMan1.h
OutY_OutConfig0
const gpio_input_pin_user_config_t OutY_OutConfig0[]
Configuration structure 0 for input pins.
Definition: OutY.c:56
_OutY_pinNames
_OutY_pinNames
Pin names.
Definition: OutY.h:81
J1_5
Definition: OutY.h:82
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.