| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - c -

- ccitt_crc16_cal() : crc.h , crc.c
- char_t : isf_types.h
- ChipSelect_OutConfig0 : ChipSelect.c , ChipSelect.h , SPIChipSelect.c , SPIChipSelect.h
- CHX : matrix.h
- CHY : matrix.h
- CHZ : matrix.h
- CI_ALLOC_MEM_ZERO : task_ci.h
- ci_callback : ci_protocol_mbox.c , ISFCore1.c
- CI_CMD_DEBUG_LOOPBACK : ci_protocol_mbox.h
- CI_CMD_DEVICE_READ : isf_ci.h
- CI_CMD_DEVICE_WRITE : isf_ci.h
- CI_CMD_GET_APP_SUBSCRIPTION : isf_ci.h
- CI_CMD_LAST : isf_ci.h
- CI_CMD_MAX : isf_ci.h
- CI_CMD_READ_APP_DATA : isf_ci.h
- CI_CMD_READ_APP_STATUS : isf_ci.h
- CI_CMD_READ_CONFIG : isf_ci.h
- CI_CMD_READ_VERSION : isf_ci.h
- CI_CMD_RESET_APP : isf_ci.h
- CI_CMD_STREAM_CREATE_STREAM : isf_ci_stream.h
- CI_CMD_STREAM_DELETE_STREAM : isf_ci_stream.h
- CI_CMD_STREAM_DISABLE_CRC : isf_ci_stream.h
- CI_CMD_STREAM_DISABLE_DATA_UPDATE : isf_ci_stream.h
- CI_CMD_STREAM_ENABLE_CRC : isf_ci_stream.h
- CI_CMD_STREAM_ENABLE_DATA_UPDATE : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_GET_FIRST_STREAMID : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_GET_NEXT_STREAMID : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_NUMBER_STREAMS : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_STREAM_CONFIG : isf_ci_stream.h
- CI_CMD_STREAM_GETINFO_TRIGGER_STATE : isf_ci_stream.h
- CI_CMD_STREAM_MAX : isf_ci_stream.h
- CI_CMD_STREAM_RESET : isf_ci_stream.h
- CI_CMD_STREAM_RESET_TRIGGER : isf_ci_stream.h
- CI_CMD_UPDATE_QUICKREAD : isf_ci.h
- CI_CMD_WRITE_CONFIG : isf_ci.h
- CI_CMD_WRITE_SREC_FLASH : isf_ci.h
- ci_commands_enum : isf_ci.h
- ci_commands_stream_enum : isf_ci_stream.h
- CI_COPY_MEM : task_ci.h
- CI_ERROR_CB_NOT_REGISTERED : isf_ci.h
- CI_ERROR_COMMAND : isf_ci.h
- CI_ERROR_FIFO_ALLOCATED : isf_ci.h
- CI_ERROR_FIFO_BUSY : isf_ci.h
- CI_ERROR_FIFO_OVERSIZE : isf_ci.h
- CI_ERROR_INVALID_LENGTH : isf_ci.h
- CI_ERROR_MAX : isf_ci.h
- CI_ERROR_NONE : isf_ci.h
- CI_ERROR_PARAM : isf_ci.h
- ci_escape_state_enum : task_ci.h
- CI_ESCAPE_STATE_WAIT_1ST_CHAR : task_ci.h
- CI_ESCAPE_STATE_WAIT_2ND_CHAR : task_ci.h
- CI_FREE_MEM : task_ci.h
- ci_funcp_t : isf_ci.h
- ci_get_first_mailbox : ci_protocol_mbox.h
- ci_get_protocol_id : task_ci.h
- ci_get_wr_appid : ci_protocol_mbox.h
- ci_get_wr_cmd : ci_protocol_mbox.h
- ci_get_wr_cmdId : ci_protocol_mbox.h
- ci_get_wr_cnt : ci_protocol_mbox.h
- ci_get_wr_offset : ci_protocol_mbox.h
- ci_init() : task_ci.c , isf_ci.h , isf_init.h
- ci_insert_crc : ci_protocol_mbox.h
- CI_INVALID_COUNT : isf_ci.h
- CI_MAX_FLASH_BYTES : isf_ci.h
- CI_MAX_PROTOCOL : isf_ci_protocol.h
- ci_mbox_init() : ci_protocol_mbox.h , ci_protocol_mbox.c , isf_ci_protocol.c
- CI_MIN_RX_BYTES : isf_ci_protocol.h
- CI_NON_STREAMING_MODE : ci_protocol_mbox.h
- CI_PACKET_MARKER : task_ci.h
- CI_PACKET_RECV_STATUS_NO : task_ci.h
- ci_packet_recv_status_t : task_ci.h
- CI_PACKET_RECV_STATUS_YES : task_ci.h
- ci_protocol_callback_funcp_t : isf_ci_protocol.h
- ci_protocol_CB_mbox() : ci_protocol_mbox.h , ci_protocol_mbox.c , isf_ci_protocol.c
- ci_protocol_CB_stream() : isf_ci_stream.h , ci_protocol_stream.c , isf_ci_protocol.c
- CI_PROTOCOL_DATA_OFFSET : isf_ci_protocol.h
- CI_PROTOCOL_ID_INDEX : isf_ci_protocol.h
- ci_protocol_id_internal_enum : isf_ci_protocol.h
- CI_PROTOCOL_ID_MAX : isf_ci_protocol.h
- CI_PROTOCOL_ID_MBOX : isf_ci_protocol.h
- CI_PROTOCOL_ID_NULL : isf_ci_protocol.h
- CI_PROTOCOL_ID_Protocol1 : isf_ci_protocol.h
- CI_PROTOCOL_ID_SIZE : isf_ci_protocol.h
- ci_protocol_init_funcp_t : isf_ci_protocol.h
- ci_protocol_initdata_ptr_t : isf_ci_protocol.h
- ci_protocol_initptr_table : isf_ci_protocol.c , task_ci.c
- ci_protocol_table : isf_ci_protocol.c , task_ci.c
- ci_qr_update() : ci_protocol_mbox.c
- CI_READ_WRITE_ADDR_LEN : fsl_fxlc95000_i2cspi_pedo.c
- CI_READ_WRITE_HDR_LEN : fsl_fxlc95000_i2cspi_pedo.c
- CI_READ_WRITE_MAX_LEN : fsl_fxlc95000_i2cspi_pedo.c
- ci_recv_state_t : task_ci.h
- CI_RESP_QUICKREAD : isf_ci.h
- ci_response_enum : isf_ci.h
- ci_response_stream_enum : isf_ci_stream.h
- ci_response_t : isf_ci.h
- ci_rw_enum : isf_ci.h
- CI_RW_NULL : isf_ci.h
- CI_RW_READ : isf_ci.h
- CI_RW_WRITE : isf_ci.h
- CI_RX_STATE_GETTINGPACKETDATA2 : task_ci.h
- CI_RX_STATE_NULL : task_ci.h
- CI_RX_STATE_WAITFORPACKETMARKER1 : task_ci.h
- ci_send_packet() : task_ci.h , task_ci.c
- ci_status_enum : isf_ci.h
- CI_STATUS_STREAM_DATA_UPDATE : isf_ci_stream.h
- CI_STATUS_STREAM_DATASETID_NOTUSED : isf_ci_stream.h
- CI_STATUS_STREAM_ERR : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_CRC : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASET_LENGTH_INVALID : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASETID_EXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_DATASETID_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_CMD : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_NUM_PARM : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_INVALID_PARM : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_NULL_POINTER : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_NUMELEMENTS_INVALID : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_OUT_OF_MEMORY : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_SENDDATA_TO_HOST : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAM_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAMID_EXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_ERR_STREAMID_NOEXISTS : isf_ci_stream.h
- CI_STATUS_STREAM_MAX : isf_ci_stream.h
- CI_STATUS_STREAM_SPECIFIC_ERROR : isf_ci_stream.h
- CI_STATUS_STREAM_SPECIFIC_STATUS : isf_ci_stream.h
- CI_STATUS_STREAM_STREAM_END_OF_LIST : isf_ci_stream.h
- CI_STATUS_STREAM_SUCCESS : isf_ci_stream.h
- ci_status_t : isf_ci.h
- ci_stream_config_t : isf_ci_stream.h
- CI_STREAM_DATASET_ID_BYTESIZE : ci_protocol_stream.h
- ci_stream_element_t : isf_ci_stream.h
- ci_stream_get_host_cmd : ci_protocol_stream.h
- ci_stream_get_host_data : ci_protocol_stream.h
- ci_stream_get_num_element_bytes() : ci_protocol_stream.c
- ci_stream_get_num_trig_bytes() : ci_protocol_stream.c
- ci_stream_init() : isf_ci_stream.h , ci_protocol_stream.c , isf_ci_protocol.c
- ci_stream_instance_t : ci_protocol_stream.h
- CI_STREAM_NUMELEMENTS_BYTESIZE : ci_protocol_stream.h
- CI_STREAM_OUTPUTPACKET_LENGTH_BYTESIZE : ci_protocol_stream.h
- CI_STREAM_OUTPUTPACKET_STREAMID_BYTESIZE : ci_protocol_stream.h
- CI_STREAM_PROTOCOL_ID_BYTESIZE : ci_protocol_stream.h
- CI_STREAMING_MODE : ci_protocol_mbox.h
- CI_task() : task_ci.c
- CI_TASK_NAME : task_ci.c
- CI_TASK_PRIORITY : task_ci.c
- CI_TASK_STACK_SIZE : task_ci.c
- CI_TX_STATE_NULL : task_ci.h
- CI_TX_STATE_SEND_ENDMARKER4 : task_ci.h
- CI_TX_STATE_SEND_PACKETDATA2 : task_ci.h
- CI_TX_STATE_SEND_STARTMARKER1 : task_ci.h
- ci_tx_state_t : task_ci.h
- ci_update_first_data_mb() : ci_protocol_mbox.c
- clockMan1_InitConfig0 : clockMan1.c , clockMan1.h
- clockMan1_InitConfig1 : clockMan1.h , clockMan1.c
- clockMan1_InitConfig2 : clockMan1.c , clockMan1.h
- clockMan1_InitConfig3 : clockMan1.c , clockMan1.h
- clockMan1_InitConfig4 : clockMan1.c , clockMan1.h
- clockMan1_InitConfig5 : clockMan1.h , clockMan1.c
- clockMan1_osc0_Config : clockMan1.c , clockMan1.h
- close_channel() : rli_project.c
- cmd_createstream_get_numelements : ci_protocol_stream.h
- cmd_createstream_get_streamID : ci_protocol_stream.h
- cmd_createstream_get_trigmask_ptr : ci_protocol_stream.h
- CMD_PACKET_BITS : ci_protocol_mbox.h
- cmdBuffer_t : rli_project.c
- COCO_BIT : ci_protocol_mbox.h
- COCO_BIT_MASK : ci_protocol_mbox.h
- comm_Address_t : isf_comm.h
- COMM_CHANNEL_I2C1 : isf_sysconf_comms.h
- COMM_CHANNEL_INTERNAL : isf_sysconf_comms.h
- COMM_CHANNEL_SPI1 : isf_sysconf_comms.h
- COMM_CHANNEL_UART2 : isf_sysconf_comms.h
- COMM_ERROR_BUF_SIZE : isf_comm.h
- COMM_ERROR_DEV_CLOSED : isf_comm.h
- COMM_ERROR_INIT : isf_comm.h
- COMM_ERROR_LOCK : isf_comm.h
- COMM_ERROR_NO_ACK : isf_comm.h
- COMM_ERROR_NOEXIST : isf_comm.h
- COMM_ERROR_NULL_PTR : isf_comm.h
- COMM_ERROR_OTHER : isf_comm.h
- COMM_ERROR_STOP : isf_comm.h
- COMM_ERROR_TIME_OUT : isf_comm.h
- comm_Error_vals : isf_comm.h
- comm_Flags_t : isf_comm.h
- comm_Id_t : isf_comm.h
- COMM_STATE_ARB_LOST : isf_comm.h
- COMM_STATE_ERROR : isf_comm.h
- COMM_STATE_INIT : isf_comm.h
- COMM_STATE_NO_INIT : isf_comm.h
- COMM_STATE_OK : isf_comm.h
- COMM_STATE_STOPPED : isf_comm.h
- comm_State_t : isf_comm.h
- comm_State_vals : isf_comm.h
- Components_Init() : Cpu.c
- CONFIGURE_PERIODIC_READ : rli_project.c
- configure_sensor() : isf_dsa_direct.c , isf_dsa_direct.h
- configuredADCh : fsl_Sensor_Analog_1_Functions.c
- ConfigureMBoxCmd1 : FXLC95000_1.c , FXLC95000_2.c
- ConfigureSequence : FXLC95000_1.c , FXLC95000_2.c
- ConfigWritePreamble : FXLC95000_2.c , FXLC95000_1.c
- convert_sensor_data() : isf_dsa_direct.h , isf_dsa_direct.c
- convertPressureToAltitude() : fsl_mpl3115_i2c_1D_press.c
- CORRUPTMATRIX : matrix.c
- CORRUPTQUAT : orientation.c
- CPU_COMPONENTS_INIT : Cpu.h
- CPU_HARDWARE_INIT : Cpu.h
- CPU_INIT_CONFIG : Cpu.h
- CPU_PERIPHERALS_INIT : Cpu.h
- CTRL_POWER_MASK : App1.c
- CTRL_POWER_SHIFT : App1.c
- CTRL_QREN_MASK : App1.c
- CTRL_QREN_SHIFT : App1.c
- CTRL_RESET_MASK : App1.c
- CTRL_RESET_SHIFT : App1.c
- CTRL_STATE_MASK : App1.c
- CTRL_STATE_SHIFT : App1.c
- Custom_1__Void_() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_ACTIVE_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_Adapter : Custom_1.c , Custom_1.h
- Custom_1_ASLP_RATE_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ASLP_RATE_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ConfigTable_Element_t : Custom_1.h
- Custom_1_CONVERT_FIXED_FACTOR : fsl_Sensor_Custom_1_Functions.c
- Custom_1_CONVERT_FLOAT_FACTOR : fsl_Sensor_Custom_1_Functions.c
- Custom_1_CTRL_REG1 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_CTRL_REG2 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_DATA_OVERWRITE : fsl_Sensor_Custom_1_Functions.h
- Custom_1_DATA_TYPE : fsl_Sensor_Custom_1_Functions.h
- Custom_1_device_check_whoami() : Custom_1.h
- Custom_1_device_wait_for_active() : Custom_1.h
- Custom_1_DeviceInfo : fsl_Sensor_Custom_1_Functions.c , Custom_1.h
- Custom_1_DR_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_DR_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ERROR : fsl_Sensor_Custom_1_Functions.h
- Custom_1_fixed_Custom_converter() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_float_Custom_converter() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_FREAD_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_FREAD_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_fsl_Sensor_Custom_Configure() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_Convert() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_EndData() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_Initialize() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_PeriodicCallback() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_Shutdown() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_StartData() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_fsl_Sensor_Custom_ValidateSettings() : fsl_Sensor_Custom_1_Functions.c
- Custom_1_GET_FIELD : fsl_Sensor_Custom_1_Functions.h
- Custom_1_MODS_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_MODS_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_RST_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_RST_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_Sensor_Specific_Config : fsl_Sensor_Custom_1_Functions.c , Custom_1.h
- Custom_1_SET_FIELD : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SLPE_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SLPE_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SMODS_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SMODS_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ST_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ST_SHIFT : fsl_Sensor_Custom_1_Functions.h
- Custom_1_STATUS_00 : fsl_Sensor_Custom_1_Functions.h
- Custom_1_Status_t : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SUCCESS : fsl_Sensor_Custom_1_Functions.h
- Custom_1_SupportedDataTypes : Custom_1.h , fsl_Sensor_Custom_1_Functions.c
- Custom_1_SupportedSensorTypes : fsl_Sensor_Custom_1_Functions.c , Custom_1.h
- Custom_1_WHO_AM_I : fsl_Sensor_Custom_1_Functions.h
- Custom_1_Who_Am_I_Values : fsl_Sensor_Custom_1_Functions.h , fsl_Sensor_Custom_1_Functions.c
- Custom_1_ZYXDR_MASK : fsl_Sensor_Custom_1_Functions.h
- Custom_1_ZYXDR_SHIFT : fsl_Sensor_Custom_1_Functions.h
- isf_ci_app_read() : ci_protocol_mbox.c , isf_ci.h
- isf_ci_app_write() : ci_protocol_mbox.c , isf_ci.h
- isf_ci_get_recv_size() : task_ci.c , isf_ci_protocol.c
- isf_ci_qr_update() : ci_protocol_mbox.c , isf_ci.h
- isf_ci_stream_create() : isf_ci_stream.h , ci_protocol_stream.c
- isf_ci_stream_delete() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_get() : ci_protocol_stream.c
- isf_ci_stream_get_config() : isf_ci_stream.h
- isf_ci_stream_get_first() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_get_next() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_get_num_streams() : isf_ci_stream.h , ci_protocol_stream.c
- isf_ci_stream_get_trigger() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_reset_trigger() : isf_ci_stream.h , ci_protocol_stream.c
- isf_ci_stream_set_CRC() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_set_stream_disable() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_set_stream_enable() : ci_protocol_stream.c , isf_ci_stream.h
- isf_ci_stream_update_data() : ci_protocol_stream.c , isf_ci_stream.h
- isf_commit_id : isf.c
- isf_Custom_1_fixed_data_t : fsl_Sensor_Custom_1_Functions.h
- isf_Custom_1_float_data_t : fsl_Sensor_Custom_1_Functions.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.