| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Typedefs
isf_gyrometer_types.h File Reference

The isf_gyrometer_types.h file contains the ISF data type definitions for use with the ISF generic gyrometer fixed and floating point interface. More...

`#include <isf_sensor_base_types.h>`
Include dependency graph for isf_gyrometer_types.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | isf_AngularVelocity1D_EngFixed_t
| Standard fixed type for single axis accelerometers. More...
struct | isf_AngularVelocity2D_EngFixed_t
| Standard fixed type for two axis accelerometers. More...
struct | isf_AngularVelocity3D_EngFixed_t
| Standard fixed type for three axis accelerometers. More...
struct | isf_AngularVelocity1D_RawCount_t
| Standard raw type for single axis accelerometers. More...
struct | isf_AngularVelocity2D_RawCount_t
| Standard raw type for two axes accelerometers. More...
struct | isf_AngularVelocity3D_RawCount_t
| Standard raw type for three axes accelerometers. More...
struct | isf_AngularVelocity1D__float_t
| Standard float type for single axis accelerometers. More...
struct | isf_AngularVelocity2D__float_t
| Standard float type for two axis accelerometers. More...
struct | isf_AngularVelocity3D__float_t
| Standard float type for three axis accelerometers. More...

## Typedefs
typedef int32 | isf_gyrometer_dps_fixed_32s1i16_t
| ISF sensors standard fixed point gyrometer type in degrees per second using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the fractional portion and the MSB is used as a sign bit. the LSB is therefore ~1.5259E-05 dps. The type can contain accelerations in the +/- 32768 dps range. More...
typedef int16 | isf_gyrometer_dps_raw_16count_t
typedef float | isf_gyrometer_dps_float_t
| ISF sensors standard fixed point gyrometer type in degrees per second. More...

## Detailed Description

The isf_gyrometer_types.h file contains the ISF data type definitions for use with the ISF generic gyrometer fixed and floating point interface.

Copyright
  Copyright (c) 2015, Freescale Semiconductor, Inc.

Definition in file isf_gyrometer_types.h.

## Typedef Documentation

typedef int32 isf_gyrometer_dps_fixed_32s1i16_t

ISF sensors standard fixed point gyrometer type in degrees per second using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the fractional portion and the MSB is used as a sign bit. the LSB is therefore ~1.5259E-05 dps. The type can contain accelerations in the +/- 32768 dps range.

Definition at line 22 of file isf_gyrometer_types.h.

typedef float isf_gyrometer_dps_float_t

ISF sensors standard fixed point gyrometer type in degrees per second.

Definition at line 61 of file isf_gyrometer_types.h.

typedef int16 isf_gyrometer_dps_raw_16count_t

Definition at line 42 of file isf_gyrometer_types.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.