| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
mag3110_DataBuffer_t Struct Reference
fsl_mag3110_i2c_3D_mag module documentation

This structure defines the dummy DSA data buffer format. More...

`#include <fsl_mag3110_i2c_3D_mag.h>`

Collaboration diagram for mag3110_DataBuffer_t:

## Data Fields
uint32 | timeStamp
int16 | mag [3]
uint8 | addr

## Detailed Description

This structure defines the dummy DSA data buffer format.

Definition at line 23 of file fsl_mag3110_i2c_3D_mag.h.

## Field Documentation

uint8 addr

The device "address" can uniquely identify the sensor

Definition at line 26 of file fsl_mag3110_i2c_3D_mag.h.

Referenced by fsl_mag3110_i2c_3D_mag_Initialize().

int16 mag[3]

The magnetometer data

Definition at line 25 of file fsl_mag3110_i2c_3D_mag.h.

Referenced by fsl_mag3110_i2c_3D_mag_Initialize(), and fsl_mag3110_i2c_3D_mag_PeriodicCallback().

uint32 timeStamp

The time stamp for the data packet.

Definition at line 24 of file fsl_mag3110_i2c_3D_mag.h.

Referenced by fsl_mag3110_i2c_3D_mag_Initialize(), and fsl_mag3110_i2c_3D_mag_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_mag3110_i2c_3D_mag.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.