| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

App1.h
Go to the documentation of this file.
1 /* ###################################################################
2 ** This component module is generated by Processor Expert. Do not modify it.
3 ** Filename : App1.h
4 ** CDE edition : Standard
5 ** Project : ISF2P2_K64F_MQX_PROJ
6 ** Processor : MK64FN1M0VLL12
7 ** Component : ISF_KSDK_EmbApp
8 ** Version : Component 02.500, Driver 02.00, CPU db: 3.00.000
9 ** Repository : My Components
10 ** Compiler : GNU C Compiler
11 ** Date/Time : 2016-10-06, 13:38, # CodeGen: 0
12 ** Abstract :
13 **
14 ** Settings :
15 ** Component Name : App1
16 ** Main Application Settings :
17 ** App ID : 2
18 ** Sensor Signalling Method : AnySensor
19 ** Processed Data Buffer Size : 34
20 ** App Control Register :
21 ** Initial Power : Normal Power
22 ** Quick Read Output Enabled : no
23 ** Initial State : STOPPED_UNSUBSCRIBED
24 ** Application Version Number : 0100
25 ** Additional User-Defined App Info :
26 ** Host Interface :
27 ** Host Command Interface Supported : yes
28 ** User Defined Host Commands : 0
29 ** ISF_Core : ISFCore1
30 ** App Task Priority : 11
31 ** App Task Stack Size : 1200
32 ** Subscription List : 20
33 ** Sensor Subscription :
34 ** Sensor Type : Accelerometer
35 ** Selected Sensor : FXLC95000_1
36 ** Settings To Use : UseGiven
37 ** Sample Period : 10000
38 ** Sensor Data Format : Raw Sensor Format
39 ** Sensor Data Type : Native Sensor Output
40 ** FIFO Depth : 1
41 ** Sensor Subscription :
42 ** Sensor Type : Accelerometer
43 ** Selected Sensor : FXLC95000_2
44 ** Settings To Use : UseGiven
45 ** Sample Period : 10000
46 ** Sensor Data Format : Raw Sensor Format
47 ** Sensor Data Type : Native Sensor Output
48 ** FIFO Depth : 1
49 ** Sensor Subscription :
50 ** Sensor Type : Accelerometer
51 ** Selected Sensor : FXLS8471_1
52 ** Settings To Use : UseGiven
53 ** Sample Period : 10000
54 ** Sensor Data Format : Raw Sensor Format
55 ** Sensor Data Type : Native Sensor Output
56 ** FIFO Depth : 1
57 ** Sensor Subscription :
58 ** Sensor Type : Accelerometer
59 ** Selected Sensor : FXLS8471_2
60 ** Settings To Use : UseGiven
61 ** Sample Period : 10000
62 ** Sensor Data Format : Raw Sensor Format
63 ** Sensor Data Type : Native Sensor Output
64 ** FIFO Depth : 1
65 ** Sensor Subscription :
66 ** Sensor Type : Accelerometer
67 ** Selected Sensor : FXLS8952_1
68 ** Settings To Use : UseGiven
69 ** Sample Period : 10000
70 ** Sensor Data Format : Raw Sensor Format
71 ** Sensor Data Type : Native Sensor Output
72 ** FIFO Depth : 1
73 ** Sensor Subscription :
74 ** Sensor Type : Accelerometer
75 ** Selected Sensor : FXOS8700_1
76 ** Settings To Use : UseGiven
77 ** Sample Period : 10000
78 ** Sensor Data Format : Raw Sensor Format
79 ** Sensor Data Type : Native Sensor Output
80 ** FIFO Depth : 1
81 ** Sensor Subscription :
82 ** Sensor Type : Accelerometer
83 ** Selected Sensor : MMA8491Q_1
84 ** Settings To Use : UseGiven
85 ** Sample Period : 10000
86 ** Sensor Data Format : Raw Sensor Format
87 ** Sensor Data Type : Native Sensor Output
88 ** FIFO Depth : 1
89 ** Sensor Subscription :
90 ** Sensor Type : Accelerometer
91 ** Selected Sensor : MMA865x_1
92 ** Settings To Use : UseGiven
93 ** Sample Period : 10000
94 ** Sensor Data Format : Raw Sensor Format
95 ** Sensor Data Type : Native Sensor Output
96 ** FIFO Depth : 1
97 ** Sensor Subscription :
98 ** Sensor Type : Magnetometer
99 ** Selected Sensor : FXOS8700_2
100 ** Settings To Use : UseGiven
101 ** Sample Period : 10000
102 ** Sensor Data Format : Raw Sensor Format
103 ** Sensor Data Type : Native Sensor Output
104 ** FIFO Depth : 1
105 ** Sensor Subscription :
106 ** Sensor Type : Magnetometer
107 ** Selected Sensor : MAG3110_1
108 ** Settings To Use : UseGiven
109 ** Sample Period : 200000
110 ** Sensor Data Format : Raw Sensor Format
111 ** Sensor Data Type : Native Sensor Output
112 ** FIFO Depth : 1
113 ** Sensor Subscription :
114 ** Sensor Type : Gyrometer
115 ** Selected Sensor : FXAS21002_1
116 ** Settings To Use : UseGiven
117 ** Sample Period : 10000
118 ** Sensor Data Format : Raw Sensor Format
119 ** Sensor Data Type : Native Sensor Output
120 ** FIFO Depth : 1
121 ** Sensor Subscription :
122 ** Sensor Type : Gyrometer
123 ** Selected Sensor : FXAS21002_2
124 ** Settings To Use : UseGiven
125 ** Sample Period : 10000
126 ** Sensor Data Format : Raw Sensor Format
127 ** Sensor Data Type : Native Sensor Output
128 ** FIFO Depth : 1
129 ** Sensor Subscription :
130 ** Sensor Type : Pressure
131 ** Selected Sensor : MPL3115_1
132 ** Settings To Use : UseGiven
133 ** Sample Period : 10000
134 ** Sensor Data Format : Raw Sensor Format
135 ** Sensor Data Type : Native Sensor Output
136 ** FIFO Depth : 1
137 ** Sensor Subscription :
138 ** Sensor Type : Temperature
139 ** Selected Sensor : MPL3115_1
140 ** Settings To Use : UseGiven
141 ** Sample Period : 10000
142 ** Sensor Data Format : Raw Sensor Format
143 ** Sensor Data Type : Native Sensor Output
144 ** FIFO Depth : 1
145 ** Sensor Subscription :
146 ** Sensor Type : Orientation
147 ** Selected Sensor : ORIENT_1
148 ** Settings To Use : UseGiven
149 ** Sample Period : 10000
150 ** Sensor Data Format : Raw Sensor Format
151 ** Sensor Data Type : Native Sensor Output
152 ** FIFO Depth : 1
153 ** Sensor Subscription :
154 ** Sensor Type : Altitude
155 ** Selected Sensor : MPL3115_1
156 ** Settings To Use : UseGiven
157 ** Sample Period : 10000
158 ** Sensor Data Format : Raw Sensor Format
159 ** Sensor Data Type : Native Sensor Output
160 ** FIFO Depth : 1
161 ** Sensor Subscription :
162 ** Sensor Type : Pedometer
163 ** Selected Sensor : MMA955x_1
164 ** Settings To Use : UseGiven
165 ** Sample Period : 8192
166 ** Sensor Data Format : Raw Sensor Format
167 ** Sensor Data Type : Native Sensor Output
168 ** FIFO Depth : 1
169 ** Sensor Subscription :
170 ** Sensor Type : Pedometer
171 ** Selected Sensor : MMA955x_2
172 ** Settings To Use : UseGiven
173 ** Sample Period : 8192
174 ** Sensor Data Format : Raw Sensor Format
175 ** Sensor Data Type : Native Sensor Output
176 ** FIFO Depth : 1
177 ** Sensor Subscription :
178 ** Sensor Type : Custom
179 ** Selected Sensor : Custom_1
180 ** Settings To Use : UseGiven
181 ** Sample Period : 10000
182 ** Sensor Data Format : Raw Sensor Format
183 ** Sensor Data Type : Native Sensor Output
184 ** FIFO Depth : 1
185 ** Sensor Subscription :
186 ** Sensor Type : Analog
187 ** Selected Sensor : Analog_1
188 ** Settings To Use : UseGiven
189 ** Sample Period : 10000
190 ** Sensor Data Format : Raw Sensor Format
191 ** Sensor Data Type : Native Sensor Output
192 ** FIFO Depth : 1
193 ** Contents :
194 ** No public methods
195 **
196 ** (c) Copyright Freescale Semiconductor, Inc., 2015,
197 **
198 http://www.freescale.com
199 ** ###################################################################*/
200 /*!
201 ** @file App1.h
202 ** @version 02.00
203 ** @brief
204 **
205 */
206 /*!
207 ** @addtogroup App1_module App1 module documentation
208 ** @{
209 */
210
211 #ifndef __App1_H
212 #define __App1_H
213
214 /* MODULE App1. */
215
216 /* Include inherited components */
217 #include "ISFCore1.h"
218 #include "FXLC95000_1.h"
219 #include "FXLC95000_2.h"
220 #include "FXLS8471_1.h"
221 #include "FXLS8471_2.h"
222 #include "FXLS8952_1.h"
223 #include "FXOS8700_1.h"
224 #include "MMA8491Q_1.h"
225 #include "MMA865x_1.h"
226 #include "FXOS8700_2.h"
227 #include "MAG3110_1.h"
228 #include "FXAS21002_1.h"
229 #include "FXAS21002_2.h"
230 #include "MPL3115_1.h"
231 #include "MPL3115_1.h"
232 #include "ORIENT_1.h"
233 #include "MPL3115_1.h"
234 #include "MMA955x_1.h"
235 #include "MMA955x_2.h"
236 #include "Custom_1.h"
237 #include "Analog_1.h"
238 #include "App1_types.h"
239
240 #include "Cpu.h"
241
242
243
244 void App1_init();
245 void App1_MainTask(void);
246
247
248 /* END App1. */
249
250 #endif
251 /* ifndef __App1_H */
252 /*!
253 ** @}
254 */
255 /*
256 ** ###################################################################
257 **
258 ** This file was created by Processor Expert 10.5 [05.21]
259 ** for the Freescale Kinetis series of microcontrollers.
260 **
261 ** ###################################################################
262 */
Cpu.h
ISFCore1.h
FXAS21002_1.h
ORIENT_1.h
App1_init
void App1_init(void)
Definition: App1.c:397
App1_MainTask
void App1_MainTask(void)
Definition: App1.c:426
MPL3115_1.h
Custom_1.h
MMA8491Q_1.h
FXLS8471_2.h
MAG3110_1.h
Analog_1.h
FXLS8471_1.h
MMA955x_2.h
FXLS8952_1.h
FXOS8700_2.h
MMA865x_1.h
FXLC95000_2.h
MMA955x_1.h
FXLC95000_1.h
FXOS8700_1.h
App1_types.h
FXAS21002_2.h
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.