| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
device_cmd_packet_t Struct Reference
Collaboration diagram for device_cmd_packet_t:

## Data Fields
uint8 | appId
uint8 | cmd
uint16 | nWrite
uint8 | nRead

## Detailed Description

Definition at line 102 of file rli_project.c.

## Field Documentation

uint8 appId

Application ID

Definition at line 105 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint8 cmd

Host command

Definition at line 108 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint8 nRead

Number of bytes to read/write

Definition at line 114 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint16 nWrite

Register Offset

Definition at line 111 of file rli_project.c.

Referenced by rli_ci_app_callback().

The documentation for this struct was generated from the following file:

- ISF/RLI/Source/rli_project.c

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.