| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Variables
FXLC95000_1.h File Reference
`#include "I2C1.h"`
`#include "fxlc95000.h"`
`#include "fsl_fxlc95000_i2cspi_pedo.h"`
`#include "fsl_i2c_master_driver.h"`
`#include "Cpu.h"`
Include dependency graph for FXLC95000_1.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | FXLC95000_1_DATA_TYPE fxlc95000_DataBuffer_t
#define | FXLC95000_1_SAMPLE_OFFSET (16)
#define | FXLC95000_1_SAMPLE_SIZE (10)
#define | FXLC95000_1_CONFIG_REGISTER_CMD_OFFSET (0)
#define | FXLC95000_1_CONFIG_REGISTER_READ_OFFSET (4)
#define | FXLC95000_1_CONFIG_REGISTER_SIZE (sizeof(fxlc95000_appConfigRegister_t))
#define | FXLC95000_1_ACC_FLOAT_CONVERSION_FACTOR (0.000061035156)
#define | FXLC95000_1_ACC_ACCEL_RANGE_2G (0x40)
#define | FXLC95000_1_ACC_ACCEL_RANGE_4G (0x80)
#define | FXLC95000_1_ACC_ACCEL_RANGE_8G (0xC0)
#define | FXLC95000_1_ACC_MODE_ACCEL_ONLY (0x00)
#define | FXLC95000_1_ACC_ACCEL_RESOLUTION_16_BIT (0x00)

## Variables
fxlc95000_Sensor_Specific_Settings_t | FXLC95000_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | FXLC95000_1_Adapter
| This allows access to the sensor adapter instance for the target sensor. More...
const i2c_device_t | FXLC95000_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...

## Detailed Description

Version
  01.00

Definition in file FXLC95000_1.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.