| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
isf_Meters1D_float_t Struct Reference

Standard floating point type for single axis altitude sensor. More...

`#include <isf_altitude_types.h>`

Collaboration diagram for isf_Meters1D_float_t:

## Data Fields
isf_timestamp_t | timestamp
isf_altitude_meters_float_t | altitude

## Detailed Description

Standard floating point type for single axis altitude sensor.

Definition at line 36 of file isf_altitude_types.h.

## Field Documentation

isf_altitude_meters_float_t altitude

Definition at line 38 of file isf_altitude_types.h.

Referenced by fsl_fusion_virt_3D_orient_PeriodicCallback().

isf_timestamp_t timestamp

Definition at line 37 of file isf_altitude_types.h.

Referenced by fsl_fusion_virt_3D_orient_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorGeneric/isf_altitude_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.