| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

BasicApp1.h
Go to the documentation of this file.
1 /* ###################################################################
2 ** This component module is generated by Processor Expert. Do not modify it.
3 ** Filename : BasicApp1.h
4 ** CDE edition : Standard
5 ** Project : ISF2P2_K64F_MQX_PROJ
6 ** Processor : MK64FN1M0VLL12
7 ** Component : ISF_KSDK_BasicApp
8 ** Version : Component 02.500, Driver 02.00, CPU db: 3.00.000
9 ** Repository : My Components
10 ** Compiler : GNU C Compiler
11 ** Date/Time : 2016-10-06, 13:38, # CodeGen: 0
12 ** Abstract :
13 **
14 ** Settings :
15 ** Component Name : BasicApp1
16 ** Main Application Settings :
17 ** Processed Data Buffer Size : 34
18 ** Application Version Number : 0100
19 ** Additional User-Defined App Info :
20 ** Host Interface :
21 ** Host Command Interface Supported : yes
22 ** ISF_Core : ISFCore1
23 ** App Task Priority : 11
24 ** App Task Stack Size : 1200
25 ** Subscription List : 20
26 ** Sensor Subscription :
27 ** Sensor Type : Accelerometer
28 ** Selected Sensor : FXLC95000_1
29 ** Settings To Use : UseGiven
30 ** Sample Period : 10000
31 ** Sensor Data Format : Raw Sensor Format
32 ** Sensor Data Type : Native Sensor Output
33 ** FIFO Depth : 1
34 ** Sensor Subscription :
35 ** Sensor Type : Accelerometer
36 ** Selected Sensor : FXLC95000_2
37 ** Settings To Use : UseGiven
38 ** Sample Period : 10000
39 ** Sensor Data Format : Raw Sensor Format
40 ** Sensor Data Type : Native Sensor Output
41 ** FIFO Depth : 1
42 ** Sensor Subscription :
43 ** Sensor Type : Accelerometer
44 ** Selected Sensor : FXLS8471_1
45 ** Settings To Use : UseGiven
46 ** Sample Period : 10000
47 ** Sensor Data Format : Raw Sensor Format
48 ** Sensor Data Type : Native Sensor Output
49 ** FIFO Depth : 1
50 ** Sensor Subscription :
51 ** Sensor Type : Accelerometer
52 ** Selected Sensor : FXLS8471_2
53 ** Settings To Use : UseGiven
54 ** Sample Period : 10000
55 ** Sensor Data Format : Raw Sensor Format
56 ** Sensor Data Type : Native Sensor Output
57 ** FIFO Depth : 1
58 ** Sensor Subscription :
59 ** Sensor Type : Accelerometer
60 ** Selected Sensor : FXLS8952_1
61 ** Settings To Use : UseGiven
62 ** Sample Period : 10000
63 ** Sensor Data Format : Raw Sensor Format
64 ** Sensor Data Type : Native Sensor Output
65 ** FIFO Depth : 1
66 ** Sensor Subscription :
67 ** Sensor Type : Accelerometer
68 ** Selected Sensor : FXOS8700_1
69 ** Settings To Use : UseGiven
70 ** Sample Period : 10000
71 ** Sensor Data Format : Raw Sensor Format
72 ** Sensor Data Type : Native Sensor Output
73 ** FIFO Depth : 1
74 ** Sensor Subscription :
75 ** Sensor Type : Accelerometer
76 ** Selected Sensor : MMA8491Q_1
77 ** Settings To Use : UseGiven
78 ** Sample Period : 10000
79 ** Sensor Data Format : Raw Sensor Format
80 ** Sensor Data Type : Native Sensor Output
81 ** FIFO Depth : 1
82 ** Sensor Subscription :
83 ** Sensor Type : Accelerometer
84 ** Selected Sensor : MMA865x_1
85 ** Settings To Use : UseGiven
86 ** Sample Period : 10000
87 ** Sensor Data Format : Raw Sensor Format
88 ** Sensor Data Type : Native Sensor Output
89 ** FIFO Depth : 1
90 ** Sensor Subscription :
91 ** Sensor Type : Magnetometer
92 ** Selected Sensor : FXOS8700_2
93 ** Settings To Use : UseGiven
94 ** Sample Period : 10000
95 ** Sensor Data Format : Raw Sensor Format
96 ** Sensor Data Type : Native Sensor Output
97 ** FIFO Depth : 1
98 ** Sensor Subscription :
99 ** Sensor Type : Magnetometer
100 ** Selected Sensor : MAG3110_1
101 ** Settings To Use : UseGiven
102 ** Sample Period : 200000
103 ** Sensor Data Format : Raw Sensor Format
104 ** Sensor Data Type : Native Sensor Output
105 ** FIFO Depth : 1
106 ** Sensor Subscription :
107 ** Sensor Type : Gyrometer
108 ** Selected Sensor : FXAS21002_1
109 ** Settings To Use : UseGiven
110 ** Sample Period : 10000
111 ** Sensor Data Format : Raw Sensor Format
112 ** Sensor Data Type : Native Sensor Output
113 ** FIFO Depth : 1
114 ** Sensor Subscription :
115 ** Sensor Type : Gyrometer
116 ** Selected Sensor : FXAS21002_2
117 ** Settings To Use : UseGiven
118 ** Sample Period : 10000
119 ** Sensor Data Format : Raw Sensor Format
120 ** Sensor Data Type : Native Sensor Output
121 ** FIFO Depth : 1
122 ** Sensor Subscription :
123 ** Sensor Type : Pressure
124 ** Selected Sensor : MPL3115_1
125 ** Settings To Use : UseGiven
126 ** Sample Period : 10000
127 ** Sensor Data Format : Raw Sensor Format
128 ** Sensor Data Type : Native Sensor Output
129 ** FIFO Depth : 1
130 ** Sensor Subscription :
131 ** Sensor Type : Temperature
132 ** Selected Sensor : MPL3115_1
133 ** Settings To Use : UseGiven
134 ** Sample Period : 10000
135 ** Sensor Data Format : Raw Sensor Format
136 ** Sensor Data Type : Native Sensor Output
137 ** FIFO Depth : 1
138 ** Sensor Subscription :
139 ** Sensor Type : Orientation
140 ** Selected Sensor : ORIENT_1
141 ** Settings To Use : UseGiven
142 ** Sample Period : 10000
143 ** Sensor Data Format : Raw Sensor Format
144 ** Sensor Data Type : Native Sensor Output
145 ** FIFO Depth : 1
146 ** Sensor Subscription :
147 ** Sensor Type : Altitude
148 ** Selected Sensor : MPL3115_1
149 ** Settings To Use : UseGiven
150 ** Sample Period : 10000
151 ** Sensor Data Format : Raw Sensor Format
152 ** Sensor Data Type : Native Sensor Output
153 ** FIFO Depth : 1
154 ** Sensor Subscription :
155 ** Sensor Type : Pedometer
156 ** Selected Sensor : MMA955x_1
157 ** Settings To Use : UseGiven
158 ** Sample Period : 8192
159 ** Sensor Data Format : Raw Sensor Format
160 ** Sensor Data Type : Native Sensor Output
161 ** FIFO Depth : 1
162 ** Sensor Subscription :
163 ** Sensor Type : Pedometer
164 ** Selected Sensor : MMA955x_2
165 ** Settings To Use : UseGiven
166 ** Sample Period : 8192
167 ** Sensor Data Format : Raw Sensor Format
168 ** Sensor Data Type : Native Sensor Output
169 ** FIFO Depth : 1
170 ** Sensor Subscription :
171 ** Sensor Type : Custom
172 ** Selected Sensor : Custom_1
173 ** Settings To Use : UseGiven
174 ** Sample Period : 10000
175 ** Sensor Data Format : Raw Sensor Format
176 ** Sensor Data Type : Native Sensor Output
177 ** FIFO Depth : 1
178 ** Sensor Subscription :
179 ** Sensor Type : Analog
180 ** Selected Sensor : Analog_1
181 ** Settings To Use : UseGiven
182 ** Sample Period : 10000
183 ** Sensor Data Format : Raw Sensor Format
184 ** Sensor Data Type : Native Sensor Output
185 ** FIFO Depth : 1
186 ** Contents :
187 ** No public methods
188 **
189 ** (c) Copyright Freescale Semiconductor, Inc., 2015,
190 **
191 http://www.freescale.com
192 ** ###################################################################*/
193 /*!
194 ** @file BasicApp1.h
195 ** @version 02.00
196 ** @brief
197 **
198 */
199 /*!
200 ** @addtogroup BasicApp1_module BasicApp1 module documentation
201 ** @{
202 */
203
204 #ifndef __BasicApp1_H
205 #define __BasicApp1_H
206
207 /* MODULE BasicApp1. */
208
209 /* Include inherited components */
210 #include "ISFCore1.h"
211 #include "FXLC95000_1.h"
212 #include "FXLC95000_2.h"
213 #include "FXLS8471_1.h"
214 #include "FXLS8471_2.h"
215 #include "FXLS8952_1.h"
216 #include "FXOS8700_1.h"
217 #include "MMA8491Q_1.h"
218 #include "MMA865x_1.h"
219 #include "FXOS8700_2.h"
220 #include "MAG3110_1.h"
221 #include "FXAS21002_1.h"
222 #include "FXAS21002_2.h"
223 #include "MPL3115_1.h"
224 #include "MPL3115_1.h"
225 #include "ORIENT_1.h"
226 #include "MPL3115_1.h"
227 #include "MMA955x_1.h"
228 #include "MMA955x_2.h"
229 #include "Custom_1.h"
230 #include "Analog_1.h"
231 #include "BasicApp1_types.h"
232
233 #include "Cpu.h"
234
235 extern void *pSensorData[];
236 extern BasicApp1DataBuffers_t gBasicApp1DataBuffers;
237
238 void BasicApp1_init();
239 int8 BasicApp1_FlashSensor(uint8 numBytes, uint8 *pFlashData);
240 /* END BasicApp1. */
241
242 #endif
243 /* ifndef __BasicApp1_H */
244 /*!
245 ** @}
246 */
247 /*
248 ** ###################################################################
249 **
250 ** This file was created by Processor Expert 10.5 [05.21]
251 ** for the Freescale Kinetis series of microcontrollers.
252 **
253 ** ###################################################################
254 */
255
Cpu.h
ISFCore1.h
uint8
unsigned char uint8
Definition: isf_types.h:76
FXAS21002_1.h
ORIENT_1.h
MPL3115_1.h
pSensorData
void * pSensorData[]
Definition: BasicApp1.c:408
Custom_1.h
MMA8491Q_1.h
BasicApp1DataBuffers_t
Definition: BasicApp1_types.h:397
BasicApp1_FlashSensor
int8 BasicApp1_FlashSensor(uint8 numBytes, uint8 *pFlashData)
Definition: BasicApp1.c:711
gBasicApp1DataBuffers
BasicApp1DataBuffers_t gBasicApp1DataBuffers
Definition: BasicApp1.c:260
BasicApp1_types.h
FXLS8471_2.h
MAG3110_1.h
Analog_1.h
FXLS8471_1.h
MMA955x_2.h
BasicApp1_init
void BasicApp1_init(void)
Definition: BasicApp1.c:683
FXLS8952_1.h
FXOS8700_2.h
MMA865x_1.h
FXLC95000_2.h
MMA955x_1.h
FXLC95000_1.h
FXOS8700_1.h
FXAS21002_2.h
int8
signed char int8
Definition: isf_types.h:72
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.