| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Macros | Functions | Variables
fsl_Sensor_Analog_1_Functions.c File Reference

This is user's event module. Put your event handler code here. More...

`#include "Cpu.h"`
`#include "Events.h"`
`#include "rtos_main_task.h"`
`#include "os_tasks.h"`
`#include "App1_Functions.h"`
`#include "BasicApp1_Functions.h"`
`#include "fsl_Sensor_Custom_1_Functions.h"`
`#include "fsl_Sensor_Analog_1_Functions.h"`
Include dependency graph for fsl_Sensor_Analog_1_Functions.c:

Go to the source code of this file.

## Data Structures
struct | AnalogVoltagetoOutputConvTable_t

## Macros
#define | Analog_1_CONVERT_FLOAT_FACTOR (1.0F/32767.0F)
#define | Analog_1_CONVERT_FIXED_FACTOR (32767)
#define | NUM_MESSAGES 64
#define | MSG_SIZE 1

## Functions
void | Analog_1__Void_ ()
isf_dsa_status_t | Analog_1_float_converter (Analog_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Analog_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | Analog_1_fixed_converter (Analog_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Analog_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | fsl_Sensor_Analog_1_Convert (isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes)
isf_dsa_status_t | fsl_Sensor_Analog_1_Configure (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Analog_1_ValidateSettings (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Analog_1_Initialize (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_StartData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_EndData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_Shutdown (isf_SensorHandle_t *pSensorHandle)
void | Analog_1_fsl_Sensor_Generic_Analog_Convert (void *pSensorHandle, uint32_t convertToType, uint8_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_AnalogCallback (void *pSensorHandle)
void | Analog_1_fsl_Sensor_Generic_Analog_Shutdown (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_EndData (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_StartData (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_Configure (void *pSensorHandle, void *pSensorSettings, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_ValidateSettings (void *pSensorHandle, void *pSensorSettings, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_Initialize (void *pSensorHandle, int8_t *retValue)

## Variables
uint8_t | sensorType = 0
uint8_t | numGpios = 1
uint8_t | configuredADCh = 1
uint32_t | operating_mode
const Analog_1_device_t | Analog_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...
Analog_1_Sensor_Specific_Settings_t | Analog_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
isf_SensorTypes_t | Analog_1_SupportedSensorTypes []
| Supported sensor and data types for the Sensor. More...
isf_SensorDataTypes_t | Analog_1_SupportedDataTypes []

## Detailed Description

This is user's event module. Put your event handler code here.

Version
  01.00

Definition in file fsl_Sensor_Analog_1_Functions.c.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.