| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Enumerations | Variables
SensorReset module documentation

## Enumerations
enum | _SensorReset_pinNames { J1_1 = GPIO_MAKE_PIN(GPIOB_IDX, 18U) }
| Pin names. More...

## Variables
const gpio_output_pin_user_config_t | ResetSensor_OutConfig0 []
| Configuration structure 0 for output pins. More...
const gpio_output_pin_user_config_t | ResetSensor_OutConfig0 []
| Configuration structure 0 for output pins. More...

## Detailed Description

## Enumeration Type Documentation

enum _SensorReset_pinNames

Pin names.

Enumerator
J1_1 |

Definition at line 81 of file SensorReset.h.

## Variable Documentation

const gpio_output_pin_user_config_t ResetSensor_OutConfig0[]

Initial value:
= {
{
.pinName = J1_1,
.config.outputLogic = 0,
.config.slewRate = kPortSlowSlewRate,
.config.isOpenDrainEnabled = false,
.config.driveStrength = kPortLowDriveStrength,
},
{
.pinName = GPIO_PINS_OUT_OF_RANGE,
}
}
J1_1
Definition: SensorReset.h:82

Configuration structure 0 for output pins.

Definition at line 56 of file SensorReset.c.

const gpio_output_pin_user_config_t ResetSensor_OutConfig0[]

Configuration structure 0 for output pins.

Definition at line 56 of file ResetSensor.c.

Referenced by Components_Init(), fsl_95000_spi_slave_init(), fsl_955x_spi_slave_init(), fsl_gauss_spi_slave_init(), fsl_leon_spi_slave_init(), and fsl_veryon_spi_slave_init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.