| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxls8952_Sensor_Specific_Settings_t Struct Reference

`#include <fxls8952.h>`

Collaboration diagram for fxls8952_Sensor_Specific_Settings_t:

## Data Fields
uint8 | accelFullScaleRange
boolean | usesInterrupts
uint32 | signal
boolean | usesBuffer
uint32 | samplePeriod
uint32 | regCount
fxls8952_Sensor_Specific_Reg_t | regPairs []

## Detailed Description

Definition at line 352 of file fxls8952.h.

## Field Documentation

uint8 accelFullScaleRange

Definition at line 354 of file fxls8952.h.

uint32 regCount

Definition at line 359 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_Configure().

fxls8952_Sensor_Specific_Reg_t regPairs[]

Definition at line 360 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_Configure().

uint32 samplePeriod

Definition at line 358 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_PeriodicCallback(), and fsl_fxls8952_i2c_3D_accel_ValidateSettings().

uint32 signal

Definition at line 356 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_Configure().

boolean usesBuffer

Definition at line 357 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_PeriodicCallback().

boolean usesInterrupts

Definition at line 355 of file fxls8952.h.

Referenced by fsl_fxls8952_i2c_3D_accel_Configure(), fsl_fxls8952_i2c_3D_accel_Shutdown(), and fsl_fxls8952_i2c_3D_accel_StartData().

The documentation for this struct was generated from the following file:

- SensorSpecific/fxls8952.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.