| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
device_periodic_read_cfg_packet_t Struct Reference

rli overall application state buffer format. More...

Collaboration diagram for device_periodic_read_cfg_packet_t:

## Data Fields
isf_duration_t | period
uint8 | streamId

## Detailed Description

rli overall application state buffer format.

Definition at line 91 of file rli_project.c.

## Field Documentation

isf_duration_t period

read period (usecs)

Definition at line 94 of file rli_project.c.

Referenced by rli_ci_app_callback().

uint8 streamId

streamId to use

Definition at line 97 of file rli_project.c.

Referenced by rli_ci_app_callback().

The documentation for this struct was generated from the following file:

- ISF/RLI/Source/rli_project.c

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.