| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros
isf_user_config.h File Reference

The isf_user_config.h file contains the user configurable settings to either include or exclude an ISF component. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | ISF_COMPONENT_CI (1)
| When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component is linked to the user application. More...
#define | ISF_COMPONENT_BM (1)
| When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component code is compiled. Note: The component must be recompiled when this setting is changed. More...
#define | ISF_COMPONENT_PM (0)
| When defined as 1, the Power Management component code will compiled. The component must be recompiled when this setting is changed. More...

## Detailed Description

The isf_user_config.h file contains the user configurable settings to either include or exclude an ISF component.

Copyright
  Copyright (c) 2015, Freescale Semiconductor, Inc.

Definition in file isf_user_config.h.

## Macro Definition Documentation

#define ISF_COMPONENT_BM (1)

When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component code is compiled.
Note: The component must be recompiled when this setting is changed.

Definition at line 33 of file isf_user_config.h.

#define ISF_COMPONENT_CI (1)

When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component is linked to the user application.

When ISF_COMPONENT_CI is defined as 1, the Command Interpreter component is linked to the user application.

Definition at line 22 of file isf_user_config.h.

#define ISF_COMPONENT_PM (0)

When defined as 1, the Power Management component
code will compiled. The component must be recompiled when this setting is changed.

Definition at line 44 of file isf_user_config.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.