| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- w
- x
- y
- z

### - s -

- SCS_BASE_ADDR : isf_systick_defs.h
- SENSOR_DATA_READY_EVENT : rli_project.c , fsl_fusion_virt_3D_orient.c
- SENSOR_IDX_Accelerometer0 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer1 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer2 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer3 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer4 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer5 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer6 : BasicApp1_types.h
- SENSOR_IDX_Accelerometer7 : BasicApp1_types.h
- SENSOR_IDX_Altitude15 : BasicApp1_types.h
- SENSOR_IDX_Analog19 : BasicApp1_types.h
- SENSOR_IDX_Custom18 : BasicApp1_types.h
- SENSOR_IDX_Gyrometer10 : BasicApp1_types.h
- SENSOR_IDX_Gyrometer11 : BasicApp1_types.h
- SENSOR_IDX_Magnetometer8 : BasicApp1_types.h
- SENSOR_IDX_Magnetometer9 : BasicApp1_types.h
- SENSOR_IDX_Orientation14 : BasicApp1_types.h
- SENSOR_IDX_Pedometer16 : BasicApp1_types.h
- SENSOR_IDX_Pedometer17 : BasicApp1_types.h
- SENSOR_IDX_Pressure12 : BasicApp1_types.h
- SENSOR_IDX_Temperature13 : BasicApp1_types.h
- SENSORFS : fusion_config.h
- SET_FIELD : App1.c , rli_project.c , mma8491q.h
- SM_API_ALTERNATE_OFFERED : isf_sm_types.h
- SM_API_ERR_ALREADY_BEGUN : isf_sm_types.h
- SM_API_ERR_BUFFERLOCK_TIMEOUT : isf_sm_types.h
- SM_API_ERR_DATATYPE_NOT_SUPPORTED : isf_sm_types.h
- SM_API_ERR_FIFO_OVER_LIMIT : isf_sm_types.h
- SM_API_ERR_INVALID_HANDLE : isf_sm_types.h
- SM_API_ERR_INVALID_PTR : isf_sm_types.h
- SM_API_ERR_LOCK_CREATION_FAILED : isf_sm_types.h
- SM_API_ERR_MAX_TAPS_PER_SENSOR : isf_sm_types.h
- SM_API_ERR_NO_MEMORY : isf_sm_types.h
- SM_API_ERR_NOT_YET_BEGUN : isf_sm_types.h
- SM_API_ERR_SAMPLE_TAP_RATE : isf_sm_types.h
- SM_API_ERR_SENSOR_ALREADY_INITIALIZED : isf_sm_types.h
- SM_API_ERR_SENSOR_ID : isf_sm_types.h
- SM_API_ERR_SENSOR_INIT_FAILED : isf_sm_types.h
- SM_API_ERR_SENSOR_NOT_AVAIL : isf_sm_types.h
- SM_API_ERR_SETTINGS_TO_USE : isf_sm_types.h
- SM_API_ERR_SUBSCRIBER_COUNT : isf_sm_types.h
- SM_API_ERR_TOKEN_ID : isf_sm_types.h
- SM_MAX_FIFO_DEPTH : isf_sm_types.h
- SM_MAX_SUBSCRIBERS_PER_SENSOR : isf_sm_types.h
- SMALLMODULUS : orientation.c
- SMALLQ0 : orientation.c
- SP_MB0 : ci_protocol_mbox.h
- SP_MB1 : ci_protocol_mbox.h
- SP_MB2 : ci_protocol_mbox.h
- SP_MB3 : ci_protocol_mbox.h
- SP_MB4 : ci_protocol_mbox.h
- START_TIMER : fusion_exec.c
- startof : App1.c , fxlc95000.h
- STATUS_00_REG : mpl3115.h
- STOP_TIMER : fusion_exec.c
- STREAM_COCO_BIT : ci_protocol_stream.h
- STREAM_COCO_BIT_MASK : ci_protocol_stream.h
- STREAM_CRC_BYTESIZE : ci_protocol_stream.h
- STREAM_CRC_DISABLED : isf_ci_stream.h
- STREAM_CRC_ENABLED : isf_ci_stream.h
- STREAM_PROTOCOL_CMD_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_CMD_STATUS_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_DISABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_DATA_ENABLED : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_LENGTH_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_OUTPUTPACKET_INDEX_STREAMID : ci_protocol_stream.h
- STREAM_PROTOCOL_RECV_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_DEFAULT_ARRAY_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_CMD_ECHO : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_COCO_STAT : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_DATASTART : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_LSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_NUMDATA_MSB : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_INDEX_PROTOCOLID : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_MIN_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_RESP_RESPDATALENGTH_BYTESIZE : ci_protocol_stream.h
- STREAM_PROTOCOL_SUBCMD_BYTESIZE : ci_protocol_stream.h
- SYST_CALIB : isf_systick_defs.h
- SYST_CSR : isf_systick_defs.h
- SYST_CVR : isf_systick_defs.h
- SYST_RVR : isf_systick_defs.h
- SYSTEM_DEVICE_ID : version.h
- SysTick : isf_systick_defs.h
- SysTick_BASE_ADDR : isf_systick_defs.h
- SysTick_BASE_PTR : isf_systick_defs.h
- SysTick_CALIB_REG : isf_systick_defs.h
- SysTick_CSR_REG : isf_systick_defs.h
- SysTick_CVR_REG : isf_systick_defs.h
- SysTick_RVR_REG : isf_systick_defs.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.