| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - d -

- DATA_BUFFER_SIZE_8491Q : fsl_mma8491q_i2c_3D_accel.c
- DATA_FIFO_LEN_SUB0 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB1 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB10 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB11 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB12 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB13 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB14 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB15 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB16 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB17 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB18 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB19 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB2 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB3 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB4 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB5 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB6 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB7 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB8 : App1_types.h , BasicApp1_types.h
- DATA_FIFO_LEN_SUB9 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB0 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB1 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB10 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB11 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB12 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB13 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB14 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB15 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB16 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB17 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB18 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB19 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB2 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB3 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB4 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB5 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB6 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB7 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB8 : App1_types.h , BasicApp1_types.h
- DATA_TYPE_SUB9 : App1_types.h , BasicApp1_types.h
- DEFAULTB : magnetic.h , magnetic_config.h
- deinit_adc_pins() : pin_init.c
- deinit_can_pins() : pin_init.h
- deinit_cmp_pins() : pin_init.c
- deinit_cmt_pins() : pin_init.h
- deinit_dac_pins() : pin_init.h
- deinit_dma_pins() : pin_init.h
- deinit_enet_pins() : pin_init.c
- deinit_ewm_pins() : pin_init.h
- deinit_fb_pins() : pin_init.h
- deinit_ftm_pins() : pin_init.h
- deinit_gpio_pins() : pin_init.c
- deinit_i2c_pins() : pin_init.c
- deinit_i2s_pins() : pin_init.h
- deinit_jtag_pins() : pin_init.c
- deinit_llwu_pins() : pin_init.c
- deinit_lptmr_pins() : pin_init.h
- deinit_osc_pins() : pin_init.c
- deinit_pdb_pins() : pin_init.h
- deinit_rcm_pins() : pin_init.h
- deinit_rtc_pins() : pin_init.h
- deinit_scb_pins() : pin_init.h
- deinit_sdhc_pins() : pin_init.h
- deinit_sim_pins() : pin_init.h
- deinit_spi_pins() : pin_init.c
- deinit_supply_pins() : pin_init.h
- deinit_tpiu_pins() : pin_init.c
- deinit_uart_pins() : pin_init.c
- deinit_usb_pins() : pin_init.h
- deinit_usbdcd_pins() : pin_init.h
- deinit_vref_pins() : pin_init.h
- device_connect() : rli_project.c
- device_disconnect() : rli_project.c
- DeviceDescriptor_t : isf_sensors.h
- dlong : isf_types.h
- dm_channel_acquire_lock() : isf_device_messaging.c , isf_devmsg.h
- dm_channel_configure() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_desc : task_ci.c
- dm_channel_get_config() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_get_descriptor() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_get_state() : isf_device_messaging.c , isf_devmsg.h
- dm_channel_init() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_release_lock() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_start() : isf_devmsg.h , isf_device_messaging.c
- dm_channel_stop() : isf_device_messaging.c , isf_devmsg.h
- dm_ChannelConfig_ptr : isf_devmsg.h
- dm_ChannelDescriptor_t : isf_devmsg.h
- dm_ChannelId_t : isf_devmsg.h
- dm_dev_desc : task_ci.c
- dm_device_close() : isf_devmsg.h , isf_device_messaging.c
- dm_device_open() : isf_devmsg.h , isf_device_messaging.c
- dm_device_read() : isf_devmsg.h , isf_device_messaging.c
- dm_device_readx() : isf_device_messaging.c , isf_devmsg.h
- dm_device_write() : isf_devmsg.h , isf_device_messaging.c
- dm_device_writex() : isf_devmsg.h , isf_device_messaging.c
- dm_DeviceDescriptor_t : isf_devmsg.h
- DR_STATUS_00_REG : mpl3115.h
- DSA_Analog_1 : isf_sensor_configuration.h
- DSA_Custom_1 : isf_sensor_configuration.h
- DSA_ERR_BAD_RESULT_TYPE : isf_dsa_adapter.h
- DSA_ERR_BAD_SENSOR_DATA_TYPE : isf_dsa_adapter.h
- DSA_ERR_CALIBRATE : isf_dsa_adapter.h
- DSA_ERR_CONFIGURE : isf_dsa_adapter.h
- DSA_ERR_END_DATA : isf_dsa_adapter.h
- DSA_ERR_INITIALIZE : isf_dsa_adapter.h
- DSA_ERR_NO_MEM : isf_dsa_adapter.h
- DSA_ERR_PARAM : isf_dsa_adapter.h
- DSA_ERR_SHUTDOWN : isf_dsa_adapter.h
- DSA_ERR_START_DATA : isf_dsa_adapter.h
- DSA_ERR_VALIDATE_SETTINGS : isf_dsa_adapter.h
- DSA_FIFO_FULL : isf_dsa_adapter.h
- DSA_FXAS21002_1 : isf_sensor_configuration.h
- DSA_FXAS21002_2 : isf_sensor_configuration.h
- DSA_FXLC95000_1 : isf_sensor_configuration.h
- DSA_FXLC95000_2 : isf_sensor_configuration.h
- DSA_FXLS8471_1 : isf_sensor_configuration.h
- DSA_FXLS8471_2 : isf_sensor_configuration.h
- DSA_FXLS8952_1 : isf_sensor_configuration.h
- DSA_FXOS8700_1 : isf_sensor_configuration.h
- DSA_FXOS8700_2 : isf_sensor_configuration.h
- DSA_MAG3110_1 : isf_sensor_configuration.h
- DSA_MMA8491Q_1 : isf_sensor_configuration.h
- DSA_MMA865x_1 : isf_sensor_configuration.h
- DSA_MMA955x_1 : isf_sensor_configuration.h
- DSA_MMA955x_2 : isf_sensor_configuration.h
- DSA_MPL3115_1 : isf_sensor_configuration.h
- DSA_NUM_SUPPORTED_SENSORS : isf_sensor_configuration.h
- DSA_ORIENT_1 : isf_sensor_configuration.h
- DSA_RESULT_TYPE_ENG_FIXED : isf_dsa_adapter.h
- DSA_RESULT_TYPE_ENG_FLOAT : isf_dsa_adapter.h
- DSA_RESULT_TYPE_RAW_COUNTS : isf_dsa_adapter.h
- DSA_RET_SETTINGS_CHANGED : isf_dsa_adapter.h
- DSA_STATE_CONFIGURED_STARTED : isf_dsa_adapter.h
- DSA_STATE_CONFIGURED_STOPPED : isf_dsa_adapter.h
- DSA_STATE_INITIALIZED : isf_dsa_adapter.h
- DSA_STATE_NOT_INITIALIZED : isf_dsa_adapter.h
- dword : isf_types.h
- isf_dsa_Adapter_t : isf_dsa_adapter.h
- isf_dsa_AdapterStatus_enums : isf_dsa_adapter.h
- isf_dsa_AdapterStatus_t : isf_dsa_adapter.h
- isf_dsa_ControlData_t : isf_dsa_adapter.h
- isf_dsa_ControlInterface_t : isf_dsa_adapter.h
- isf_dsa_data_converter_t : isf_dsa_adapter.h
- isf_dsa_DeviceInfoBlock_t : isf_dsa_adapter.h
- isf_dsa_err_t : isf_dsa_adapter.h
- isf_dsa_error_enums : isf_dsa_adapter.h
- isf_dsa_get_data_converter() : isf_dsa_utils.h , isf_dsa_utils.c
- isf_dsa_get_info() : isf_dsa_utils.h , isf_dsa_utils.c
- isf_dsa_get_sensor_data_types() : isf_dsa_utils.c , isf_dsa_utils.h
- isf_dsa_get_sensor_types() : isf_dsa_utils.c , isf_dsa_utils.h
- isf_dsa_get_sizeof_native_data_type() : isf_dsa_utils.h , isf_dsa_utils.c
- isf_dsa_result_enums : isf_dsa_adapter.h
- isf_dsa_result_types_t : isf_dsa_adapter.h
- isf_dsa_SensorSettings_t : isf_dsa_adapter.h
- isf_dsa_status_t : isf_dsa_adapter.h
- isf_duration_t : isf.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.