| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - b -

- BasicApp1_APP_DATA : BasicApp1_types.h
- BasicApp1_ci_app_callback() : BasicApp1.c , ISFCore1.c
- BasicApp1_CI_Callback() : BasicApp1_Functions.c
- BasicApp1_FlashSensor() : BasicApp1.c
- BasicApp1_init() : BasicApp1.c
- BasicApp1_Initialization() : BasicApp1_Functions.c
- BasicApp1_MainTask() : BasicApp1.c
- BasicApp1_OnAnySensor_Data_Ready() : BasicApp1_Functions.c
- BasicApp1_TASK_NAME : BasicApp1.c
- BasicApp1_TASK_PRIORITY : BasicApp1.c
- BasicApp1_TASK_STACK_SIZE : BasicApp1.c
- bitrev() : isf_util.h , isf_util.c
- bm : bus_management.c , bm_internal.h
- bm_active_cb_query() : bm_internal.h , bus_management.c
- BM_ALL_TOKENS : isf_bm.h
- BM_ALLOC_MEM_ZERO : bm_internal.h
- bm_callback_t : isf_bm.h
- bm_callback_token_t : isf_bm.h
- bm_cb_occurred_query() : bm_internal.h , bus_management.c
- BM_CURRENT_PERIOD : bm_internal.h
- BM_ERROR : isf_bm.h
- bm_find_cb() : bus_management.c
- bm_find_smallest_active_period() : bus_management.c
- BM_FREE_MEM : bm_internal.h
- BM_FULL_PERIOD : bm_internal.h
- bm_generate_token() : bus_management.c
- bm_get_num_callback() : bus_management.c , isf_bm.h
- bm_init() : bus_management.c , isf_bm.h , isf_init.h
- BM_MIN_REMAINING_THRESHOLD_USEC : bm_internal.h
- BM_MINIMUM_CB_TIMELEFT_USEC : bm_internal.h
- BM_PIPELINE_STAGES : bm_internal.h
- BM_PIT_SCALER : BM_pit_instance.h
- BM_PIT_SOURCE_CLK : BM_pit_instance.h
- bm_powerdown() : bm_internal.h , bus_management.c
- bm_register_periodic_callback() : bus_management.c , isf_bm.h
- bm_reset_period() : bus_management.c
- BM_ROLLOVER_PERIOD : BM_pit_instance.h
- bm_sort_cb_list() : bus_management.c
- bm_start() : bus_management.c , isf_bm.h
- bm_statechange_query() : bm_internal.h , bus_management.c
- bm_statechange_reset() : bm_internal.h , bus_management.c
- BM_STATIC : bm_internal.h
- bm_stop() : bus_management.c , isf_bm.h
- BM_task() : bus_management.c
- BM_TASK_NAME : bus_management.c
- BM_TASK_PRIORITY : bus_management.c
- BM_TASK_STACK_SIZE : bus_management.c
- bm_timer_init() : ISFBusManager1.c , bus_management.c
- BM_TOKEN_STARTING_VAL : bus_management.c
- BM_TOKEN_VAL_ERROR : isf_bm.h
- BM_TOKEN_VAL_MAX : isf_bm.h
- bm_unregister_callback() : isf_bm.h , bus_management.c
- bm_update_cb_list() : bus_management.c
- BM_VOLATILE : bm_internal.h
- bmPITInstance : bus_management.c , ISFBusManager1.c
- bmRolloverPeriod : ISFBusManager1.c , bus_management.c
- BMTIMER1_InitConfig0 : BMTIMER1.h , BMTIMER1.c
- BMTIMER1_IRQHandler() : Events.c
- BOARD_DEBUG_UART_BASEADDR : board.h
- BOARD_DEBUG_UART_BAUD : board.h
- BOARD_DEBUG_UART_INSTANCE : board.h
- BOARD_FRDM_K20D50M : build.h
- BOARD_FRDM_K22F : build.h
- BOARD_FRDM_K64F : build.h
- BOARD_FRDM_KL16Z : build.h
- BOARD_FRDM_KL25Z : build.h
- BOARD_FRDM_KL26Z : build.h
- BOARD_FRDM_KL46Z : build.h
- BOARD_FRDM_KL46Z_STANDALONE : build.h
- BOARD_FXLC95000CL : build.h
- BOARD_USE_UART : board.h
- BOARD_WIN8_REV05 : build.h
- boolean : isf_types.h
- BootToFlash : FXLC95000_1.c , FXLC95000_2.c
- busHandle_t : isf_protocol_adapter.h
- byte : isf_types.h
- BYTES_FOR_FULL_READ : fsl_mpl3115_i2c_1D_press.c , fsl_Sensor_Custom_1_Functions.c , fsl_fxls8471_i2cspi_3D_accel.c , fsl_mma865x_i2c_3D_accel.c
- byteswap() : ci_protocol_stream.c

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.