| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
mma955x_DataBuffer_t Struct Reference
fsl_mma955x module documentation

This structure defines the Pedometer sample data buffer format. More...

`#include <fsl_mma955x_i2cspi_pedo.h>`

Collaboration diagram for mma955x_DataBuffer_t:

## Data Fields
uint32 | timeStamp
int16 | accel [3]
int16 | temp
mma955x_PedometerData_t | pedometerData

## Detailed Description

This structure defines the Pedometer sample data buffer format.

Definition at line 28 of file fsl_mma955x_i2cspi_pedo.h.

## Field Documentation

int16 accel[3]

The accelerometer data.

Definition at line 30 of file fsl_mma955x_i2cspi_pedo.h.

Referenced by fsl_mma955x_PeriodicCallback().

mma955x_PedometerData_t pedometerData

The pedometer native data.

Definition at line 32 of file fsl_mma955x_i2cspi_pedo.h.

Referenced by fsl_mma955x_PeriodicCallback().

int16 temp

The temperature data.

Definition at line 31 of file fsl_mma955x_i2cspi_pedo.h.

uint32 timeStamp

The time stamp for the data packet.

Definition at line 29 of file fsl_mma955x_i2cspi_pedo.h.

Referenced by fsl_mma955x_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_mma955x_i2cspi_pedo.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.