| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
i2c_Master_BusConfig_struct Struct Reference

`#include <isf_i2c_master_types.h>`

Collaboration diagram for i2c_Master_BusConfig_struct:

## Data Fields
isf_duration_t | timeout
uint16 | defaultSpeed

## Detailed Description

Definition at line 17 of file isf_i2c_master_types.h.

## Field Documentation

uint16 defaultSpeed

The speed at which to run the bus.

Definition at line 19 of file isf_i2c_master_types.h.

Referenced by i2c_master_adapter_configure().

isf_duration_t timeout

The bus timeout value to use.

Definition at line 18 of file isf_i2c_master_types.h.

Referenced by i2c_master_adapter_acquire_lock(), i2c_master_adapter_configure(), i2c_master_adapter_get_endpoint(), i2c_master_adapter_read(), i2c_master_adapter_start(), i2c_master_adapter_stop(), and i2c_master_adapter_write().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_i2c_master_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.