| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

### - e -

- emb_apps_present : device_info_t
- enable_crc : ci_stream_ctrl_reg1_t
- enable_stream_data : ci_stream_ctrl_reg1_t
- EndData : isf_dsa_ControlInterface_st
- endDataCommands : fxlc95000_Sensor_Specific_Settings_t , mma955x_Sensor_Specific_Settings_t
- engFixedIntegerWidth : fxlc95000_Sensor_Specific_Settings_t , mma955x_Sensor_Specific_Settings_t
- engFixedSignBit : fxlc95000_Sensor_Specific_Settings_t , mma955x_Sensor_Specific_Settings_t
- engFixedTotalWidth : fxlc95000_Sensor_Specific_Settings_t , mma955x_Sensor_Specific_Settings_t
- engFloatConversionFactor : fxlc95000_Sensor_Specific_Settings_t , mma955x_Sensor_Specific_Settings_t
- error : rliAppStatus_t
- extctrlen : fxas21002_Sensor_Specific_Settings_t
- extrapolationBehavior : fLfiTable_t

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.