| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxas21002_DataBuffer_t Struct Reference
fsl_fxas21002_i2cspi_3D_gyro module documentation

This structure defines the dummy DSA data buffer format. More...

`#include <fsl_fxas21002_i2cspi_3D_gyro.h>`

Collaboration diagram for fxas21002_DataBuffer_t:

## Data Fields
uint32 | timeStamp
int16 | gyro [3]
uint8 | temperature

## Detailed Description

This structure defines the dummy DSA data buffer format.

Definition at line 25 of file fsl_fxas21002_i2cspi_3D_gyro.h.

## Field Documentation

int16 gyro[3]

The gyronetometer data

Definition at line 27 of file fsl_fxas21002_i2cspi_3D_gyro.h.

Referenced by fsl_fxas21002_i2cspi_3D_gyro_Initialize(), and fsl_fxas21002_i2cspi_3D_gyro_PeriodicCallback().

uint8 temperature

The device temperature measured in celsius scale

Definition at line 28 of file fsl_fxas21002_i2cspi_3D_gyro.h.

Referenced by fsl_fxas21002_i2cspi_3D_gyro_PeriodicCallback().

uint32 timeStamp

The time stamp for the data packet.

Definition at line 26 of file fsl_fxas21002_i2cspi_3D_gyro.h.

Referenced by fsl_fxas21002_i2cspi_3D_gyro_Initialize(), and fsl_fxas21002_i2cspi_3D_gyro_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxas21002_i2cspi_3D_gyro.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.