| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

### - n -

- name : isf_dsa_info_t
- nByteWrite : fxlc95000_Command_t , mma955x_Command_t
- nCurrentReportRate : fxlc95000_SensorSetting_t
- nCurrentResolution : fxlc95000_SensorSetting_t
- nEventFieldIndex : isf_dsa_ControlData_st
- nFifoDepth : fxlc95000_SensorSetting_t , isf_SubscriptionSettings_t
- nLock : busHandle_struct
- nMode : fxlc95000_SensorSetting_t
- nNativeDataSetSize : isf_dsa_DeviceInfoBlock_st
- nRange : fxlc95000_SensorSetting_t
- nRdLock : busHandle_struct
- nRead : device_cmd_packet_t
- nSamplePeriod : isf_dsa_SensorSettings_st , isf_SubscriptionSettings_t
- nSettingsToUse : fxlc95000_SensorSetting_t , isf_SubscriptionSettings_t
- nToken : bm_cb_config_t
- numBytes : App1_app_info_t , BasicApp1_app_info_t , ci_mbox_app_info_t , rli_app_info_t
- numCommands : fxlc95000_CommandList_t , mma955x_CommandList_t
- numSensors : appSubscriptionResponse_t
- nWrite : device_cmd_packet_t

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.