| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Functions
crc.c File Reference
`#include "isf.h"`
`#include "crc.h"`
Include dependency graph for crc.c:

Go to the source code of this file.

## Functions
uint16 | ccitt_crc16_cal (uint32 anumBytes, uint8 *apBuf)
| This crc function contains the standard CCITT CRC 16-bit implementation. More...

## Function Documentation

uint16 ccitt_crc16_cal | ( | uint32 | anumBytes,
|  | uint8 * | apBuf
| ) |  |

This crc function contains the standard CCITT CRC 16-bit implementation.

This function is used to to generate the CCITT CRC 16-bit value. It uses the standard polynomial value 0x1021.

Parameters

  [in] | apBuf | Buffer of data to perform CRC calculation on.
  [in] | anumBytes | The number of bytes to perform CRC calculation. The range is 0 to (2^32 - 1) bytes.

Returns
  ccitt_crc16_cal() returns a value of type uint16 which is the CRC value.

Constraints:
  The following constraints must be observed when using this function. If these constraints are not met, this API returns a zero for the number of bytes read from the mailboxes.
  - anumBytes must be within the valid range of 1 to (2^32-1)

Reentrant: No

Link Libraries:
  isf_ci.lib

Definition at line 18 of file crc.c.

References POLY_CRC16_GENERATOR.

Referenced by ci_protocol_CB_mbox(), ci_protocol_CB_stream(), isf_ci_qr_update(), and isf_ci_stream_update_data().

Here is the caller graph for this function:
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.