| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Macros | Variables
ISF_I2C1 module documentation

## Macros
#define | FSL_ISF_I2C1 1
| Device instance number. More...

## Variables
i2c_master_state_t | ISF_I2C1_MasterState
| Driver state structure which holds driver runtime data. More...
const i2c_device_t | ISF_I2C1_MasterConfig0
| Master configuration declaration. More...
i2c_master_state_t | ISF_I2C1_MasterState
| Driver state structure which holds driver runtime data. More...
const i2c_device_t | ISF_I2C1_MasterConfig0
| Master configuration declaration. More...

## Detailed Description

## Macro Definition Documentation

#define FSL_ISF_I2C1 1

Device instance number.

Definition at line 91 of file ISF_I2C1.h.

Referenced by Components_Init(), and ISF_I2C1_IRQHandler().

## Variable Documentation

const i2c_device_t ISF_I2C1_MasterConfig0

Initial value:
= {
.address = 0U,
.baudRate_kbps = 0U,
}

Master configuration declaration.

Definition at line 60 of file ISF_I2C1.c.

Referenced by Components_Init().

const i2c_device_t ISF_I2C1_MasterConfig0

Master configuration declaration.

Definition at line 60 of file ISF_I2C1.c.

Referenced by Components_Init().

i2c_master_state_t ISF_I2C1_MasterState

Driver state structure which holds driver runtime data.

Definition at line 57 of file ISF_I2C1.c.

Referenced by Components_Init().

i2c_master_state_t ISF_I2C1_MasterState

Driver state structure which holds driver runtime data.

Definition at line 57 of file ISF_I2C1.c.

Referenced by Components_Init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.