| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Enumerations | Functions
isf_sysconf_comms.h File Reference

This file defines the system configuration for the communication channel. More...

`#include "isf.h"`
Include dependency graph for isf_sysconf_comms.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | { COMM_CHANNEL_INTERNAL = 255, COMM_CHANNEL_I2C1 = 0, COMM_CHANNEL_SPI1 = 1, COMM_CHANNEL_UART2 = 2, SYS_NUM_CHANNEL_IDS }
| Declaration of the actual channels available for a particular device. These enums are indexes into the gSys_ConfiguredChannelList array and facilitate accessing channel configuration data. More...

## Functions
uint32 | get_ci_comm (void)

## Detailed Description

This file defines the system configuration for the communication channel.

File: isf_sysconf_comms.h

Copyright (c) 2015, Freescale Semiconductor, Inc.

Definition in file isf_sysconf_comms.h.

## Enumeration Type Documentation

anonymous enum

Declaration of the actual channels available for a particular device. These enums are indexes into the gSys_ConfiguredChannelList array and facilitate accessing channel configuration data.

Enumerator
COMM_CHANNEL_INTERNAL | The channel ID for the on-board accelerometer channel.
COMM_CHANNEL_I2C1 |
COMM_CHANNEL_SPI1 |
COMM_CHANNEL_UART2 |
SYS_NUM_CHANNEL_IDS | The number of channels in the system.

Definition at line 28 of file isf_sysconf_comms.h.

## Function Documentation

uint32 get_ci_comm | ( | void |  | ) |

Definition at line 93 of file isf_sysconf_comms.c.

References COMM_CHANNEL_UART2.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.