| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
device_info_t Struct Reference

This structure holds the ROM device information such as device id and number of EmbApps present. This information is returned by the _fw_device_info_get() API. More...

`#include <isf.h>`

Collaboration diagram for device_info_t:

## Data Fields
uint32 | system_device_id
uint8 | emb_apps_present
isf_info_t | isf_info

## Detailed Description

This structure holds the ROM device information such as device id and number of EmbApps present. This information is returned by the _fw_device_info_get() API.

Definition at line 187 of file isf.h.

## Field Documentation

uint8 emb_apps_present

The ISF library version and build information

Definition at line 191 of file isf.h.

Referenced by _fw_device_info_get().

isf_info_t isf_info

Definition at line 193 of file isf.h.

Referenced by _fw_device_info_get().

uint32 system_device_id

< System Device Identification information of the device (SIM_SDID Register) Number of Embedded Applications present in the image

Definition at line 189 of file isf.h.

Referenced by _fw_device_info_get().

The documentation for this struct was generated from the following file:

- ISF/Core/Include/isf.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.