| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxls8952_ODR_Table_tag Struct Reference
fsl_fxls8952_i2c_3D_accel module documentation

the structure defines the ODR table between Hybrid and normal mode of device operation. More...

`#include <fsl_fxls8952_i2c_3D_accel.h>`

Collaboration diagram for fxls8952_ODR_Table_tag:

## Data Fields
uint32 | periodNormalMode
uint8 | configVal

## Detailed Description

the structure defines the ODR table between Hybrid and normal mode of device operation.

Definition at line 81 of file fsl_fxls8952_i2c_3D_accel.h.

## Field Documentation

uint8 configVal

configuration value correspond to given ODR in millisecond.

Definition at line 83 of file fsl_fxls8952_i2c_3D_accel.h.

uint32 periodNormalMode

Normal Mode ODR value in millisecond.

Definition at line 82 of file fsl_fxls8952_i2c_3D_accel.h.

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxls8952_i2c_3D_accel.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.