| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxos8700_DataBuffer_t Struct Reference
fsl_fxos8700_i2cspi_6D_AccMag module documentation

This structure defines the dummy DSA data buffer format. More...

`#include <fsl_fxos8700_i2cspi_6D_AccMag.h>`

Collaboration diagram for fxos8700_DataBuffer_t:

## Data Fields
uint32 | timeStamp
int16 | accel [3]
int16 | mag [3]
uint8 | addr

## Detailed Description

This structure defines the dummy DSA data buffer format.

Definition at line 104 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

## Field Documentation

int16 accel[3]

The accelerometer data

Definition at line 106 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Initialize(), and fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback().

uint8 addr

The device "address" can uniquely identify the sensor

Definition at line 108 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

int16 mag[3]

The magnetometer data

Definition at line 107 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Initialize(), and fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback().

uint32 timeStamp

The time stamp for the data packet.

Definition at line 105 of file fsl_fxos8700_i2cspi_6D_AccMag.h.

Referenced by fsl_fxos8700_i2cspi_6D_AccMag_Initialize(), and fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback().

The documentation for this struct was generated from the following file:

- SensorSpecific/fsl_fxos8700_i2cspi_6D_AccMag.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.