| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Macros | Variables
BMTIMER1 module documentation

## Macros
#define | FSL_BMTIMER1 0
| Device instance number. More...
#define | FSL_BMTIMER1_CHANNEL 0
| PIT timer channel. More...

## Variables
const pit_user_config_t | BMTIMER1_InitConfig0
| PIT configuration declaration. More...
const pit_user_config_t | BMTIMER1_InitConfig0
| PIT configuration declaration. More...

## Detailed Description

## Macro Definition Documentation

#define FSL_BMTIMER1 0

Device instance number.

Definition at line 77 of file BMTIMER1.h.

Referenced by BMTIMER1_IRQHandler(), and Components_Init().

#define FSL_BMTIMER1_CHANNEL 0

PIT timer channel.

Definition at line 79 of file BMTIMER1.h.

Referenced by BMTIMER1_IRQHandler(), and Components_Init().

## Variable Documentation

const pit_user_config_t BMTIMER1_InitConfig0

Initial value:
= {
.isInterruptEnabled = true,
.periodUs = 1000000U,
}

PIT configuration declaration.

Definition at line 57 of file BMTIMER1.c.

Referenced by Components_Init().

const pit_user_config_t BMTIMER1_InitConfig0

PIT configuration declaration.

Definition at line 57 of file BMTIMER1.c.

Referenced by Components_Init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.