| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Functions | Variables
fsl_Sensor_Custom_1_Functions.c File Reference

This is user's event module. Put your event handler code here. More...

`#include "Cpu.h"`
`#include "Events.h"`
`#include "rtos_main_task.h"`
`#include "os_tasks.h"`
`#include "App1_Functions.h"`
`#include "BasicApp1_Functions.h"`
`#include "fsl_Sensor_Custom_1_Functions.h"`
`#include "fsl_Sensor_Analog_1_Functions.h"`
Include dependency graph for fsl_Sensor_Custom_1_Functions.c:

Go to the source code of this file.

## Macros
#define | Custom_1_CONVERT_FLOAT_FACTOR 0.000061
#define | Custom_1_CONVERT_FIXED_FACTOR 4
#define | BYTES_FOR_FULL_READ 7

## Functions
void | Custom_1__Void_ ()
isf_dsa_status_t | Custom_1_float_Custom_converter (Custom_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Custom_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | Custom_1_fixed_Custom_converter (Custom_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Custom_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | fsl_Sensor_Custom_1_Convert (volatile isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes)
isf_dsa_status_t | fsl_Sensor_Custom_1_Configure (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Custom_1_ValidateSettings (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Custom_1_Initialize (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Custom_1_StartData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Custom_1_EndData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Custom_1_Shutdown (isf_SensorHandle_t *pSensorHandle)
void | Custom_1_fsl_Sensor_Custom_Convert (volatile void *pSensorHandle, uint32_t convertToType, uint8_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_PeriodicCallback (void *pSensorHandle)
void | Custom_1_fsl_Sensor_Custom_Shutdown (void *pSensorHandle, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_EndData (void *pSensorHandle, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_StartData (void *pSensorHandle, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_Configure (void *pSensorHandle, void *pSensorSettings, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_ValidateSettings (void *pSensorHandle, void *pSensorSettings, uint8_t *retVal)
void | Custom_1_fsl_Sensor_Custom_Initialize (void *pSensorHandle, uint8_t *retVal)

## Variables
const uint8_t | Custom_1_Who_Am_I_Values [] = {0x4A, 0x5A}
| Define the WHO_AM_I register values for both possible sensor variations. More...
Custom_1_Sensor_Specific_Settings_t | Custom_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const i2c_device_t | Custom_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...
isf_SensorTypes_t | Custom_1_SupportedSensorTypes []
| Supported sensor and data types for the Sensor. More...
isf_SensorDataTypes_t | Custom_1_SupportedDataTypes []

## Detailed Description

This is user's event module. Put your event handler code here.

Version
  01.00

Definition in file fsl_Sensor_Custom_1_Functions.c.

## Macro Definition Documentation

#define BYTES_FOR_FULL_READ 7

Referenced by Custom_1_fsl_Sensor_Custom_PeriodicCallback().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.