| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
uart_BusConfig_struct Struct Reference

`#include <isf_uart_types.h>`

Collaboration diagram for uart_BusConfig_struct:

## Data Fields
isf_duration_t | timeout
uart_user_config_t | config

## Detailed Description

Definition at line 22 of file isf_uart_types.h.

## Field Documentation

uart_user_config_t config

Uart configuration information.

Definition at line 24 of file isf_uart_types.h.

Referenced by uart_adapter_configure().

isf_duration_t timeout

The bus timeout value to use.

Definition at line 23 of file isf_uart_types.h.

Referenced by uart_adapter_acquire_lock(), uart_adapter_configure(), uart_adapter_get_endpoint(), uart_adapter_read(), uart_adapter_start(), uart_adapter_stop(), and uart_adapter_write().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_uart_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.