| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - f -

- F180OVERPI : fusion_types.h
- F180OVERPISQ : fusion_types.h
- f3DOFMagnetometerMatrixAndroid() : orientation.h , orientation.c
- f3DOFMagnetometerMatrixNED() : orientation.c , orientation.h
- f3DOFMagnetometerMatrixWin8() : orientation.h , orientation.c
- f3DOFTiltAndroid() : orientation.c , orientation.h
- f3DOFTiltNED() : orientation.c , orientation.h
- f3DOFTiltWin8() : orientation.c , orientation.h
- f3x3matrixAeqAxScalar() : matrix.h , matrix.c
- f3x3matrixAeqB() : matrix.c , matrix.h
- f3x3matrixAeqI() : matrix.c , matrix.h
- f3x3matrixAeqInvSymB() : matrix.c , matrix.h
- f3x3matrixAeqMinusA() : matrix.c , matrix.h
- f3x3matrixAeqScalar() : matrix.c , matrix.h
- f3x3matrixDetA() : matrix.c , matrix.h
- facos_deg() : approximations.c , approximations.h
- false : basic_types.h
- FALSE : isf_types.h
- fAndroidAnglesDegFromRotationMatrix() : orientation.c , orientation.h
- fasin_deg() : approximations.c , approximations.h
- fatan2_deg() : approximations.c , approximations.h
- fatan_15deg() : approximations.c , approximations.h
- fatan_deg() : approximations.c , approximations.h
- FDEGTORAD : math_constants.h
- feCompassAndroid() : orientation.c , orientation.h
- feCompassNED() : orientation.c , orientation.h
- feCompassWin8() : orientation.c , orientation.h
- ff1() : isf_util.h , isf_util.c
- ff1_lsb() : isf_util.h , isf_util.c
- FGYRO_OFFSET_MAX_9DOF_GBY_KALMAN : fusion.h
- FGYRO_OFFSET_MIN_9DOF_GBY_KALMAN : fusion.h
- FIFO_FULL_BIT : isf_fifo.c
- FIFO_FULL_CLR_MASK : isf_fifo.c
- fInit_1DOF_P_BASIC() : fusion.c , fusion.h
- fInit_3DOF_B_BASIC() : fusion.c , fusion.h
- fInit_3DOF_G_BASIC() : fusion.c , fusion.h
- fInit_3DOF_Y_BASIC() : fusion.c , fusion.h
- fInit_6DOF_GB_BASIC() : fusion.c , fusion.h
- fInit_6DOF_GY_KALMAN() : fusion.c , fusion.h
- fInit_9DOF_GBY_KALMAN() : fusion.c , fusion.h
- fInitFusion() : fusion.h
- fInitMagCalibration() : magnetic.c , magnetic.h
- fInvertMagCal() : magnetic.c , magnetic.h
- FIRST_DATA_MAILBOX_NUM : ci_protocol_mbox.h
- FIRST_QR_MAILBOX_NUM : ci_protocol_mbox.h
- FITERRORAGINGSECS : magnetic_config.h
- fixedFactor : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_mma865x_i2c_3D_accel.c
- fixedOffset : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_mma865x_i2c_3D_accel.c
- FlashPostprocessSequence : FXLC95000_1.c , FXLC95000_2.c
- FlashPreprocessSequence : FXLC95000_1.c , FXLC95000_2.c
- fLeastSquareseCompassAndroid() : orientation.c , orientation.h
- fLeastSquareseCompassNED() : orientation.c , orientation.h
- fLeastSquareseCompassWin8() : orientation.c , orientation.h
- fLfi() : fsl_mpl3115_i2c_1D_press.c
- float32_To_AcFixed() : Ac_Fixed_utils.h , Ac_Fixed_utils.c , Ac_Fixed_utils.h
- floatFactor : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_mma865x_i2c_3D_accel.c
- floatOffset : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_mma865x_i2c_3D_accel.c
- fLPFOrientationQuaternion() : orientation.c , orientation.h
- fmatrixAeqI() : matrix.c , matrix.h
- fmatrixAeqInvA() : matrix.c , matrix.h
- fmatrixAeqRenormRotA() : matrix.c
- fnAcquireLock_t : isf_protocol_adapter.h
- fnConfigure_t : isf_protocol_adapter.h
- fnConnectToEndpoint_t : isf_protocol_adapter.h
- fnDisconnectEndpoint_t : isf_protocol_adapter.h
- fNEDAnglesDegFromRotationMatrix() : orientation.c , orientation.h
- fnGetConfig_t : isf_protocol_adapter.h
- fnGetState_t : isf_protocol_adapter.h
- fnInit_t : isf_protocol_adapter.h
- fnRead_t : isf_protocol_adapter.h
- fnreadpostProcossing_t : isf_spi_master_types.h
- fnreadpreProcessing_t : isf_spi_master_types.h
- fnReleaseLock_t : isf_protocol_adapter.h
- fnslaveinit_t : isf_spi_master_types.h
- fnStart_t : isf_protocol_adapter.h
- fnStop_t : isf_protocol_adapter.h
- fnWrite_t : isf_protocol_adapter.h
- fnwritepostProcossing_t : isf_spi_master_types.h
- fnwritepreProcessing_t : isf_spi_master_types.h
- FPIOVER180 : fusion_types.h
- fqAeq1() : orientation.c , orientation.h
- fqAeqNormqA() : orientation.c , orientation.h
- fQuaternionFromRotationMatrix() : orientation.c , orientation.h
- fQuaternionFromRotationVectorDeg() : orientation.c , orientation.h
- FQVBQD_MIN_9DOF_GBY_KALMAN : fusion.h
- FQVY_6DOF_GY_KALMAN : fusion.h
- FQVY_9DOF_GBY_KALMAN : fusion.h
- FQWB_6DOF_GY_KALMAN : fusion.h
- FQWB_9DOF_GBY_KALMAN : fusion.h
- FQWDLT_9DOF_GBY_KALMAN : fusion.h
- FRADTODEG : math_constants.h
- fRotationMatrixFromQuaternion() : orientation.c , orientation.h
- fRotationVectorDegFromQuaternion() : orientation.c , orientation.h
- fRun_1DOF_P_BASIC() : fusion.c , fusion.h
- fRun_3DOF_B_BASIC() : fusion.c , fusion.h
- fRun_3DOF_G_BASIC() : fusion.c , fusion.h
- fRun_3DOF_Y_BASIC() : fusion.c , fusion.h
- fRun_6DOF_GB_BASIC() : fusion.c , fusion.h
- fRun_6DOF_GY_KALMAN() : fusion.c , fusion.h
- fRun_9DOF_GBY_KALMAN() : fusion.c , fusion.h
- fRunMagCalibration() : magnetic.c , magnetic.h
- fsl_95000_spi_slave_init() : FXLC95000_2.c
- fsl_95000_spi_slave_read_postprocess() : FXLC95000_2.c
- fsl_95000_spi_slave_read_preprocess() : FXLC95000_2.c
- fsl_95000_spi_slave_write_postprocess() : FXLC95000_2.c
- fsl_95000_spi_slave_write_preprocess() : FXLC95000_2.c
- fsl_955x_spi_slave_init() : MMA955x_2.c
- fsl_955x_spi_slave_read_postprocess() : MMA955x_2.c
- fsl_955x_spi_slave_read_preprocess() : MMA955x_2.c
- fsl_955x_spi_slave_write_postprocess() : MMA955x_2.c
- fsl_955x_spi_slave_write_preprocess() : MMA955x_2.c
- FSL_ADC1 : ADC1.h
- FSL_BMTIMER1 : BMTIMER1.h
- FSL_BMTIMER1_CHANNEL : BMTIMER1.h
- FSL_CLOCK_MANAGER_CALLBACK_CNT : clockMan1.h
- FSL_CLOCK_MANAGER_CONFIG_CNT : clockMan1.h
- FSL_FSL_HWTIMER1_LL_DEVIF : fsl_hwtimer1.h
- FSL_FSL_HWTIMER1_LL_ID : fsl_hwtimer1.h
- FSL_FSL_HWTIMER1_PERIOD_CNF0 : fsl_hwtimer1.h
- FSL_FSL_MPU1 : fsl_mpu1.h
- fsl_fusion_SupportedDataTypes : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_SupportedSensorTypes : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_task() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_Calibrate() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_Configure() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_Convert() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_EndData() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_Initialize() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_PeriodicCallback() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_Shutdown() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_StartData() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fusion_virt_3D_orient_ValidateSettings() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_fxas21002_i2cspi_3D_gyro_Calibrate() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_Configure() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_Convert() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_EndData() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_Initialize() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_PeriodicCallback() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_Shutdown() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_StartData() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxas21002_i2cspi_3D_gyro_ValidateSettings() : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fsl_fxlc95000_Calibrate() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_Configure() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_Convert() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_EndData() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_Flash() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_Initialize() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_PeriodicCallback() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_Shutdown() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_StartData() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fsl_fxlc95000_ValidateSettings() : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- FSL_FXLS8471_ACCEL_100HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_12p5HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_1p56HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_200HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_400HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_50HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_6p25HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_800HZ : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_SCALE_2G : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_SCALE_4G : fsl_fxls8471_i2cspi_3D_accel.h
- FSL_FXLS8471_ACCEL_SCALE_8G : fsl_fxls8471_i2cspi_3D_accel.h
- fsl_fxls8471_i2cspi_3D_accel_Calibrate() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_Configure() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_Convert() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_EndData() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_Initialize() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_PeriodicCallback() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_Shutdown() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_StartData() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8471_i2cspi_3D_accel_ValidateSettings() : fsl_fxls8471_i2cspi_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_Calibrate() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_Configure() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_Convert() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_EndData() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_Initialize() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_PeriodicCallback() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_Shutdown() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_StartData() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxls8952_i2c_3D_accel_ValidateSettings() : fsl_fxls8952_i2c_3D_accel.c
- fsl_fxos8700_i2cspi_6D_AccMag_Calibrate() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_Configure() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_Convert() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_EndData() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_Initialize() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_PeriodicCallback() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_Shutdown() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_StartData() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings() : fsl_fxos8700_i2cspi_6D_AccMag.c , fsl_fxos8700_i2cspi_6D_AccMag.h
- fsl_gauss_spi_slave_init() : FXOS8700_2.c
- fsl_gauss_spi_slave_read_postprocess() : FXOS8700_2.c
- fsl_gauss_spi_slave_read_preprocess() : FXOS8700_2.c
- fsl_gauss_spi_slave_write_postprocess() : FXOS8700_2.c
- fsl_gauss_spi_slave_write_preprocess() : FXOS8700_2.c
- FSL_ISF_I2C1 : ISF_I2C1.h
- FSL_ISF_SPI1 : ISF_SPI1.h
- FSL_ISF_UART1 : ISF_UART1.h
- fsl_leon_spi_slave_init() : FXAS21002_2.c
- fsl_leon_spi_slave_read_postprocess() : FXAS21002_2.c
- fsl_leon_spi_slave_read_preprocess() : FXAS21002_2.c
- fsl_leon_spi_slave_write_postprocess() : FXAS21002_2.c
- fsl_leon_spi_slave_write_preprocess() : FXAS21002_2.c
- fsl_mag3110_i2c_3D_mag_Calibrate() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_Configure() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_Convert() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_EndData() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_Initialize() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_PeriodicCallback() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_Shutdown() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_StartData() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_mag3110_i2c_3D_mag_ValidateSettings() : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- fsl_MagCal_task() : fsl_fusion_virt_3D_orient.c , fsl_fusion_virt_3D_orient.h
- fsl_mma8491q_i2c_3D_accel_Calibrate() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_Configure() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_Convert() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_EndData() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_Initialize() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_PeriodicCallback() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_Shutdown() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_StartData() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_i2c_3D_accel_ValidateSettings() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- fsl_mma8491q_read_data_OneShotCallback() : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_100HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_12p5HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_1p56HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_200HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_400HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_50HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_6p25HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_800HZ : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_DATA_8BIT : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_DATA_FULL : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_SCALE_2G : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_SCALE_4G : fsl_mma865x_i2c_3D_accel.h
- FSL_MMA865x_ACCEL_SCALE_8G : fsl_mma865x_i2c_3D_accel.h
- fsl_mma865x_i2c_3D_accel_Calibrate() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_Configure() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_Convert() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_EndData() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_Initialize() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_PeriodicCallback() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_Shutdown() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_StartData() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma865x_i2c_3D_accel_ValidateSettings() : fsl_mma865x_i2c_3D_accel.c
- fsl_mma955x_Calibrate() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_Configure() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_Convert() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_EndData() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_Initialize() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_PeriodicCallback() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_Shutdown() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_StartData() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- fsl_mma955x_ValidateSettings() : fsl_mma955x_i2cspi_pedo.c , fsl_mma955x_i2cspi_pedo.h
- FSL_MPL3115_ACCEL_100HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_12p5HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_1p56HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_200HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_400HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_50HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_6p25HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_800HZ : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_SCALE_2G : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_SCALE_4G : fsl_mpl3115_i2c_1D_press.h
- FSL_MPL3115_ACCEL_SCALE_8G : fsl_mpl3115_i2c_1D_press.h
- fsl_mpl3115_i2c_1D_press_Calibrate() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_Configure() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_Convert() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_EndData() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_Initialize() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_PeriodicCallback() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_Shutdown() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_StartData() : fsl_mpl3115_i2c_1D_press.c
- fsl_mpl3115_i2c_1D_press_ValidateSettings() : fsl_mpl3115_i2c_1D_press.c
- FSL_OSC0_INSTANCE : clockMan1.h
- fsl_Sensor_Analog_1_Configure() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_Convert() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_EndData() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_Initialize() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_Shutdown() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_StartData() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Analog_1_ValidateSettings() : fsl_Sensor_Analog_1_Functions.c
- fsl_Sensor_Custom_1_Configure() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_Convert() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_EndData() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_Initialize() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_Shutdown() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_StartData() : fsl_Sensor_Custom_1_Functions.c
- fsl_Sensor_Custom_1_ValidateSettings() : fsl_Sensor_Custom_1_Functions.c
- FSL_SENSOR_SPI_CMD_LENG : FXAS21002_2.c , FXLC95000_2.c , FXLS8471_1.c , FXOS8700_2.c , MMA955x_2.c
- fsl_spi_sensor_type_FXAS21002_2 : FXAS21002_2.c
- fsl_spi_sensor_type_FXLC95000_2 : FXLC95000_2.c
- fsl_spi_sensor_type_FXLS8471_1 : FXLS8471_1.c
- fsl_spi_sensor_type_FXOS8700_2 : FXOS8700_2.c
- fsl_spi_sensor_type_MMA955x_2 : MMA955x_2.c
- FSL_UART1 : uart1.h
- fsl_veryon_spi_slave_init() : FXLS8471_1.c
- fsl_veryon_spi_slave_read_postprocess() : FXLS8471_1.c
- fsl_veryon_spi_slave_read_preprocess() : FXLS8471_1.c
- fsl_veryon_spi_slave_write_postprocess() : FXLS8471_1.c
- fsl_veryon_spi_slave_write_preprocess() : FXLS8471_1.c
- FSRange_2g : MMA955x_1.c , MMA955x_2.c
- FSRange_4g : MMA955x_1.c , MMA955x_2.c
- FSRange_8g : MMA955x_1.c , MMA955x_2.c
- fUpdateCalibration10EIG() : magnetic.c , magnetic.h
- fUpdateCalibration4INV() : magnetic.c , magnetic.h
- fUpdateCalibration7EIG() : magnetic.c , magnetic.h
- Fusion_Init() : fusion_exec.c , fusion_exec.h
- Fusion_Run() : fusion_exec.c , fusion_exec.h
- FUTPERCOUNT : magnetic_config.h
- fveqconjgquq() : orientation.c , orientation.h
- fWin8AnglesDegFromRotationMatrix() : orientation.c , orientation.h
- FX0S8700_ERRO_READ : fsl_fxos8700_i2cspi_6D_AccMag.h
- FX0S8700_ERRO_WRITE : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxas21000_ODR_Table_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21000_odrTable : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21000_WHO_AM_I_VALUE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21000_WHOAMI_VALUE : fxas21002.h
- fxas21000GyroConvTable : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_1_Adapter : FXAS21002_1.c , FXAS21002_1.h
- FXAS21002_1_DATA_TYPE : FXAS21002_1.h
- FXAS21002_1_DeviceInfo : FXAS21002_1.c , FXAS21002_1.h
- FXAS21002_1_Sensor_Specific_Config : FXAS21002_1.c , FXAS21002_1.h
- FXAS21002_2_Adapter : FXAS21002_2.c , FXAS21002_2.h
- FXAS21002_2_DATA_TYPE : FXAS21002_2.h
- FXAS21002_2_DeviceInfo : FXAS21002_2.c , FXAS21002_2.h
- FXAS21002_2_Sensor_Specific_Config : FXAS21002_2.c , FXAS21002_2.h
- FXAS21002_ACTIVE_MASK : fxas21002.h
- FXAS21002_ACTIVE_SHIFT : fxas21002.h
- FXAS21002_BOOTEND_MASK : fxas21002.h
- FXAS21002_BOOTEND_SHIFT : fxas21002.h
- FXAS21002_BW_MASK : fxas21002.h
- FXAS21002_BW_SHIFT : fxas21002.h
- fxas21002_ConfigTable_t : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_CTRL_REG0 : fxas21002.h
- FXAS21002_CTRL_REG1 : fxas21002.h
- FXAS21002_CTRL_REG2 : fxas21002.h
- FXAS21002_CTRL_REG3 : fxas21002.h
- FXAS21002_DR_MASK : fxas21002.h
- FXAS21002_DR_SHIFT : fxas21002.h
- FXAS21002_DR_STATUS : fxas21002.h
- FXAS21002_ERROR_BURSTWRITE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_CONFIG : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_READ : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_SETPOWER : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_Error_tag : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_WAITFORACTIVE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_WHOAMI : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_ERROR_WRITE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_EXTCTRLEN_MASK : fxas21002.h
- FXAS21002_EXTCTRLEN_SHIFT : fxas21002.h
- fxas21002_extendAddress : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_F_EVENT : fxas21002.h
- FXAS21002_F_EVENT_MASK : fxas21002.h
- FXAS21002_F_EVENT_SHIFT : fxas21002.h
- FXAS21002_F_MODE_MASK : fxas21002.h
- FXAS21002_F_MODE_SHIFT : fxas21002.h
- FXAS21002_F_OVF_MASK : fxas21002.h
- FXAS21002_F_OVF_SHIFT : fxas21002.h
- FXAS21002_F_SETUP : fxas21002.h
- FXAS21002_F_STATUS : fxas21002.h
- FXAS21002_F_WMKF_MASK : fxas21002.h
- FXAS21002_F_WMKF_SHIFT : fxas21002.h
- FXAS21002_F_WMRK_MASK : fxas21002.h
- FXAS21002_F_WMRK_SHIFT : fxas21002.h
- FXAS21002_FE_TIME_MASK : fxas21002.h
- FXAS21002_FE_TIME_SHIFT : fxas21002.h
- FXAS21002_FS_MASK : fxas21002.h
- FXAS21002_FS_SHIFT : fxas21002.h
- FXAS21002_FSDOUBLE_MASK : fxas21002.h
- FXAS21002_FSDOUBLE_SHIFT : fxas21002.h
- FXAS21002_GET_FIELD : fxas21002.h
- FXAS21002_HPF_EN_MASK : fxas21002.h
- FXAS21002_HPF_EN_SHIFT : fxas21002.h
- FXAS21002_IIC_ADDRESS : fxas21002.h
- FXAS21002_INT_CFG_DRDY_MASK : fxas21002.h
- FXAS21002_INT_CFG_DRDY_SHIFT : fxas21002.h
- FXAS21002_INT_CFG_FIFO_MASK : fxas21002.h
- FXAS21002_INT_CFG_FIFO_SHIFT : fxas21002.h
- FXAS21002_INT_CFG_RT_MASK : fxas21002.h
- FXAS21002_INT_CFG_RT_SHIFT : fxas21002.h
- FXAS21002_INT_EN_DRDY_MASK : fxas21002.h
- FXAS21002_INT_EN_DRDY_SHIFT : fxas21002.h
- FXAS21002_INT_EN_FIFO_MASK : fxas21002.h
- FXAS21002_INT_EN_FIFO_SHIFT : fxas21002.h
- FXAS21002_INT_EN_RT_MASK : fxas21002.h
- FXAS21002_INT_EN_RT_SHIFT : fxas21002.h
- FXAS21002_INT_SRC_FLAG : fxas21002.h
- fxas21002_InternalState_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_InternalState_tag : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_IPOL_MASK : fxas21002.h
- FXAS21002_IPOL_SHIFT : fxas21002.h
- FXAS21002_NUMBER_AXIS : fxas21002.h
- FXAS21002_NUMBER_BYTES_AXIS : fxas21002.h
- fxas21002_ODR_Table_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_odrTable : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_OUT_X_LSB : fxas21002.h
- FXAS21002_OUT_X_MSB : fxas21002.h
- FXAS21002_OUT_Y_LSB : fxas21002.h
- FXAS21002_OUT_Y_MSB : fxas21002.h
- FXAS21002_OUT_Z_LSB : fxas21002.h
- FXAS21002_OUT_Z_MSB : fxas21002.h
- FXAS21002_POWER_ACTIVE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_POWER_STANDBY : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_Power_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_Power_tag : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_PP_OD_MASK : fxas21002.h
- FXAS21002_PP_OD_SHIFT : fxas21002.h
- FXAS21002_RANGE_1000DPS : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_RANGE_2000DPS : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_RANGE_500DPS : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_RANGE_MAX : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_Range_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_Range_tag : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_READY_MASK : fxas21002.h
- FXAS21002_READY_SHIFT : fxas21002.h
- FXAS21002_RESERVED : fxas21002.h
- FXAS21002_RST_MASK : fxas21002.h
- FXAS21002_RST_SHIFT : fxas21002.h
- FXAS21002_RT_CFG : fxas21002.h
- FXAS21002_RT_COUNT : fxas21002.h
- FXAS21002_RT_SRC : fxas21002.h
- FXAS21002_RT_THS : fxas21002.h
- FXAS21002_SAMPLE_PERIOD_MAX : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_SAMPLE_PERIOD_MIN : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_SEL_MASK : fxas21002.h
- FXAS21002_SEL_SHIFT : fxas21002.h
- FXAS21002_SET_FIELD : fxas21002.h
- FXAS21002_SPIW_MASK : fxas21002.h
- FXAS21002_SPIW_SHIFT : fxas21002.h
- FXAS21002_SRC_DRDY_MASK : fxas21002.h
- FXAS21002_SRC_DRDY_SHIFT : fxas21002.h
- FXAS21002_SRC_FIFO_MASK : fxas21002.h
- FXAS21002_SRC_FIFO_SHIFT : fxas21002.h
- FXAS21002_SRC_RT_MASK : fxas21002.h
- FXAS21002_SRC_RT_SHIFT : fxas21002.h
- FXAS21002_ST_MASK : fxas21002.h
- FXAS21002_ST_SHIFT : fxas21002.h
- FXAS21002_STANDBY_TO_ACTIVE_SAMPLE_WAIT : fxas21002.h
- FXAS21002_STATE_CONFIGURED : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_STATE_INITIALIZED : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_STATE_STARTED : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_STATE_UNINTIALIZED : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_STATUS : fxas21002.h
- fxas21002_Status_t : fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_status_t : fxas21002.h
- fxas21002_SupportedDataTypes : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- fxas21002_SupportedSensorTypes : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_TEMP : fxas21002.h
- FXAS21002_TEMP_FIXED_CONVERSION_FACTOR : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_TEMP_FIXED_CONVERSION_OFFSET : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_TEMP_FLOAT_CONVERSION_FACTOR : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_TEMP_FLOAT_CONVERSION_OFFSET : fsl_fxas21002_i2cspi_3D_gyro.c
- FXAS21002_WHO_AM_I : fxas21002.h
- FXAS21002_WHO_AM_I_VALUE_PRE_RELEASE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_WHO_AM_I_VALUE_RELEASE : fsl_fxas21002_i2cspi_3D_gyro.h
- FXAS21002_WHOAMI_VALUE_PRE_RELEASE : fxas21002.h
- FXAS21002_WHOAMI_VALUE_RELEASE : fxas21002.h
- FXAS21002_WRAPTOONE_MASK : fxas21002.h
- FXAS21002_WRAPTOONE_SHIFT : fxas21002.h
- FXAS21002_XDR_MASK : fxas21002.h
- FXAS21002_XDR_SHIFT : fxas21002.h
- FXAS21002_XOW_MASK : fxas21002.h
- FXAS21002_XOW_SHIFT : fxas21002.h
- FXAS21002_YDR_MASK : fxas21002.h
- FXAS21002_YDR_SHIFT : fxas21002.h
- FXAS21002_YOW_MASK : fxas21002.h
- FXAS21002_YOW_SHIFT : fxas21002.h
- FXAS21002_ZDR_MASK : fxas21002.h
- FXAS21002_ZDR_SHIFT : fxas21002.h
- FXAS21002_ZOW_MASK : fxas21002.h
- FXAS21002_ZOW_SHIFT : fxas21002.h
- FXAS21002_ZYXDR_MASK : fxas21002.h
- FXAS21002_ZYXDR_SHIFT : fxas21002.h
- FXAS21002_ZYXOW_MASK : fxas21002.h
- FXAS21002_ZYXOW_SHIFT : fxas21002.h
- fxas21002GyroConvTable : fsl_fxas21002_i2cspi_3D_gyro.c
- FXLC95000_1_ACC_ACCEL_RANGE_2G : FXLC95000_1.h
- FXLC95000_1_ACC_ACCEL_RANGE_4G : FXLC95000_1.h
- FXLC95000_1_ACC_ACCEL_RANGE_8G : FXLC95000_1.h
- FXLC95000_1_ACC_ACCEL_RESOLUTION_16_BIT : FXLC95000_1.h
- FXLC95000_1_ACC_FLOAT_CONVERSION_FACTOR : FXLC95000_1.h
- FXLC95000_1_ACC_MODE_ACCEL_ONLY : FXLC95000_1.h
- FXLC95000_1_Adapter : FXLC95000_1.c , FXLC95000_1.h
- FXLC95000_1_CONFIG_REGISTER_CMD_OFFSET : FXLC95000_1.h
- FXLC95000_1_CONFIG_REGISTER_READ_OFFSET : FXLC95000_1.h
- FXLC95000_1_CONFIG_REGISTER_SIZE : FXLC95000_1.h
- FXLC95000_1_ConfigRegisterBuffer : FXLC95000_1.c
- FXLC95000_1_DATA_TYPE : FXLC95000_1.h
- FXLC95000_1_DeviceInfo : FXLC95000_1.c , FXLC95000_1.h
- FXLC95000_1_SAMPLE_OFFSET : FXLC95000_1.h
- FXLC95000_1_SAMPLE_SIZE : FXLC95000_1.h
- FXLC95000_1_Sensor_Specific_Config : FXLC95000_1.c , FXLC95000_1.h
- FXLC95000_2_ACC_ACCEL_RANGE_2G : FXLC95000_2.h
- FXLC95000_2_ACC_ACCEL_RANGE_4G : FXLC95000_2.h
- FXLC95000_2_ACC_ACCEL_RANGE_8G : FXLC95000_2.h
- FXLC95000_2_ACC_ACCEL_RESOLUTION_16_BIT : FXLC95000_2.h
- FXLC95000_2_ACC_FLOAT_CONVERSION_FACTOR : FXLC95000_2.h
- FXLC95000_2_ACC_MODE_ACCEL_ONLY : FXLC95000_2.h
- FXLC95000_2_Adapter : FXLC95000_2.c , FXLC95000_2.h
- FXLC95000_2_CONFIG_REGISTER_CMD_OFFSET : FXLC95000_2.h
- FXLC95000_2_CONFIG_REGISTER_READ_OFFSET : FXLC95000_2.h
- FXLC95000_2_CONFIG_REGISTER_SIZE : FXLC95000_2.h
- FXLC95000_2_ConfigRegisterBuffer : FXLC95000_2.c
- FXLC95000_2_DATA_TYPE : FXLC95000_2.h
- FXLC95000_2_DeviceInfo : FXLC95000_2.c , FXLC95000_2.h
- FXLC95000_2_SAMPLE_OFFSET : FXLC95000_2.h
- FXLC95000_2_SAMPLE_SIZE : FXLC95000_2.h
- FXLC95000_2_Sensor_Specific_Config : FXLC95000_2.c , FXLC95000_2.h
- fxlc95000_GetConfig() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_GetData() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_read() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_send() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_status_t : fxlc95000.h
- fxlc95000_SupportedDataTypes : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fxlc95000_SupportedSensorTypes : fsl_fxlc95000_i2cspi_pedo.c , fsl_fxlc95000_i2cspi_pedo.h
- fxlc95000_ValidateConfig() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_waitForCoCo() : fsl_fxlc95000_i2cspi_pedo.c
- fxlc95000_WriteConfig() : fsl_fxlc95000_i2cspi_pedo.c
- FXLN83x1Q : Analog_1.h
- FXLN83x2Q : Analog_1.h
- FXLS8471_1_Adapter : FXLS8471_1.c , FXLS8471_1.h
- FXLS8471_1_DATA_TYPE : FXLS8471_1.h
- FXLS8471_1_DeviceInfo : FXLS8471_1.c , FXLS8471_1.h
- FXLS8471_1_Sensor_Specific_Config : FXLS8471_1.c , FXLS8471_1.h
- FXLS8471_2_Adapter : FXLS8471_2.c , FXLS8471_2.h
- FXLS8471_2_DATA_TYPE : FXLS8471_2.h
- FXLS8471_2_DeviceInfo : FXLS8471_2.c , FXLS8471_2.h
- FXLS8471_2_Sensor_Specific_Config : FXLS8471_2.c , FXLS8471_2.h
- FXLS8471_A_FFMT_DBCNTM_MASK : fxls8471.h
- FXLS8471_A_FFMT_DBCNTM_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_EA_MASK : fxls8471.h
- FXLS8471_A_FFMT_EA_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_ELE_MASK : fxls8471.h
- FXLS8471_A_FFMT_ELE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_OAE_MASK : fxls8471.h
- FXLS8471_A_FFMT_OAE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_THS_MASK : fxls8471.h
- FXLS8471_A_FFMT_THS_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_THS_X_LSB : fxls8471.h
- FXLS8471_A_FFMT_THS_X_MSB : fxls8471.h
- FXLS8471_A_FFMT_THS_XYZ_EN_MASK : fxls8471.h
- FXLS8471_A_FFMT_THS_XYZ_EN_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_THS_Y_LSB : fxls8471.h
- FXLS8471_A_FFMT_THS_Y_MSB : fxls8471.h
- FXLS8471_A_FFMT_THS_Z_LSB : fxls8471.h
- FXLS8471_A_FFMT_THS_Z_MSB : fxls8471.h
- FXLS8471_A_FFMT_XEFE_MASK : fxls8471.h
- FXLS8471_A_FFMT_XEFE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_XHE_MASK : fxls8471.h
- FXLS8471_A_FFMT_XHE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_XHP_MASK : fxls8471.h
- FXLS8471_A_FFMT_XHP_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_YEFE_MASK : fxls8471.h
- FXLS8471_A_FFMT_YEFE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_YHE_MASK : fxls8471.h
- FXLS8471_A_FFMT_YHE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_YHP_MASK : fxls8471.h
- FXLS8471_A_FFMT_YHP_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_ZEFE_MASK : fxls8471.h
- FXLS8471_A_FFMT_ZEFE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_ZHE_MASK : fxls8471.h
- FXLS8471_A_FFMT_ZHE_SHIFT : fxls8471.h
- FXLS8471_A_FFMT_ZHP_MASK : fxls8471.h
- FXLS8471_A_FFMT_ZHP_SHIFT : fxls8471.h
- FXLS8471_A_VECM_CFG : fxls8471.h
- FXLS8471_A_VECM_CNT : fxls8471.h
- FXLS8471_A_VECM_DBCNTM_MASK : fxls8471.h
- FXLS8471_A_VECM_DBCNTM_SHIFT : fxls8471.h
- FXLS8471_A_VECM_ELE_MASK : fxls8471.h
- FXLS8471_A_VECM_ELE_SHIFT : fxls8471.h
- FXLS8471_A_VECM_EN_MASK : fxls8471.h
- FXLS8471_A_VECM_EN_SHIFT : fxls8471.h
- FXLS8471_A_VECM_INITM_MASK : fxls8471.h
- FXLS8471_A_VECM_INITM_SHIFT : fxls8471.h
- FXLS8471_A_VECM_INITX_LSB : fxls8471.h
- FXLS8471_A_VECM_INITX_MSB : fxls8471.h
- FXLS8471_A_VECM_INITY_LSB : fxls8471.h
- FXLS8471_A_VECM_INITY_MSB : fxls8471.h
- FXLS8471_A_VECM_INITZ_LSB : fxls8471.h
- FXLS8471_A_VECM_INITZ_MSB : fxls8471.h
- FXLS8471_A_VECM_THS_LSB : fxls8471.h
- FXLS8471_A_VECM_THS_MSB : fxls8471.h
- FXLS8471_A_VECM_THS_MSB_MASK : fxls8471.h
- FXLS8471_A_VECM_THS_MSB_SHIFT : fxls8471.h
- FXLS8471_A_VECM_UPDM_MASK : fxls8471.h
- FXLS8471_A_VECM_UPDM_SHIFT : fxls8471.h
- FXLS8471_ACTIVE : fxls8471.h
- FXLS8471_ACTIVE_MASK : fxls8471.h
- FXLS8471_ACTIVE_SHIFT : fxls8471.h
- FXLS8471_ASLP_COUNT : fxls8471.h
- FXLS8471_ASLP_RATE_MASK : fxls8471.h
- FXLS8471_ASLP_RATE_SHIFT : fxls8471.h
- FXLS8471_AXX_MASK : fxls8471.h
- FXLS8471_AXY_MASK : fxls8471.h
- FXLS8471_AXZ_MASK : fxls8471.h
- FXLS8471_BAFRO_MASK : fxls8471.h
- FXLS8471_BAFRO_SHIFT : fxls8471.h
- FXLS8471_BKFR_MASK : fxls8471.h
- FXLS8471_BKFR_SHIFT : fxls8471.h
- fxls8471_CheckId() : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_CTRL_REG1 : fxls8471.h
- FXLS8471_CTRL_REG2 : fxls8471.h
- FXLS8471_CTRL_REG3 : fxls8471.h
- FXLS8471_CTRL_REG4 : fxls8471.h
- FXLS8471_CTRL_REG5 : fxls8471.h
- FXLS8471_DATA_OVERWRITE : fxls8471.h
- FXLS8471_DBCNTM_MASK : fxls8471.h
- FXLS8471_DBCNTM_SHIFT : fxls8471.h
- FXLS8471_DPA_MASK : fxls8471.h
- FXLS8471_DPA_SHIFT : fxls8471.h
- FXLS8471_DPE_MASK : fxls8471.h
- FXLS8471_DR_MASK : fxls8471.h
- FXLS8471_DR_SHIFT : fxls8471.h
- FXLS8471_ERROR : fxls8471.h
- FXLS8471_F_CNT_MASK : fxls8471.h
- FXLS8471_F_CNT_SHIFT : fxls8471.h
- FXLS8471_F_MODE_CIRCULAR : fxls8471.h
- FXLS8471_F_MODE_DISABLED : fxls8471.h
- FXLS8471_F_MODE_FILL : fxls8471.h
- FXLS8471_F_MODE_MASK : fxls8471.h
- FXLS8471_F_MODE_SHIFT : fxls8471.h
- FXLS8471_F_MODE_TRIGGER : fxls8471.h
- FXLS8471_F_OVF_MASK : fxls8471.h
- FXLS8471_F_OVF_SHIFT : fxls8471.h
- FXLS8471_F_SETUP : fxls8471.h
- FXLS8471_F_WMRK_FLAG_MASK : fxls8471.h
- FXLS8471_F_WMRK_FLAG_SHIFT : fxls8471.h
- FXLS8471_F_WMRK_MASK : fxls8471.h
- FXLS8471_F_WMRK_SHIFT : fxls8471.h
- FXLS8471_FFMT_CFG : fxls8471.h
- FXLS8471_FFMT_COUNT : fxls8471.h
- FXLS8471_FFMT_SRC : fxls8471.h
- FXLS8471_FFMT_THS : fxls8471.h
- FXLS8471_FGERR_MASK : fxls8471.h
- FXLS8471_FGERR_SHIFT : fxls8471.h
- FXLS8471_FGT_MASK : fxls8471.h
- FXLS8471_FGT_SHIFT : fxls8471.h
- FXLS8471_FIFO_GATE_MASK : fxls8471.h
- FXLS8471_FIFO_GATE_SHIFT : fxls8471.h
- FXLS8471_FREAD_MASK : fxls8471.h
- FXLS8471_FREAD_SHIFT : fxls8471.h
- FXLS8471_FS_MASK : fxls8471.h
- FXLS8471_FS_SHIFT : fxls8471.h
- FXLS8471_GET_FIELD : fxls8471.h
- fxls8471_GetConfig() : fsl_fxls8471_i2cspi_3D_accel.c
- fxls8471_GetData() : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_HP_FILTER_CUTOFF : fxls8471.h
- FXLS8471_HPF_BYP_MASK : fxls8471.h
- FXLS8471_HPF_BYP_SHIFT : fxls8471.h
- FXLS8471_HPF_OUT_MASK : fxls8471.h
- FXLS8471_HPF_OUT_SHIFT : fxls8471.h
- FXLS8471_HYS_MASK : fxls8471.h
- FXLS8471_HYS_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_A_VECM_MASK : fxls8471.h
- FXLS8471_INT_CFG_A_VECM_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_ASLP_MASK : fxls8471.h
- FXLS8471_INT_CFG_ASLP_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_DRDY_MASK : fxls8471.h
- FXLS8471_INT_CFG_DRDY_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_FFMT_MASK : fxls8471.h
- FXLS8471_INT_CFG_FFMT_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_FIFO_MASK : fxls8471.h
- FXLS8471_INT_CFG_FIFO_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_LNDPRT_MASK : fxls8471.h
- FXLS8471_INT_CFG_LNDPRT_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_PULSE_MASK : fxls8471.h
- FXLS8471_INT_CFG_PULSE_SHIFT : fxls8471.h
- FXLS8471_INT_CFG_TRANS_MASK : fxls8471.h
- FXLS8471_INT_CFG_TRANS_SHIFT : fxls8471.h
- FXLS8471_INT_EN_A_VECM_MASK : fxls8471.h
- FXLS8471_INT_EN_A_VECM_SHIFT : fxls8471.h
- FXLS8471_INT_EN_ASLP_MASK : fxls8471.h
- FXLS8471_INT_EN_ASLP_SHIFT : fxls8471.h
- FXLS8471_INT_EN_DRDY_MASK : fxls8471.h
- FXLS8471_INT_EN_DRDY_SHIFT : fxls8471.h
- FXLS8471_INT_EN_FFMT_MASK : fxls8471.h
- FXLS8471_INT_EN_FFMT_SHIFT : fxls8471.h
- FXLS8471_INT_EN_FIFO_MASK : fxls8471.h
- FXLS8471_INT_EN_FIFO_SHIFT : fxls8471.h
- FXLS8471_INT_EN_LNDPRT_MASK : fxls8471.h
- FXLS8471_INT_EN_LNDPRT_SHIFT : fxls8471.h
- FXLS8471_INT_EN_PULSE_MASK : fxls8471.h
- FXLS8471_INT_EN_PULSE_SHIFT : fxls8471.h
- FXLS8471_INT_EN_TRANS_MASK : fxls8471.h
- FXLS8471_INT_EN_TRANS_SHIFT : fxls8471.h
- FXLS8471_INT_SOURCE : fxls8471.h
- FXLS8471_IPOL_MASK : fxls8471.h
- FXLS8471_IPOL_SHIFT : fxls8471.h
- FXLS8471_LAPO_MASK : fxls8471.h
- FXLS8471_LAPO_SHIFT : fxls8471.h
- FXLS8471_LNOISE_MASK : fxls8471.h
- FXLS8471_LNOISE_SHIFT : fxls8471.h
- FXLS8471_LO_MASK : fxls8471.h
- FXLS8471_LO_SHIFT : fxls8471.h
- FXLS8471_MODS_MASK : fxls8471.h
- FXLS8471_MODS_SHIFT : fxls8471.h
- FXLS8471_NEWLP_MASK : fxls8471.h
- FXLS8471_NEWLP_SHIFT : fxls8471.h
- FXLS8471_OFF_X : fxls8471.h
- FXLS8471_OFF_Y : fxls8471.h
- FXLS8471_OFF_Z : fxls8471.h
- FXLS8471_OUT_X_LSB : fxls8471.h
- FXLS8471_OUT_X_MSB : fxls8471.h
- FXLS8471_OUT_Y_lSB : fxls8471.h
- FXLS8471_OUT_Y_MSB : fxls8471.h
- FXLS8471_OUT_Z_LSB : fxls8471.h
- FXLS8471_OUT_Z_MSB : fxls8471.h
- FXLS8471_PEA_MASK : fxls8471.h
- FXLS8471_PELE_MASK : fxls8471.h
- FXLS8471_PELE_SHIFT : fxls8471.h
- FXLS8471_PL_BF_ZCOMP : fxls8471.h
- FXLS8471_PL_CFG : fxls8471.h
- FXLS8471_PL_COUNT : fxls8471.h
- FXLS8471_PL_EN_MASK : fxls8471.h
- FXLS8471_PL_EN_SHIFT : fxls8471.h
- FXLS8471_PL_STATUS : fxls8471.h
- FXLS8471_PL_THS : fxls8471.h
- FXLS8471_PL_THS_MASK : fxls8471.h
- FXLS8471_PL_THS_SHIFT : fxls8471.h
- FXLS8471_POLX_MASK : fxls8471.h
- FXLS8471_POLY_MASK : fxls8471.h
- FXLS8471_POLZ_MASK : fxls8471.h
- FXLS8471_PP_OD_MASK : fxls8471.h
- FXLS8471_PP_OD_SHIFT : fxls8471.h
- FXLS8471_PTHS_MASK : fxls8471.h
- FXLS8471_PTHS_SHIFT : fxls8471.h
- FXLS8471_PULSE_CFG : fxls8471.h
- FXLS8471_PULSE_HPF_BYP_MASK : fxls8471.h
- FXLS8471_PULSE_HPF_BYP_SHIFT : fxls8471.h
- FXLS8471_PULSE_LPF_EN_MASK : fxls8471.h
- FXLS8471_PULSE_LPF_EN_SHIFT : fxls8471.h
- FXLS8471_PULSE_LTCY : fxls8471.h
- FXLS8471_PULSE_SRC : fxls8471.h
- FXLS8471_PULSE_THSX : fxls8471.h
- FXLS8471_PULSE_THSY : fxls8471.h
- FXLS8471_PULSE_THSZ : fxls8471.h
- FXLS8471_PULSE_TMLT : fxls8471.h
- FXLS8471_PULSE_WIND : fxls8471.h
- fxls8471_Reset() : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_RST_MASK : fxls8471.h
- FXLS8471_RST_SHIFT : fxls8471.h
- FXLS8471_SEL_MASK : fxls8471.h
- FXLS8471_SEL_SHIFT : fxls8471.h
- FXLS8471_SET_FIELD : fxls8471.h
- fxls8471_SetConfig() : fsl_fxls8471_i2cspi_3D_accel.c
- fxls8471_SetMode() : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_SLPE_MASK : fxls8471.h
- FXLS8471_SLPE_SHIFT : fxls8471.h
- FXLS8471_SMODS_MASK : fxls8471.h
- FXLS8471_SMODS_SHIFT : fxls8471.h
- FXLS8471_SRC_A_VECM_MASK : fxls8471.h
- FXLS8471_SRC_A_VECM_SHIFT : fxls8471.h
- FXLS8471_SRC_ASLP_MASK : fxls8471.h
- FXLS8471_SRC_ASLP_SHIFT : fxls8471.h
- FXLS8471_SRC_DRDY_MASK : fxls8471.h
- FXLS8471_SRC_DRDY_SHIFT : fxls8471.h
- FXLS8471_SRC_FFMT_MASK : fxls8471.h
- FXLS8471_SRC_FFMT_SHIFT : fxls8471.h
- FXLS8471_SRC_FIFO_MASK : fxls8471.h
- FXLS8471_SRC_FIFO_SHIFT : fxls8471.h
- FXLS8471_SRC_LNDPRT_MASK : fxls8471.h
- FXLS8471_SRC_LNDPRT_SHIFT : fxls8471.h
- FXLS8471_SRC_PULSE_MASK : fxls8471.h
- FXLS8471_SRC_PULSE_SHIFT : fxls8471.h
- FXLS8471_SRC_TRANS_MASK : fxls8471.h
- FXLS8471_SRC_TRANS_SHIFT : fxls8471.h
- FXLS8471_ST_MASK : fxls8471.h
- FXLS8471_ST_SHIFT : fxls8471.h
- FXLS8471_STANDBY : fxls8471.h
- FXLS8471_STATUS : fxls8471.h
- fxls8471_status_t : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_SUCCESS : fxls8471.h
- fxls8471_SupportedDataTypes : fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8471_i2cspi_3D_accel.h
- fxls8471_SupportedSensorTypes : fsl_fxls8471_i2cspi_3D_accel.c , fsl_fxls8471_i2cspi_3D_accel.h
- FXLS8471_SYSMOD : fxls8471.h
- FXLS8471_SYSMOD_MASK : fxls8471.h
- FXLS8471_SYSMOD_SHIFT : fxls8471.h
- FXLS8471_SYSMOD_SLEEP : fxls8471.h
- FXLS8471_SYSMOD_STANDBY : fxls8471.h
- FXLS8471_SYSMOD_WAKE : fxls8471.h
- FXLS8471_TEA_MASK : fxls8471.h
- FXLS8471_TELE_MASK : fxls8471.h
- FXLS8471_TELE_SHIFT : fxls8471.h
- FXLS8471_TRANSIENT_CFG : fxls8471.h
- FXLS8471_TRANSIENT_COUNT : fxls8471.h
- FXLS8471_TRANSIENT_SRC : fxls8471.h
- FXLS8471_TRANSIENT_THS : fxls8471.h
- FXLS8471_TRIG_A_VECM_MASK : fxls8471.h
- FXLS8471_TRIG_A_VECM_SHIFT : fxls8471.h
- FXLS8471_TRIG_CFG : fxls8471.h
- FXLS8471_TRIG_FFMT_MASK : fxls8471.h
- FXLS8471_TRIG_FFMT_SHIFT : fxls8471.h
- FXLS8471_TRIG_LNDPRT_MASK : fxls8471.h
- FXLS8471_TRIG_LNDPRT_SHIFT : fxls8471.h
- FXLS8471_TRIG_PULSE_MASK : fxls8471.h
- FXLs8471_TRIG_PULSE_SHIFT : fxls8471.h
- FXLS8471_TRIG_TRANS_MASK : fxls8471.h
- FXLS8471_TRIG_TRANS_SHIFT : fxls8471.h
- fxls8471_ValidateConfig() : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8471_WAKE_A_VECM_MASK : fxls8471.h
- FXLS8471_WAKE_A_VECM_SHIFT : fxls8471.h
- FXLS8471_WAKE_FFMT_MASK : fxls8471.h
- FXLS8471_WAKE_FFMT_SHIFT : fxls8471.h
- FXLS8471_WAKE_LNDPRT_MASK : fxls8471.h
- FXLS8471_WAKE_LNDPRT_SHIFT : fxls8471.h
- FXLS8471_WAKE_PULSE_MASK : fxls8471.h
- FXLS8471_WAKE_PULSE_SHIFT : fxls8471.h
- FXLS8471_WAKE_TRANS_MASK : fxls8471.h
- FXLS8471_WAKE_TRANS_SHIFT : fxls8471.h
- FXLS8471_WHO_AM_I : fxls8471.h
- FXLS8471_WHOAMI_VALUE : fxls8471.h
- FXLS8471_X_TRANS_POL_MASK : fxls8471.h
- FXLS8471_XDPEFE_MASK : fxls8471.h
- FXLS8471_XDPEFE_SHIFT : fxls8471.h
- FXLS8471_XDR_MASK : fxls8471.h
- FXLS8471_XOW_MASK : fxls8471.h
- FXLS8471_XSPEFE_MASK : fxls8471.h
- FXLS8471_XSPEFE_SHIFT : fxls8471.h
- FXLS8471_XTEFE_MASK : fxls8471.h
- FXLS8471_XTEFE_SHIFT : fxls8471.h
- FXLS8471_XTRANSE_MASK : fxls8471.h
- FXLS8471_XYZ_DATA_CFG : fxls8471.h
- FXLS8471_Y_TRANS_POL_MASK : fxls8471.h
- FXLS8471_YDPEFE_MASK : fxls8471.h
- FXLS8471_YDPEFE_SHIFT : fxls8471.h
- FXLS8471_YDR_MASK : fxls8471.h
- FXLS8471_YOW_MASK : fxls8471.h
- FXLS8471_YSPEFE_MASK : fxls8471.h
- FXLS8471_YSPEFE_SHIFT : fxls8471.h
- FXLS8471_YTEFE_MASK : fxls8471.h
- FXLS8471_YTEFE_SHIFT : fxls8471.h
- FXLS8471_YTRANSE_MASK : fxls8471.h
- FXLS8471_Z_TRANS_POL_MASK : fxls8471.h
- FXLS8471_ZDPEFE_MASK : fxls8471.h
- FXLS8471_ZDPEFE_SHIFT : fxls8471.h
- FXLS8471_ZDR_MASK : fxls8471.h
- FXLS8471_ZLOCK_MASK : fxls8471.h
- FXLS8471_ZLOCK_SHIFT : fxls8471.h
- FXLS8471_ZOW_MASK : fxls8471.h
- FXLS8471_ZSPEFE_MASK : fxls8471.h
- FXLS8471_ZSPEFE_SHIFT : fxls8471.h
- FXLS8471_ZTEFE_MASK : fxls8471.h
- FXLS8471_ZTEFE_SHIFT : fxls8471.h
- FXLS8471_ZTRANSE_MASK : fxls8471.h
- FXLS8471_ZYXDR_MASK : fxls8471.h
- FXLS8471_ZYXDR_SHIFT : fxls8471.h
- FXLS8471_ZYXOW_MASK : fxls8471.h
- FXLS8471_ZYXOW_SHIFT : fxls8471.h
- fxls8471AccelConvTable : fsl_fxls8471_i2cspi_3D_accel.c
- FXLS8952_1_Adapter : FXLS8952_1.c , FXLS8952_1.h
- FXLS8952_1_DATA_TYPE : FXLS8952_1.h
- FXLS8952_1_DeviceInfo : FXLS8952_1.h , FXLS8952_1.c
- FXLS8952_1_Sensor_Specific_Config : FXLS8952_1.c , FXLS8952_1.h
- FXLS8952_ACCEL_FIXED_CONVERSION_FACTOR : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_ACCEL_FIXED_CONVERSION_OFFSET : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_ACCEL_FLOAT_CONVERSION_FACTOR : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_ACCEL_FLOAT_CONVERSION_OFFSET : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_ACTIVE_MASK : fxls8952.h
- FXLS8952_ACTIVE_SHIFT : fxls8952.h
- FXLS8952_AINC_TEMP_MASK : fxls8952.h
- FXLS8952_AINC_TEMP_SHIFT : fxls8952.h
- FXLS8952_ASLP_COUNT_LSB : fxls8952.h
- FXLS8952_ASLP_COUNT_MSB : fxls8952.h
- FXLS8952_ASLP_EN_MASK : fxls8952.h
- FXLS8952_ASLP_EN_SHIFT : fxls8952.h
- FXLS8952_ASLP_INT2_MASK : fxls8952.h
- FXLS8952_ASLP_INT2_SHIFT : fxls8952.h
- FXLS8952_BAFRO_MASK : fxls8952.h
- FXLS8952_BAFRO_SHIFT : fxls8952.h
- FXLS8952_BOOT_DIS_MASK : fxls8952.h
- FXLS8952_BOOT_DIS_SHIFT : fxls8952.h
- FXLS8952_BOOT_INT2_MASK : fxls8952.h
- FXLS8952_BOOT_INT2_SHIFT : fxls8952.h
- FXLS8952_BUF_CFG_WMRK_MASK : fxls8952.h
- FXLS8952_BUF_CFG_WMRK_SHIFT : fxls8952.h
- FXLS8952_BUF_CNT_MASK : fxls8952.h
- FXLS8952_BUF_CNT_SHIFT : fxls8952.h
- FXLS8952_BUF_CONFIG1 : fxls8952.h
- FXLS8952_BUF_CONFIG2 : fxls8952.h
- FXLS8952_BUF_EN_MASK : fxls8952.h
- FXLS8952_BUF_EN_SHIFT : fxls8952.h
- FXLS8952_BUF_FLUSH_MASK : fxls8952.h
- FXLS8952_BUF_FLUSH_SHIFT : fxls8952.h
- FXLS8952_BUF_GATE_CNT_MASK : fxls8952.h
- FXLS8952_BUF_GATE_CNT_SHIFT : fxls8952.h
- FXLS8952_BUF_GATE_ERR_MASK : fxls8952.h
- FXLS8952_BUF_GATE_ERR_SHIFT : fxls8952.h
- FXLS8952_BUF_GATE_MASK : fxls8952.h
- FXLS8952_BUF_GATE_SHIFT : fxls8952.h
- FXLS8952_BUF_INT2_MASK : fxls8952.h
- FXLS8952_BUF_INT2_SHIFT : fxls8952.h
- FXLS8952_BUF_MODE_MASK : fxls8952.h
- FXLS8952_BUF_MODE_SHIFT : fxls8952.h
- FXLS8952_BUF_OVF_MASK : fxls8952.h
- FXLS8952_BUF_OVF_SHIFT : fxls8952.h
- FXLS8952_BUF_STATUS : fxls8952.h
- FXLS8952_BUF_TYPE_MASK : fxls8952.h
- FXLS8952_BUF_TYPE_SHIFT : fxls8952.h
- FXLS8952_BUF_WMRK_MASK : fxls8952.h
- FXLS8952_BUF_WMRK_SHIFT : fxls8952.h
- FXLS8952_BUF_X_LSB : fxls8952.h
- FXLS8952_BUF_X_MSB : fxls8952.h
- FXLS8952_BUF_Y_LSB : fxls8952.h
- FXLS8952_BUF_Y_MSB : fxls8952.h
- FXLS8952_BUF_Z_LSB : fxls8952.h
- FXLS8952_BUF_Z_MSB : fxls8952.h
- fxls8952_ConfigTable_t : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_DATA_OVERWRITE : fxls8952.h
- FXLS8952_DRDY_EN_MASK : fxls8952.h
- FXLS8952_DRDY_EN_SHIFT : fxls8952.h
- FXLS8952_DRDY_INT2_MASK : fxls8952.h
- FXLS8952_DRDY_INT2_SHIFT : fxls8952.h
- FXLS8952_DRDY_PUL_MASK : fxls8952.h
- FXLS8952_DRDY_PUL_SHIFT : fxls8952.h
- FXLS8952_ERRO_READ : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERRO_WRITE : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERROR : fxls8952.h
- FXLS8952_ERROR_BURSTWRITE : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERROR_CONFIG : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERROR_SETPOWER : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Error_tag : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERROR_WAITFORACTIVE : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_ERROR_WHOAMI : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_EXT_TRIG_M_MASK : fxls8952.h
- FXLS8952_EXT_TRIG_M_SHIFT : fxls8952.h
- FXLS8952_F_READ_MASK : fxls8952.h
- FXLS8952_F_READ_SHIFT : fxls8952.h
- FXLS8952_FSR_MASK : fxls8952.h
- FXLS8952_FSR_SHIFT : fxls8952.h
- FXLS8952_GET_FIELD : fxls8952.h
- FXLS8952_HYS_MASK : fxls8952.h
- FXLS8952_HYS_SHIFT : fxls8952.h
- FXLS8952_INT2_FUNC_MASK : fxls8952.h
- FXLS8952_INT2_FUNC_SHIFT : fxls8952.h
- FXLS8952_INT_EN : fxls8952.h
- FXLS8952_INT_PIN_SEL : fxls8952.h
- FXLS8952_INT_POL_MASK : fxls8952.h
- FXLS8952_INT_POL_SHIFT : fxls8952.h
- FXLS8952_INT_PP_OD_MASK : fxls8952.h
- FXLS8952_INT_PP_OD_SHIFT : fxls8952.h
- FXLS8952_INT_STATUS : fxls8952.h
- fxls8952_InternalState_t : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_InternalState_tag : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_LAPO_MASK : fxls8952.h
- FXLS8952_LAPO_SHIFT : fxls8952.h
- FXLS8952_LE_BE_MASK : fxls8952.h
- FXLS8952_LE_BE_SHIFT : fxls8952.h
- FXLS8952_LO_MASK : fxls8952.h
- FXLS8952_LO_SHIFT : fxls8952.h
- FXLS8952_NEW_ORIENT_MASK : fxls8952.h
- FXLS8952_NEW_ORIENT_SHIFT : fxls8952.h
- fxls8952_ODR_Table_t : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_odrTable : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_OFF_X : fxls8952.h
- FXLS8952_OFF_Y : fxls8952.h
- FXLS8952_OFF_Z : fxls8952.h
- FXLS8952_ORIENT_BF_ZCOMP : fxls8952.h
- FXLS8952_ORIENT_BKFR_MASK : fxls8952.h
- FXLS8952_ORIENT_BKFR_SHIFT : fxls8952.h
- FXLS8952_ORIENT_CFG : fxls8952.h
- FXLS8952_ORIENT_DBCNTM_MASK : fxls8952.h
- FXLS8952_ORIENT_DBCNTM_SHIFT : fxls8952.h
- FXLS8952_ORIENT_DBCOUNT : fxls8952.h
- FXLS8952_ORIENT_DBCOUNT_MASK : fxls8952.h
- FXLS8952_ORIENT_DBCOUNT_SHIFT : fxls8952.h
- FXLS8952_ORIENT_EN_MASK : fxls8952.h
- FXLS8952_ORIENT_EN_SHIFT : fxls8952.h
- FXLS8952_ORIENT_ENABLE_MASK : fxls8952.h
- FXLS8952_ORIENT_ENABLE_SHIFT : fxls8952.h
- FXLS8952_ORIENT_INT2_MASK : fxls8952.h
- FXLS8952_ORIENT_INT2_SHIFT : fxls8952.h
- FXLS8952_ORIENT_STATUS : fxls8952.h
- FXLS8952_ORIENT_THS_MASK : fxls8952.h
- FXLS8952_ORIENT_THS_REG : fxls8952.h
- FXLS8952_ORIENT_THS_SHIFT : fxls8952.h
- FXLS8952_ORIENT_ZLOCK_MASK : fxls8952.h
- FXLS8952_ORIENT_ZLOCK_SHIFT : fxls8952.h
- FXLS8952_OT_DBCTM_MASK : fxls8952.h
- FXLS8952_OT_DBCTM_SHIFT : fxls8952.h
- FXLS8952_OT_ELE_MASK : fxls8952.h
- FXLS8952_OT_ELE_SHIFT : fxls8952.h
- FXLS8952_OUT_X_LSB : fxls8952.h
- FXLS8952_OUT_X_MSB : fxls8952.h
- FXLS8952_OUT_Y_LSB : fxls8952.h
- FXLS8952_OUT_Y_MSB : fxls8952.h
- FXLS8952_OUT_Z_LSB : fxls8952.h
- FXLS8952_OUT_Z_MSB : fxls8952.h
- FXLS8952_POWER_ACTIVE : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_POWER_STANDBY : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Power_t : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Power_tag : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_RANGE_16G : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_RANGE_2G : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_RANGE_4G : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_RANGE_8G : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_RANGE_MAX : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Range_t : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Range_tag : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_REF_UPD_MASK : fxls8952.h
- FXLS8952_REF_UPD_SHIFT : fxls8952.h
- FXLS8952_REF_UPDM_MASK : fxls8952.h
- FXLS8952_REF_UPDM_SHIFT : fxls8952.h
- FXLS8952_RST_MASK : fxls8952.h
- FXLS8952_RST_SHIFT : fxls8952.h
- FXLS8952_SAMPLE_PERIOD_MAX : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_SAMPLE_PERIOD_MIN : fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_SDCD_CONFIG1 : fxls8952.h
- FXLS8952_SDCD_CONFIG2 : fxls8952.h
- FXLS8952_SDCD_EN_MASK : fxls8952.h
- FXLS8952_SDCD_EN_SHIFT : fxls8952.h
- FXLS8952_SDCD_INT_SRC : fxls8952.h
- FXLS8952_SDCD_LTHS_LSB : fxls8952.h
- FXLS8952_SDCD_LTHS_MSB : fxls8952.h
- FXLS8952_SDCD_OT_DBCNT : fxls8952.h
- FXLS8952_SDCD_OT_EN_MASK : fxls8952.h
- FXLS8952_SDCD_OT_EN_SHIFT : fxls8952.h
- FXLS8952_SDCD_OT_INT2_MASK : fxls8952.h
- FXLS8952_SDCD_OT_INT2_SHIFT : fxls8952.h
- FXLS8952_SDCD_UTHS_LSB : fxls8952.h
- FXLS8952_SDCD_UTHS_MSB : fxls8952.h
- FXLS8952_SDCD_WT_DBCNT : fxls8952.h
- FXLS8952_SDCD_WT_EN_MASK : fxls8952.h
- FXLS8952_SDCD_WT_EN_SHIFT : fxls8952.h
- FXLS8952_SDCD_WT_INT2_MASK : fxls8952.h
- FXLS8952_SDCD_WT_INT2_SHIFT : fxls8952.h
- FXLS8952_SDCD_X_WT_EF_MASK : fxls8952.h
- FXLS8952_SDCD_X_WT_EF_SHIFT : fxls8952.h
- FXLS8952_SDCD_Y_WT_EF_MASK : fxls8952.h
- FXLS8952_SDCD_Y_WT_EF_SHIFT : fxls8952.h
- FXLS8952_SDCD_Z_WT_EF_MASK : fxls8952.h
- FXLS8952_SDCD_Z_WT_EF_SHIFT : fxls8952.h
- FXLS8952_SENS_CONFIG1 : fxls8952.h
- FXLS8952_SENS_CONFIG2 : fxls8952.h
- FXLS8952_SENS_CONFIG3 : fxls8952.h
- FXLS8952_SENS_CONFIG4 : fxls8952.h
- FXLS8952_SET_FIELD : fxls8952.h
- FXLS8952_SLEEP_IDLE_LSB : fxls8952.h
- FXLS8952_SLEEP_IDLE_MSB : fxls8952.h
- FXLS8952_SLEEP_ODR_MASK : fxls8952.h
- FXLS8952_SLEEP_ODR_SHIFT : fxls8952.h
- FXLS8952_SLEEP_PM_MASK : fxls8952.h
- FXLS8952_SLEEP_PM_SHIFT : fxls8952.h
- FXLS8952_SRC_ASLP_MASK : fxls8952.h
- FXLS8952_SRC_ASLP_SHIFT : fxls8952.h
- FXLS8952_SRC_BOOT_MASK : fxls8952.h
- FXLS8952_SRC_BOOT_SHIFT : fxls8952.h
- FXLS8952_SRC_BUF_MASK : fxls8952.h
- FXLS8952_SRC_BUF_SHIFT : fxls8952.h
- FXLS8952_SRC_DRDY_MASK : fxls8952.h
- FXLS8952_SRC_DRDY_SHIFT : fxls8952.h
- FXLS8952_SRC_ORIENT_MASK : fxls8952.h
- FXLS8952_SRC_ORIENT_SHIFT : fxls8952.h
- FXLS8952_SRC_OVF_MASK : fxls8952.h
- FXLS8952_SRC_OVF_SHIFT : fxls8952.h
- FXLS8952_SRC_SDCD_AND_MASK : fxls8952.h
- FXLS8952_SRC_SDCD_AND_SHIFT : fxls8952.h
- FXLS8952_SRC_SDCD_OR_MASK : fxls8952.h
- FXLS8952_SRC_SDCD_OR_SHIFT : fxls8952.h
- FXLS8952_ST_AXIS_SEL_MASK : fxls8952.h
- FXLS8952_ST_AXIS_SEL_SHIFT : fxls8952.h
- FXLS8952_ST_POL_MASK : fxls8952.h
- FXLS8952_ST_POL_SHIFT : fxls8952.h
- FXLS8952_STATE_CONFIGURED : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_STATE_INITIALIZED : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_STATE_STARTED : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_STATE_UNINTIALIZED : fsl_fxls8952_i2c_3D_accel.h
- fxls8952_Status_t : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_SUCCESS : fxls8952.h
- fxls8952_SupportedDataTypes : fsl_fxls8952_i2c_3D_accel.c , fsl_fxls8952_i2c_3D_accel.h
- fxls8952_SupportedSensorTypes : fsl_fxls8952_i2c_3D_accel.h , fsl_fxls8952_i2c_3D_accel.c
- FXLS8952_SYS_MODE : fxls8952.h
- FXLS8952_SYS_MODE_MASK : fxls8952.h
- FXLS8952_SYS_MODE_SHIFT : fxls8952.h
- FXLS8952_TEMP_OUT : fxls8952.h
- FXLS8952_TRIG_ORIENT_MASK : fxls8952.h
- FXLS8952_TRIG_ORIENT_SHIFT : fxls8952.h
- FXLS8952_TRIG_SDCD_OT_MASK : fxls8952.h
- FXLS8952_TRIG_SDCD_OT_SHIFT : fxls8952.h
- FXLS8952_TRIG_SDCD_WT_MASK : fxls8952.h
- FXLS8952_TRIG_SDCD_WT_SHIFT : fxls8952.h
- FXLS8952_WAKE_IDLE_LSB : fxls8952.h
- FXLS8952_WAKE_IDLE_MSB : fxls8952.h
- FXLS8952_WAKE_ODR_MASK : fxls8952.h
- FXLS8952_WAKE_ODR_SHIFT : fxls8952.h
- FXLS8952_WAKE_ORIENT_MASK : fxls8952.h
- FXLS8952_WAKE_ORIENT_SHIFT : fxls8952.h
- FXLS8952_WAKE_OUT_EN_MASK : fxls8952.h
- FXLS8952_WAKE_OUT_EN_SHIFT : fxls8952.h
- FXLS8952_WAKE_OUT_INT2_MASK : fxls8952.h
- FXLS8952_WAKE_OUT_INT2_SHIFT : fxls8952.h
- FXLS8952_WAKE_PM_MASK : fxls8952.h
- FXLS8952_WAKE_PM_SHIFT : fxls8952.h
- FXLS8952_WAKE_SDCD_OT_MASK : fxls8952.h
- FXLS8952_WAKE_SDCD_OT_SHIFT : fxls8952.h
- FXLS8952_WAKE_SDCD_WT_MASK : fxls8952.h
- FXLS8952_WAKE_SDCD_WT_SHIFT : fxls8952.h
- FXLS8952_WAKE_SRC_BUF_MASK : fxls8952.h
- FXLS8952_WAKE_SRC_BUF_SHIFT : fxls8952.h
- FXLS8952_WHO_AM_I : fxls8952.h
- FXLS8952_WHO_AM_I_VALUE : fsl_fxls8952_i2c_3D_accel.h
- FXLS8952_WHOAMI_VALUE : fxls8952.h
- FXLS8952_WT_DBCTM_MASK : fxls8952.h
- FXLS8952_WT_DBCTM_SHIFT : fxls8952.h
- FXLS8952_WT_ELE_MASK : fxls8952.h
- FXLS8952_WT_ELE_SHIFT : fxls8952.h
- FXLS8952_WT_LOG_SEL_MASK : fxls8952.h
- FXLS8952_WT_LOG_SEL_SHIFT : fxls8952.h
- FXLS8952_X_OT_EN_MASK : fxls8952.h
- FXLS8952_X_OT_EN_SHIFT : fxls8952.h
- FXLS8952_X_WT_EN_MASK : fxls8952.h
- FXLS8952_X_WT_EN_SHIFT : fxls8952.h
- FXLS8952_Y_OT_EN_MASK : fxls8952.h
- FXLS8952_Y_OT_EN_SHIFT : fxls8952.h
- FXLS8952_Y_WT_EN_MASK : fxls8952.h
- FXLS8952_Y_WT_EN_SHIFT : fxls8952.h
- FXLS8952_Z_OT_EN_MASK : fxls8952.h
- FXLS8952_Z_OT_EN_SHIFT : fxls8952.h
- FXLS8952_Z_WT_EN_MASK : fxls8952.h
- FXLS8952_Z_WT_EN_SHIFT : fxls8952.h
- fxls8952AccelConvTable : fsl_fxls8952_i2c_3D_accel.c
- fxo8700_ODR_Table_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_1_Adapter : FXOS8700_1.h , FXOS8700_1.c
- FXOS8700_1_DATA_TYPE : FXOS8700_1.h
- FXOS8700_1_DeviceInfo : FXOS8700_1.c , FXOS8700_1.h
- FXOS8700_1_Sensor_Specific_Config : FXOS8700_1.h , FXOS8700_1.c
- FXOS8700_2_Adapter : FXOS8700_2.c , FXOS8700_2.h
- FXOS8700_2_DATA_TYPE : FXOS8700_2.h
- FXOS8700_2_DeviceInfo : FXOS8700_2.h , FXOS8700_2.c
- FXOS8700_2_Sensor_Specific_Config : FXOS8700_2.c , FXOS8700_2.h
- FXOS8700_A_FFMT_THS_X_LSB : fxos8700.h
- FXOS8700_A_FFMT_THS_X_MSB : fxos8700.h
- FXOS8700_A_FFMT_THS_Y_LSB : fxos8700.h
- FXOS8700_A_FFMT_THS_Y_MSB : fxos8700.h
- FXOS8700_A_FFMT_THS_Z_LSB : fxos8700.h
- FXOS8700_A_FFMT_THS_Z_MSB : fxos8700.h
- FXOS8700_A_VECM_CFG : fxos8700.h
- FXOS8700_A_VECM_CNT : fxos8700.h
- FXOS8700_A_VECM_INITX_LSB : fxos8700.h
- FXOS8700_A_VECM_INITX_MSB : fxos8700.h
- FXOS8700_A_VECM_INITY_LSB : fxos8700.h
- FXOS8700_A_VECM_INITY_MSB : fxos8700.h
- FXOS8700_A_VECM_INITZ_LSB : fxos8700.h
- FXOS8700_A_VECM_INITZ_MSB : fxos8700.h
- FXOS8700_A_VECM_THS_LSB : fxos8700.h
- FXOS8700_A_VECM_THS_MSB : fxos8700.h
- FXOS8700_ACTIVE_MASK : fxos8700.h
- FXOS8700_ACTIVE_SHIFT : fxos8700.h
- FXOS8700_ASLP_COUNT : fxos8700.h
- FXOS8700_ASLP_RATE_MASK : fxos8700.h
- FXOS8700_ASLP_RATE_SHIFT : fxos8700.h
- FXOS8700_AXX_MASK : fxos8700.h
- FXOS8700_AXY_MASK : fxos8700.h
- FXOS8700_AXZ_MASK : fxos8700.h
- FXOS8700_BAFRO_MASK : fxos8700.h
- FXOS8700_BAFRO_SHIFT : fxos8700.h
- FXOS8700_BKFR_MASK : fxos8700.h
- FXOS8700_BKFR_SHIFT : fxos8700.h
- FXOS8700_CMP_X_LSB : fxos8700.h
- FXOS8700_CMP_X_MSB : fxos8700.h
- FXOS8700_CMP_Y_LSB : fxos8700.h
- FXOS8700_CMP_Y_MSB : fxos8700.h
- FXOS8700_CMP_Z_LSB : fxos8700.h
- FXOS8700_CMP_Z_MSB : fxos8700.h
- fxos8700_ConfigTable_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_CTRL_REG1 : fxos8700.h
- FXOS8700_CTRL_REG2 : fxos8700.h
- FXOS8700_CTRL_REG3 : fxos8700.h
- FXOS8700_CTRL_REG4 : fxos8700.h
- FXOS8700_CTRL_REG5 : fxos8700.h
- FXOS8700_DBCNTM_MASK : fxos8700.h
- FXOS8700_DBCNTM_SHIFT : fxos8700.h
- FXOS8700_DPA_MASK : fxos8700.h
- FXOS8700_DPA_SHIFT : fxos8700.h
- FXOS8700_DPE_MASK : fxos8700.h
- FXOS8700_DR_MASK : fxos8700.h
- FXOS8700_DR_SHIFT : fxos8700.h
- FXOS8700_DR_STATUS : fxos8700.h
- FXOS8700_EA_MASK : fxos8700.h
- FXOS8700_ELE_MASK : fxos8700.h
- FXOS8700_ELE_SHIFT : fxos8700.h
- FXOS8700_ERROR_BURSTWRITE : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_ERROR_CONFIG : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_ERROR_SETPOWER : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Error_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_ERROR_WAITFORACTIVE : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_ERROR_WHOAMI : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_F_READ_MASK : fxos8700.h
- FXOS8700_F_READ_SHIFT : fxos8700.h
- FXOS8700_F_SETUP : fxos8700.h
- FXOS8700_F_STATUS : fxos8700.h
- FXOS8700_FF_MT_CFG : fxos8700.h
- FXOS8700_FF_MT_COUNT : fxos8700.h
- FXOS8700_FF_MT_SRC : fxos8700.h
- FXOS8700_FF_MT_THS : fxos8700.h
- FXOS8700_FIFO_GATE_MASK : fxos8700.h
- FXOS8700_FIFO_GATE_SHIFT : fxos8700.h
- FXOS8700_FS_MASK : fxos8700.h
- FXOS8700_FS_SHIFT : fxos8700.h
- FXOS8700_GET_FIELD : fxos8700.h
- FXOS8700_HP_FILTER_CUTOFF : fxos8700.h
- FXOS8700_HPF_BYP_MASK : fxos8700.h
- FXOS8700_HPF_BYP_SHIFT : fxos8700.h
- FXOS8700_HPF_OUT_MASK : fxos8700.h
- FXOS8700_HPF_OUT_SHIFT : fxos8700.h
- FXOS8700_HYS_MASK : fxos8700.h
- FXOS8700_HYS_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_ASLP_MASK : fxos8700.h
- FXOS8700_INT_CFG_ASLP_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_DRDY_MASK : fxos8700.h
- FXOS8700_INT_CFG_DRDY_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_FF_MT_MASK : fxos8700.h
- FXOS8700_INT_CFG_FF_MT_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_FIFO_MASK : fxos8700.h
- FXOS8700_INT_CFG_FIFO_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_LNDPRT_MASK : fxos8700.h
- FXOS8700_INT_CFG_LNDPRT_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_PULSE_MASK : fxos8700.h
- FXOS8700_INT_CFG_PULSE_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_TRANS_MASK : fxos8700.h
- FXOS8700_INT_CFG_TRANS_SHIFT : fxos8700.h
- FXOS8700_INT_CFG_VECM_MASK : fxos8700.h
- FXOS8700_INT_CFG_VECM_SHIFT : fxos8700.h
- FXOS8700_INT_EN_ASLP_MASK : fxos8700.h
- FXOS8700_INT_EN_ASLP_SHIFT : fxos8700.h
- FXOS8700_INT_EN_DRDY_MASK : fxos8700.h
- FXOS8700_INT_EN_DRDY_SHIFT : fxos8700.h
- FXOS8700_INT_EN_FF_MT_MASK : fxos8700.h
- FXOS8700_INT_EN_FF_MT_SHIFT : fxos8700.h
- FXOS8700_INT_EN_FIFO_MASK : fxos8700.h
- FXOS8700_INT_EN_FIFO_SHIFT : fxos8700.h
- FXOS8700_INT_EN_LNDPRT_MASK : fxos8700.h
- FXOS8700_INT_EN_LNDPRT_SHIFT : fxos8700.h
- FXOS8700_INT_EN_PULSE_MASK : fxos8700.h
- FXOS8700_INT_EN_PULSE_SHIFT : fxos8700.h
- FXOS8700_INT_EN_TRANS_MASK : fxos8700.h
- FXOS8700_INT_EN_TRANS_SHIFT : fxos8700.h
- FXOS8700_INT_SOURCE : fxos8700.h
- fxos8700_InternalState_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_InternalState_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_IPOL_MASK : fxos8700.h
- FXOS8700_IPOL_SHIFT : fxos8700.h
- FXOS8700_LAPO_MASK : fxos8700.h
- FXOS8700_LAPO_SHIFT : fxos8700.h
- FXOS8700_LNOISE_MASK : fxos8700.h
- FXOS8700_LNOISE_SHIFT : fxos8700.h
- FXOS8700_LO_MASK : fxos8700.h
- FXOS8700_LO_SHIFT : fxos8700.h
- FXOS8700_M_ACAL_MASK : fxos8700.h
- FXOS8700_M_ACAL_SHIFT : fxos8700.h
- FXOS8700_M_ASLP_OS_MASK : fxos8700.h
- FXOS8700_M_ASLP_OS_SHIFT : fxos8700.h
- FXOS8700_M_AUTOINC_MASK : fxos8700.h
- FXOS8700_M_AUTOINC_SHIFT : fxos8700.h
- FXOS8700_M_CTRL_REG1 : fxos8700.h
- FXOS8700_M_CTRL_REG2 : fxos8700.h
- FXOS8700_M_CTRL_REG3 : fxos8700.h
- FXOS8700_M_DR_STATUS : fxos8700.h
- FXOS8700_M_HMS_MASK : fxos8700.h
- FXOS8700_M_HMS_SHIFT : fxos8700.h
- FXOS8700_M_INT_SRC : fxos8700.h
- FXOS8700_M_MAXMIN_DIS_MASK : fxos8700.h
- FXOS8700_M_MAXMIN_DIS_SHIFT : fxos8700.h
- FXOS8700_M_MAXMIN_DIS_THS_MASK : fxos8700.h
- FXOS8700_M_MAXMIN_DIS_THS_SHIFT : fxos8700.h
- FXOS8700_M_MAXMIN_RST_MASK : fxos8700.h
- FXOS8700_M_MAXMIN_RST_SHIFT : fxos8700.h
- FXOS8700_M_OFF_X_LSB : fxos8700.h
- FXOS8700_M_OFF_X_MSB : fxos8700.h
- FXOS8700_M_OFF_Y_LSB : fxos8700.h
- FXOS8700_M_OFF_Y_MSB : fxos8700.h
- FXOS8700_M_OFF_Z_LSB : fxos8700.h
- FXOS8700_M_OFF_Z_MSB : fxos8700.h
- FXOS8700_M_OS_MASK : fxos8700.h
- FXOS8700_M_OS_SHIFT : fxos8700.h
- FXOS8700_M_OST_MASK : fxos8700.h
- FXOS8700_M_OST_SHIFT : fxos8700.h
- FXOS8700_M_OUT_X_LSB : fxos8700.h
- FXOS8700_M_OUT_X_MSB : fxos8700.h
- FXOS8700_M_OUT_Y_LSB : fxos8700.h
- FXOS8700_M_OUT_Y_MSB : fxos8700.h
- FXOS8700_M_OUT_Z_LSB : fxos8700.h
- FXOS8700_M_OUT_Z_MSB : fxos8700.h
- FXOS8700_M_RAW_MASK : fxos8700.h
- FXOS8700_M_RAW_SHIFT : fxos8700.h
- FXOS8700_M_RST_CNT_MASK : fxos8700.h
- FXOS8700_M_RST_CNT_SHIFT : fxos8700.h
- FXOS8700_M_RST_MASK : fxos8700.h
- FXOS8700_M_RST_SHIFT : fxos8700.h
- FXOS8700_M_ST_XY_MASK : fxos8700.h
- FXOS8700_M_ST_XY_SHIFT : fxos8700.h
- FXOS8700_M_ST_Z_MASK : fxos8700.h
- FXOS8700_M_ST_Z_SHIFT : fxos8700.h
- FXOS8700_M_THS_CFG : fxos8700.h
- FXOS8700_M_THS_COUNT : fxos8700.h
- FXOS8700_M_THS_EA_MASK : fxos8700.h
- FXOS8700_M_THS_EA_SHIFT : fxos8700.h
- FXOS8700_M_THS_ELE_MASK : fxos8700.h
- FXOS8700_M_THS_ELE_SHIFT : fxos8700.h
- FXOS8700_M_THS_INT_CFG_MASK : fxos8700.h
- FXOS8700_M_THS_INT_CFG_SHIFT : fxos8700.h
- FXOS8700_M_THS_INT_EN_MASK : fxos8700.h
- FXOS8700_M_THS_INT_EN_SHIFT : fxos8700.h
- FXOS8700_M_THS_OAE_MASK : fxos8700.h
- FXOS8700_M_THS_OAE_SHIFT : fxos8700.h
- FXOS8700_M_THS_SRC : fxos8700.h
- FXOS8700_M_THS_WAKE_EN_MASK : fxos8700.h
- FXOS8700_M_THS_WAKE_EN_SHIFT : fxos8700.h
- FXOS8700_M_THS_X_LSB : fxos8700.h
- FXOS8700_M_THS_X_MSB : fxos8700.h
- FXOS8700_M_THS_XEFE_MASK : fxos8700.h
- FXOS8700_M_THS_XEFE_SHIFT : fxos8700.h
- FXOS8700_M_THS_XHE_MASK : fxos8700.h
- FXOS8700_M_THS_XHE_SHIFT : fxos8700.h
- FXOS8700_M_THS_XHP_MASK : fxos8700.h
- FXOS8700_M_THS_XHP_SHIFT : fxos8700.h
- FXOS8700_M_THS_XYZ_UPDATE_MASK : fxos8700.h
- FXOS8700_M_THS_XYZ_UPDATE_SHIFT : fxos8700.h
- FXOS8700_M_THS_Y_LSB : fxos8700.h
- FXOS8700_M_THS_Y_MSB : fxos8700.h
- FXOS8700_M_THS_YEFE_MASK : fxos8700.h
- FXOS8700_M_THS_YEFE_SHIFT : fxos8700.h
- FXOS8700_M_THS_YHE_MASK : fxos8700.h
- FXOS8700_M_THS_YHE_SHIFT : fxos8700.h
- FXOS8700_M_THS_YHP_MASK : fxos8700.h
- FXOS8700_M_THS_YHP_SHIFT : fxos8700.h
- FXOS8700_M_THS_Z_LSB : fxos8700.h
- FXOS8700_M_THS_Z_MSB : fxos8700.h
- FXOS8700_M_THS_ZEFE_MASK : fxos8700.h
- FXOS8700_M_THS_ZEFE_SHIFT : fxos8700.h
- FXOS8700_M_THS_ZHE_MASK : fxos8700.h
- FXOS8700_M_THS_ZHE_SHIFT : fxos8700.h
- FXOS8700_M_THS_ZHP_MASK : fxos8700.h
- FXOS8700_M_THS_ZHP_SHIFT : fxos8700.h
- FXOS8700_M_VECM_CFG : fxos8700.h
- FXOS8700_M_VECM_CNT : fxos8700.h
- FXOS8700_M_VECM_INITX_LSB : fxos8700.h
- FXOS8700_M_VECM_INITX_MSB : fxos8700.h
- FXOS8700_M_VECM_INITY_LSB : fxos8700.h
- FXOS8700_M_VECM_INITY_MSB : fxos8700.h
- FXOS8700_M_VECM_INITZ_LSB : fxos8700.h
- FXOS8700_M_VECM_INITZ_MSB : fxos8700.h
- FXOS8700_M_VECM_THS_LSB : fxos8700.h
- FXOS8700_M_VECM_THS_MSB : fxos8700.h
- FXOS8700_MAG_FIXED_CONVERSION_FACTOR : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_MAG_FIXED_CONVERSION_OFFSET : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_MAG_FLOAT_CONVERSION_FACTOR : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_MAG_FLOAT_CONVERSION_OFFSET : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_MAX_X_LSB : fxos8700.h
- FXOS8700_MAX_X_MSB : fxos8700.h
- FXOS8700_MAX_Y_LSB : fxos8700.h
- FXOS8700_MAX_Y_MSB : fxos8700.h
- FXOS8700_MAX_Z_LSB : fxos8700.h
- FXOS8700_MAX_Z_MSB : fxos8700.h
- FXOS8700_MIN_X_LSB : fxos8700.h
- FXOS8700_MIN_X_MSB : fxos8700.h
- FXOS8700_MIN_Y_LSB : fxos8700.h
- FXOS8700_MIN_Y_MSB : fxos8700.h
- FXOS8700_MIN_Z_LSB : fxos8700.h
- FXOS8700_MIN_Z_MSB : fxos8700.h
- FXOS8700_MODE_ACCELEROMETER : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_MODE_EXTEND : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_MODE_HYBRID : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_MODE_MAGNETOMETER : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Mode_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Mode_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_MODS_MASK : fxos8700.h
- FXOS8700_MODS_SHIFT : fxos8700.h
- FXOS8700_NEWLP_MASK : fxos8700.h
- FXOS8700_NEWLP_SHIFT : fxos8700.h
- FXOS8700_OAE_MASK : fxos8700.h
- FXOS8700_OAE_SHIFT : fxos8700.h
- FXOS8700_OFF_X : fxos8700.h
- FXOS8700_OFF_Y : fxos8700.h
- FXOS8700_OFF_Z : fxos8700.h
- FXOS8700_OUT_X_LSB : fxos8700.h
- FXOS8700_OUT_X_MSB : fxos8700.h
- FXOS8700_OUT_Y_LSB : fxos8700.h
- FXOS8700_OUT_Y_MSB : fxos8700.h
- FXOS8700_OUT_Z_LSB : fxos8700.h
- FXOS8700_OUT_Z_MSB : fxos8700.h
- FXOS8700_PEA_MASK : fxos8700.h
- FXOS8700_PELE_MASK : fxos8700.h
- FXOS8700_PELE_SHIFT : fxos8700.h
- FXOS8700_PL_BF_ZCOMP : fxos8700.h
- FXOS8700_PL_CFG : fxos8700.h
- FXOS8700_PL_COUNT : fxos8700.h
- FXOS8700_PL_EN_MASK : fxos8700.h
- FXOS8700_PL_EN_SHIFT : fxos8700.h
- FXOS8700_PL_STATUS : fxos8700.h
- FXOS8700_PL_THS_MASK : fxos8700.h
- FXOS8700_PL_THS_REG : fxos8700.h
- FXOS8700_PL_THS_SHIFT : fxos8700.h
- FXOS8700_POLX_MASK : fxos8700.h
- FXOS8700_POLY_MASK : fxos8700.h
- FXOS8700_POLZ_MASK : fxos8700.h
- FXOS8700_POWER_ACTIVE : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_POWER_STANDBY : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Power_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Power_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_PP_OD_MASK : fxos8700.h
- FXOS8700_PP_OD_SHIFT : fxos8700.h
- FXOS8700_PULSE_CFG : fxos8700.h
- FXOS8700_PULSE_HPF_BYP_MASK : fxos8700.h
- FXOS8700_PULSE_HPF_BYP_SHIFT : fxos8700.h
- FXOS8700_PULSE_LPF_EN_MASK : fxos8700.h
- FXOS8700_PULSE_LPF_EN_SHIFT : fxos8700.h
- FXOS8700_PULSE_LTCY : fxos8700.h
- FXOS8700_PULSE_SRC : fxos8700.h
- FXOS8700_PULSE_THSX : fxos8700.h
- FXOS8700_PULSE_THSY : fxos8700.h
- FXOS8700_PULSE_THSZ : fxos8700.h
- FXOS8700_PULSE_WIND : fxos8700.h
- FXOS8700_RANGE_2G : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_RANGE_4G : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_RANGE_8G : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_RANGE_MAX : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Range_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Range_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_regmap_tag : fxos8700.h
- FXOS8700_RESOLUTION_8_BIT : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_RESOLUTION_NORMAL : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Resolution_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_Resolution_tag : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_RST_MASK : fxos8700.h
- FXOS8700_RST_SHIFT : fxos8700.h
- FXOS8700_SAMPLE_PERIOD_MAX : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_SAMPLE_PERIOD_MIN : fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_SEL_MASK : fxos8700.h
- FXOS8700_SEL_SHIFT : fxos8700.h
- FXOS8700_SET_FIELD : fxos8700.h
- FXOS8700_SLPE_MASK : fxos8700.h
- FXOS8700_SLPE_SHIFT : fxos8700.h
- FXOS8700_SMODS_MASK : fxos8700.h
- FXOS8700_SMODS_SHIFT : fxos8700.h
- FXOS8700_SRC_M_DRDY_MASK : fxos8700.h
- FXOS8700_SRC_M_DRDY_SHIFT : fxos8700.h
- FXOS8700_SRC_M_THS_MASK : fxos8700.h
- FXOS8700_SRC_M_THS_SHIFT : fxos8700.h
- FXOS8700_SRC_M_VECM_MASK : fxos8700.h
- FXOS8700_SRC_M_VECM_SHIFT : fxos8700.h
- FXOS8700_STATE_CONFIGURED : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_STATE_INITIALIZED : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_STATE_STARTED : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_STATE_UNINTIALIZED : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_STATUS : fxos8700.h
- fxos8700_Status_t : fsl_fxos8700_i2cspi_6D_AccMag.h
- fxos8700_SupportedDataTypes : fsl_fxos8700_i2cspi_6D_AccMag.h , fsl_fxos8700_i2cspi_6D_AccMag.c
- fxos8700_SupportedSensorTypes : fsl_fxos8700_i2cspi_6D_AccMag.h , fsl_fxos8700_i2cspi_6D_AccMag.c
- FXOS8700_SYSMOD : fxos8700.h
- FXOS8700_TEA_MASK : fxos8700.h
- FXOS8700_TELE_MASK : fxos8700.h
- FXOS8700_TELE_SHIFT : fxos8700.h
- FXOS8700_TEMP : fxos8700.h
- FXOS8700_THS_MASK : fxos8700.h
- FXOS8700_THS_SHIFT : fxos8700.h
- FXOS8700_TMLT : fxos8700.h
- FXOS8700_TRANSIENT_CFG : fxos8700.h
- FXOS8700_TRANSIENT_COUNT : fxos8700.h
- FXOS8700_TRANSIENT_SRC : fxos8700.h
- FXOS8700_TRANSIENT_THS : fxos8700.h
- FXOS8700_TRIG_CFG : fxos8700.h
- FXOS8700_WAKE_FF_MT_MASK : fxos8700.h
- FXOS8700_WAKE_FF_MT_SHIFT : fxos8700.h
- FXOS8700_WAKE_LNDPRT_MASK : fxos8700.h
- FXOS8700_WAKE_LNDPRT_SHIFT : fxos8700.h
- FXOS8700_WAKE_PULSE_MASK : fxos8700.h
- FXOS8700_WAKE_PULSE_SHIFT : fxos8700.h
- FXOS8700_WAKE_TRANS_MASK : fxos8700.h
- FXOS8700_WAKE_TRANS_SHIFT : fxos8700.h
- FXOS8700_WHO_AM_I : fxos8700.h
- FXOS8700_WHO_AM_I_VALUE1 : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_WHO_AM_I_VALUE2 : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_WHO_AM_I_VALUE3 : fsl_fxos8700_i2cspi_6D_AccMag.h
- FXOS8700_X_TRANS_POL_MASK : fxos8700.h
- FXOS8700_XDPEFE_MASK : fxos8700.h
- FXOS8700_XDPEFE_SHIFT : fxos8700.h
- FXOS8700_XDR_MASK : fxos8700.h
- FXOS8700_XEFE_MASK : fxos8700.h
- FXOS8700_XEFE_SHIFT : fxos8700.h
- FXOS8700_XHE_MASK : fxos8700.h
- FXOS8700_XHP_MASK : fxos8700.h
- FXOS8700_XOW_MASK : fxos8700.h
- FXOS8700_XSPEFE_MASK : fxos8700.h
- FXOS8700_XSPEFE_SHIFT : fxos8700.h
- FXOS8700_XTEFE_MASK : fxos8700.h
- FXOS8700_XTEFE_SHIFT : fxos8700.h
- FXOS8700_XTRANSE_MASK : fxos8700.h
- FXOS8700_XYZ_DATA_CFG : fxos8700.h
- FXOS8700_Y_TRANS_POL_MASK : fxos8700.h
- FXOS8700_YDPEFE_MASK : fxos8700.h
- FXOS8700_YDPEFE_SHIFT : fxos8700.h
- FXOS8700_YDR_MASK : fxos8700.h
- FXOS8700_YEFE_MASK : fxos8700.h
- FXOS8700_YEFE_SHIFT : fxos8700.h
- FXOS8700_YHE_MASK : fxos8700.h
- FXOS8700_YHP_MASK : fxos8700.h
- FXOS8700_YOW_MASK : fxos8700.h
- FXOS8700_YSPEFE_MASK : fxos8700.h
- FXOS8700_YSPEFE_SHIFT : fxos8700.h
- FXOS8700_YTEFE_MASK : fxos8700.h
- FXOS8700_YTEFE_SHIFT : fxos8700.h
- FXOS8700_YTRANSE_MASK : fxos8700.h
- FXOS8700_Z_TRANS_POL_MASK : fxos8700.h
- FXOS8700_ZDPEFE_MASK : fxos8700.h
- FXOS8700_ZDPEFE_SHIFT : fxos8700.h
- FXOS8700_ZDR_MASK : fxos8700.h
- FXOS8700_ZEFE_MASK : fxos8700.h
- FXOS8700_ZEFE_SHIFT : fxos8700.h
- FXOS8700_ZHE_MASK : fxos8700.h
- FXOS8700_ZHP_MASK : fxos8700.h
- FXOS8700_ZLOCK_MASK : fxos8700.h
- FXOS8700_ZLOCK_SHIFT : fxos8700.h
- FXOS8700_ZOW_MASK : fxos8700.h
- FXOS8700_ZSPEFE_MASK : fxos8700.h
- FXOS8700_ZSPEFE_SHIFT : fxos8700.h
- FXOS8700_ZTEFE_MASK : fxos8700.h
- FXOS8700_ZTEFE_SHIFT : fxos8700.h
- FXOS8700_ZTRANSE_MASK : fxos8700.h
- FXOS8700_ZYXDR_MASK : fxos8700.h
- FXOS8700_ZYXDR_SHIFT : fxos8700.h
- FXOS8700_ZYXOW_MASK : fxos8700.h
- fxos8700AccelConvTable : fsl_fxos8700_i2cspi_6D_AccMag.c
- isf_fieldStrength_uT_float_t : isf_magnetometer_types.h
- isf_fifo_alloc() : isf_fifo.h , isf_fifo.c
- isf_fifo_data_copy() : isf_fifo.c , isf_fifo.h
- isf_fifo_el_clear() : isf_fifo.h , isf_fifo.c
- isf_fifo_el_get_insert_pointer() : isf_fifo.c , isf_fifo.h
- isf_fifo_el_increment() : isf_fifo.c , isf_fifo.h
- isf_fifo_el_traverse() : isf_fifo.h , isf_fifo.c
- isf_fifo_free() : isf_fifo.c , isf_fifo.h
- isf_fifo_get_buffer_size() : isf_fifo.c , isf_fifo.h
- isf_fifo_init() : isf_fifo.h , isf_fifo.c
- isf_fifo_lock() : isf_fifo.c , isf_fifo.h
- isf_fifo_resize() : isf_fifo.h , isf_fifo.c
- isf_fifo_status_t : isf_fifo.h
- isf_fifo_try_lock() : isf_fifo.h , isf_fifo.c
- isf_fifo_unlock() : isf_fifo.c , isf_fifo.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.